<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="17.78" y1="29.21" x2="73.584" y2="29.21" width="0" layer="20"/>
<wire x1="73.584" y1="29.21" x2="73.584" y2="75.2248" width="0" layer="20"/>
<wire x1="73.584" y1="75.2248" x2="17.78" y2="75.2248" width="0" layer="20"/>
<wire x1="17.78" y1="75.2248" x2="17.78" y2="29.21" width="0" layer="20"/>
<text>1</text>
<hole x="71.3232" y="72.8472" drill="3"/>
<hole x="20.4216" y="31.6992" drill="3"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
</packages>
</library>
<library name="Seeed-OPL-Resistor">
<packages>
<package name="R0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-1101NE">
<description>SparkFun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1_BASIC">
</package>
</packages>
</library>
<library name="roblib">
<packages>
<package name="TINYCON">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P1600X1600X120-64N">
</package>
</packages>
</library>
<library name="Seeed-OPL-crystal-osctllator">
<packages>
<package name="X4-SMD-3.2X2.5X0.7MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="IOS1" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IOS2" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IOS3" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IOS4" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IOS5" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IOS6" library="pinhead" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="MATRIX_CONNECTOR" library="pinhead" package="2X08" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="Seeed-OPL-Resistor" package="R0603" value="330R">
<attribute name="MPN" value="RC0603FR-07330RL"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="SWITCH-MOMENTARY-2SMD-1101NE">
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_BASIC" value="TEENSY_3.1_BASIC"/>
<element name="U$2" library="roblib" package="TINYCON" value="TINYCON"/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P1600X1600X120-64N" value="ATMEGA128A-AU">
<attribute name="PACKAGE" value="TQFP-64"/>
<attribute name="OC_FARNELL" value="1773397"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_NEWARK" value="51R8675"/>
<attribute name="MPN" value="ATMEGA128A-AU"/>
</element>
<element name="X1" library="Seeed-OPL-crystal-osctllator" package="X4-SMD-3.2X2.5X0.7MM" value=""/>
</elements>
<signals>
<signal name="VBAT">
<contactref element="U$1" pad="VBAT"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="3-GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="GND@1"/>
<contactref element="U$2" pad="GND"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="53"/>
<contactref element="U1" pad="22"/>
<contactref element="RESET" pad="1"/>
<contactref element="MATRIX_CONNECTOR" pad="4"/>
<contactref element="MATRIX_CONNECTOR" pad="8"/>
<contactref element="MATRIX_CONNECTOR" pad="16"/>
<contactref element="U$1" pad="AGND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
</signal>
<signal name="3V3">
<contactref element="LED1" pad="1-VDD"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="U$2" pad="3V3@1"/>
<contactref element="U$2" pad="3V3"/>
<contactref element="U1" pad="62"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="52"/>
<contactref element="U1" pad="21"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="U$1" pad="3.3V1"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="SCK"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="13"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="12"/>
</signal>
<signal name="XTAL1">
<contactref element="C5" pad="1"/>
<contactref element="X1" pad="4"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="XTAL2">
<contactref element="C6" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="RGB_LED">
<contactref element="U1" pad="4"/>
<contactref element="LED1" pad="4-DIN"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="R4" pad="2"/>
<contactref element="RESET" pad="2"/>
<contactref element="U$2" pad="RST"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="5"/>
<contactref element="IOS1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="6"/>
<contactref element="IOS1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="7"/>
<contactref element="IOS1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="8"/>
<contactref element="IOS1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="9"/>
<contactref element="IOS1" pad="5"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="14"/>
<contactref element="IOS1" pad="6"/>
</signal>
<signal name="D13">
<contactref element="U1" pad="15"/>
<contactref element="IOS1" pad="7"/>
</signal>
<signal name="D14">
<contactref element="U1" pad="16"/>
<contactref element="IOS1" pad="8"/>
</signal>
<signal name="SS">
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="25"/>
<contactref element="IOS2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="26"/>
<contactref element="IOS2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="27"/>
<contactref element="IOS2" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="28"/>
<contactref element="IOS2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="29"/>
<contactref element="IOS2" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="30"/>
<contactref element="IOS2" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="31"/>
<contactref element="IOS2" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="32"/>
<contactref element="IOS2" pad="8"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="33"/>
<contactref element="IOS3" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="34"/>
<contactref element="IOS3" pad="2"/>
</signal>
<signal name="D28">
<contactref element="U1" pad="35"/>
<contactref element="IOS3" pad="3"/>
</signal>
<signal name="D29">
<contactref element="U1" pad="36"/>
<contactref element="IOS3" pad="4"/>
</signal>
<signal name="D30">
<contactref element="U1" pad="37"/>
<contactref element="IOS3" pad="5"/>
</signal>
<signal name="D31">
<contactref element="U1" pad="38"/>
<contactref element="IOS3" pad="6"/>
</signal>
<signal name="D32">
<contactref element="U1" pad="39"/>
<contactref element="IOS3" pad="7"/>
</signal>
<signal name="D33">
<contactref element="U1" pad="40"/>
<contactref element="IOS3" pad="8"/>
</signal>
<signal name="D34">
<contactref element="U1" pad="41"/>
<contactref element="IOS4" pad="1"/>
</signal>
<signal name="D35">
<contactref element="U1" pad="42"/>
<contactref element="IOS4" pad="2"/>
</signal>
<signal name="D36">
<contactref element="U1" pad="43"/>
<contactref element="IOS4" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="44"/>
<contactref element="IOS4" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="IOS4" pad="6"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="45"/>
<contactref element="IOS4" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="IOS4" pad="7"/>
<contactref element="U1" pad="47"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="48"/>
<contactref element="IOS4" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="61"/>
<contactref element="IOS5" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="60"/>
<contactref element="IOS5" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U1" pad="59"/>
<contactref element="IOS5" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="U1" pad="58"/>
<contactref element="IOS5" pad="4"/>
</signal>
<signal name="N$29">
<contactref element="U1" pad="57"/>
<contactref element="IOS5" pad="5"/>
</signal>
<signal name="N$30">
<contactref element="U1" pad="56"/>
<contactref element="IOS5" pad="6"/>
</signal>
<signal name="N$31">
<contactref element="U1" pad="55"/>
<contactref element="IOS5" pad="7"/>
</signal>
<signal name="N$32">
<contactref element="U1" pad="54"/>
<contactref element="IOS5" pad="8"/>
</signal>
<signal name="R1">
<contactref element="U$1" pad="2"/>
<contactref element="MATRIX_CONNECTOR" pad="1"/>
</signal>
<signal name="LATCH">
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="8"/>
<contactref element="MATRIX_CONNECTOR" pad="14"/>
</signal>
<signal name="OE">
<contactref element="U$1" pad="4"/>
<contactref element="MATRIX_CONNECTOR" pad="15"/>
</signal>
<signal name="G1">
<contactref element="U$1" pad="5"/>
<contactref element="MATRIX_CONNECTOR" pad="2"/>
</signal>
<signal name="B1">
<contactref element="U$1" pad="6"/>
<contactref element="MATRIX_CONNECTOR" pad="3"/>
</signal>
<signal name="G2">
<contactref element="U$1" pad="7"/>
<contactref element="MATRIX_CONNECTOR" pad="6"/>
</signal>
<signal name="ADX0">
<contactref element="U$1" pad="9"/>
<contactref element="MATRIX_CONNECTOR" pad="9"/>
</signal>
<signal name="ADX1">
<contactref element="U$1" pad="10"/>
<contactref element="MATRIX_CONNECTOR" pad="10"/>
</signal>
<signal name="ADX2">
<contactref element="U$1" pad="22/A8"/>
<contactref element="MATRIX_CONNECTOR" pad="11"/>
</signal>
<signal name="ADX3">
<contactref element="U$1" pad="23/A9"/>
<contactref element="MATRIX_CONNECTOR" pad="12"/>
</signal>
<signal name="R2">
<contactref element="U$1" pad="21/A7"/>
<contactref element="MATRIX_CONNECTOR" pad="5"/>
</signal>
<signal name="B2">
<contactref element="U$1" pad="20/A6"/>
<contactref element="MATRIX_CONNECTOR" pad="7"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="14/A0"/>
<contactref element="MATRIX_CONNECTOR" pad="13"/>
</signal>
<signal name="ATMEGA_RX">
<contactref element="U1" pad="2"/>
<contactref element="U$2" pad="RX"/>
<contactref element="U$2" pad="MOSI"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="ATMEGA_TX">
<contactref element="U1" pad="3"/>
<contactref element="U$2" pad="TX"/>
<contactref element="U$2" pad="MISO"/>
<contactref element="U$1" pad="0"/>
</signal>
<signal name="N$2">
<contactref element="IOS6" pad="1"/>
<contactref element="U$1" pad="15/A1"/>
</signal>
<signal name="N$3">
<contactref element="IOS6" pad="2"/>
<contactref element="U$1" pad="16/A2"/>
</signal>
<signal name="N$21">
<contactref element="IOS6" pad="3"/>
<contactref element="U$1" pad="17/A3"/>
</signal>
<signal name="N$33">
<contactref element="IOS6" pad="4"/>
<contactref element="U$1" pad="18/A4"/>
</signal>
<signal name="N$34">
<contactref element="IOS6" pad="5"/>
<contactref element="U$1" pad="19/A5"/>
</signal>
<signal name="DAC">
<contactref element="U$1" pad="A14"/>
<contactref element="IOS6" pad="8"/>
</signal>
<signal name="TEENSY_D11">
<contactref element="U$1" pad="11"/>
<contactref element="IOS6" pad="6"/>
</signal>
<signal name="TEENSY_D12">
<contactref element="U$1" pad="12"/>
<contactref element="IOS6" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
