<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="112" y2="0" width="0" layer="20"/>
<wire x1="112" y1="0" x2="112" y2="32" width="0" layer="20"/>
<wire x1="110" y1="34" x2="2" y2="34" width="0" layer="20"/>
<wire x1="0" y1="32" x2="0" y2="0" width="0" layer="20"/>
<wire x1="112" y1="32" x2="110" y2="34" width="0" layer="20" curve="90"/>
<wire x1="0" y1="32" x2="2" y2="34" width="0" layer="20" curve="-90"/>
<text>v1.2
2/25/2017</text>
<text>14</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>2</text>
<text>2</text>
</plain>
<libraries>
<library name="#mine">
<packages>
<package name="JST_XH_2">
<description>A package for a 2 pin JST XH connector.</description>
</package>
<package name="JST_XH_14">
<description>A package for a JST XH 14 pin connector.</description>
</package>
<package name="SWITCH_4">
<description>Footprint for a 4 leg tactile switch, specifically the 1825910-6 from TE Connectivity.</description>
</package>
<package name="DB_15_PLUG">
<description>Footprint for a Amphenol Commercial Products's L717SDA15PA4CH4F a through hole mount DB 15 connector.</description>
</package>
</packages>
</library>
<library name="JAMMA">
<packages>
<package name="JAMMA_TOP_COMPACT_PLUG">
<description>&lt;b&gt;JAMMA Connector Top&lt;/b&gt;&lt;br&gt;
Parts side&lt;br&gt;
&lt;br&gt;
for these card-edge connenctors&lt;br&gt;
HIROSE CR7E-56DA-3.96E&lt;br&gt;
HIROSE CR7E-56DB-3.96E&lt;br&gt;
KEL 1168-056-009&lt;br&gt;</description>
</package>
<package name="JAMMA_BOTTOM_COMPACT_PLUG">
<description>&lt;b&gt;JAMMA Connector Bottom&lt;/b&gt;&lt;br&gt;
Solder side&lt;br&gt;
&lt;br&gt;
for these card-edge connenctors&lt;br&gt;
HIROSE CR7E-56DA-3.96E&lt;br&gt;
HIROSE CR7E-56DB-3.96E&lt;br&gt;
KEL 1168-056-009&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12V_MONITOR" library="#mine" package="JST_XH_2" value="JST_XH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V_MONITOR" library="#mine" package="JST_XH_2" value="JST_XH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V_OUT" library="#mine" package="JST_XH_2" value="JST_XH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN3_IN" library="#mine" package="JST_XH_14" value="JST_XH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="COIN1" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="COIN2" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JAMMA1" library="JAMMA" package="JAMMA_TOP_COMPACT_PLUG" value="JAMMA_TOPPLUG"/>
<element name="JAMMA2" library="JAMMA" package="JAMMA_BOTTOM_COMPACT_PLUG" value="JAMMA_BOTTOMPLUG"/>
<element name="P1" library="#mine" package="DB_15_PLUG" value="L717SDA15PA4CH4F">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="P2" library="#mine" package="DB_15_PLUG" value="L717SDA15PA4CH4F">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERVICE" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEST" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JAMMA2" pad="J"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="JAMMA1" pad="8"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="GND_NET">
<contactref element="JAMMA1" pad="1"/>
<contactref element="TEST" pad="P$3"/>
<contactref element="TEST" pad="P$4"/>
<contactref element="5V_OUT" pad="P$2"/>
<contactref element="5V_MONITOR" pad="P$2"/>
<contactref element="12V_MONITOR" pad="P$2"/>
<contactref element="P1" pad="P$1"/>
<contactref element="P2" pad="P$1"/>
<contactref element="JAMMA2" pad="A"/>
<contactref element="JAMMA1" pad="2"/>
<contactref element="JAMMA2" pad="B"/>
<contactref element="SERVICE" pad="P$4"/>
<contactref element="SERVICE" pad="P$3"/>
</signal>
<signal name="N$6">
<contactref element="JAMMA1" pad="16"/>
<contactref element="COIN1" pad="P$1"/>
<contactref element="COIN1" pad="P$2"/>
<contactref element="P1" pad="P$3"/>
</signal>
<signal name="N$7">
<contactref element="TEST" pad="P$1"/>
<contactref element="TEST" pad="P$2"/>
<contactref element="JAMMA1" pad="15"/>
</signal>
<signal name="N$5">
<contactref element="JAMMA2" pad="R"/>
<contactref element="SERVICE" pad="P$1"/>
<contactref element="SERVICE" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="JAMMA2" pad="T"/>
<contactref element="COIN2" pad="P$1"/>
<contactref element="COIN2" pad="P$2"/>
<contactref element="P2" pad="P$3"/>
</signal>
<signal name="N$11">
<contactref element="JAMMA1" pad="23"/>
<contactref element="P1" pad="P$5"/>
</signal>
<signal name="N$12">
<contactref element="JAMMA2" pad="_A"/>
<contactref element="P2" pad="P$5"/>
</signal>
<signal name="N$16">
<contactref element="JAMMA1" pad="21"/>
<contactref element="P1" pad="P$6"/>
</signal>
<signal name="N$17">
<contactref element="P2" pad="P$6"/>
<contactref element="JAMMA2" pad="Y"/>
</signal>
<signal name="N$18">
<contactref element="P1" pad="P$7"/>
<contactref element="JAMMA1" pad="19"/>
</signal>
<signal name="N$19">
<contactref element="P2" pad="P$7"/>
<contactref element="JAMMA2" pad="W"/>
</signal>
<signal name="5V_NET">
<contactref element="JAMMA2" pad="D"/>
<contactref element="P2" pad="P$8"/>
<contactref element="JAMMA2" pad="C"/>
<contactref element="JAMMA1" pad="4"/>
<contactref element="5V_OUT" pad="P$1"/>
<contactref element="5V_MONITOR" pad="P$1"/>
<contactref element="P1" pad="P$8"/>
<contactref element="JAMMA1" pad="3"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="12V_NET">
<contactref element="JAMMA1" pad="6"/>
<contactref element="12V_MONITOR" pad="P$1"/>
<contactref element="JAMMA2" pad="F"/>
</signal>
<signal name="N$13">
<contactref element="P1" pad="P$11"/>
<contactref element="JAMMA1" pad="17"/>
</signal>
<signal name="N$15">
<contactref element="P2" pad="P$11"/>
<contactref element="JAMMA2" pad="U"/>
</signal>
<signal name="N$21">
<contactref element="P1" pad="P$12"/>
<contactref element="JAMMA1" pad="24"/>
</signal>
<signal name="N$22">
<contactref element="P2" pad="P$12"/>
<contactref element="JAMMA2" pad="_B"/>
</signal>
<signal name="N$23">
<contactref element="P2" pad="P$13"/>
<contactref element="JAMMA2" pad="Z"/>
</signal>
<signal name="N$24">
<contactref element="P1" pad="P$13"/>
<contactref element="JAMMA1" pad="22"/>
</signal>
<signal name="N$25">
<contactref element="JAMMA1" pad="20"/>
<contactref element="P1" pad="P$14"/>
</signal>
<signal name="N$26">
<contactref element="P1" pad="P$15"/>
<contactref element="JAMMA1" pad="18"/>
</signal>
<signal name="N$27">
<contactref element="P2" pad="P$14"/>
<contactref element="JAMMA2" pad="X"/>
</signal>
<signal name="N$28">
<contactref element="JAMMA2" pad="V"/>
<contactref element="P2" pad="P$15"/>
</signal>
<signal name="N$29">
<contactref element="P1" pad="P$4"/>
<contactref element="JAMMA1" pad="25"/>
</signal>
<signal name="N$30">
<contactref element="P2" pad="P$4"/>
<contactref element="JAMMA2" pad="_C"/>
</signal>
<signal name="N$14">
<contactref element="JAMMA1" pad="26"/>
<contactref element="P1" pad="P$10"/>
</signal>
<signal name="N$33">
<contactref element="P2" pad="P$10"/>
<contactref element="JAMMA2" pad="_D"/>
</signal>
<signal name="N$3">
<contactref element="P1" pad="P$2"/>
<contactref element="CN3_IN" pad="P$4"/>
</signal>
<signal name="N$4">
<contactref element="CN3_IN" pad="P$8"/>
<contactref element="P2" pad="P$2"/>
</signal>
<signal name="-5V">
<contactref element="JAMMA1" pad="5"/>
<contactref element="JAMMA2" pad="E"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$20">
</signal>
<signal name="GND_NET2">
<contactref element="JAMMA1" pad="27"/>
<contactref element="JAMMA1" pad="28"/>
<contactref element="JAMMA2" pad="_E"/>
<contactref element="JAMMA2" pad="_F"/>
<contactref element="COIN2" pad="P$4"/>
<contactref element="COIN2" pad="P$3"/>
<contactref element="COIN1" pad="P$3"/>
<contactref element="COIN1" pad="P$4"/>
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
