<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="3.6576" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="3.6576" y2="80" width="0" layer="20"/>
<wire x1="3.6576" y1="80" x2="3.6576" y2="0" width="0" layer="20"/>
<text>311308 Checker</text>
<text>By: Ryan Ledford</text>
<text>Orange</text>
<text>Gray</text>
<text>White</text>
<text>Red</text>
<text>Black</text>
<text>Green</text>
<text>Blue</text>
<text>Black</text>
<text>Red</text>
<hole x="27.2288" y="56.5912" drill="3.81"/>
<hole x="95.7072" y="75.9968" drill="3.81"/>
<hole x="94.8944" y="4.8768" drill="3.81"/>
<hole x="10.2616" y="6.4008" drill="3.81"/>
<hole x="95.4024" y="41.5544" drill="3.81"/>
<hole x="56.9976" y="5.08" drill="1"/>
<hole x="95.9104" y="25.5016" drill="1"/>
<hole x="95.8088" y="53.6448" drill="1"/>
<hole x="68.58" y="74.8792" drill="1"/>
<hole x="48.3616" y="74.3712" drill="1"/>
<hole x="27.94" y="74.8792" drill="1"/>
<hole x="15.748" y="4.3688" drill="1"/>
<hole x="88.2904" y="4.9784" drill="1"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-5MM-3">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -3 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="292133-3">
<packages>
<package name="TE_292133-3">
</package>
</packages>
</library>
<library name="arduino">
<description>&lt;b&gt;Arduino Boards&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;MegaArduino
&lt;li&gt;Arduino Duemilanove (2009)
&lt;/ul&gt;
Based on the following sources:
&lt;br&gt;&lt;br&gt;
Schematic &amp; Reference Design from:
&lt;ul&gt;
&lt;li&gt; http://arduino.cc/en/Main/ArduinoBoardMega
&lt;li&gt;http://arduino.cc/en/Main/ArduinoBoardDuemilanove
&lt;/ul&gt;
Version: 1.0 / 30.08.2009&lt;br&gt;
&lt;author&gt;Created by atami@gmx.net&lt;/author&gt;</description>
<packages>
<package name="MEGA_ARDUINO">
</package>
</packages>
</library>
<library name="5-103669-5">
<packages>
<package name="TE_5-103669-5">
</package>
</packages>
</library>
<library name="0039281083">
<packages>
<package name="CONN_B6B-XH-A_JST">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5566-8">
<description>&lt;b&gt;Mini-Fit Jr.™ Vertical Header, 4.20mm Pitch, Dual Row, 8 Circuits, without Snap-in Plastic Peg PCB Lock, Tin, Natural&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/039281083_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12V_POWER_SUPPLY" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="BLUE_BLACK_RED" library="292133-3" package="TE_292133-3" value="292133-3">
<attribute name="COMMENT" value="292133-3"/>
<attribute name="DESCRIPTION" value=" AMP CT Series; 2mm Pitch 3 Way 1 Row Straight PCB Header; Solder Termination "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="A100945-ND"/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=2185732"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=2185732"/>
<attribute name="MP" value="292133-3"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="BTTN" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2-NS" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="arduino" package="MEGA_ARDUINO" value=""/>
<element name="J4" library="5-103669-5" package="TE_5-103669-5" value="5-103669-5">
<attribute name="CENTERLINE_PITCH" value="2.54 mm[.1 in]"/>
<attribute name="COMMENT" value="5-103669-5"/>
<attribute name="DESCRIPTION" value=" Header; 6; 3 A; 600 V; MTE (IDC); 1; Vertical; 0.100 in.; 5000 Megohms; Brass "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="A35016-ND"/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=481099"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=481099"/>
<attribute name="MP" value="5-103669-5"/>
<attribute name="NUMBER_OF_POSITIONS" value="6"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRODUCT_TYPE" value="Connector"/>
</element>
<element name="J5" library="0039281083" package="CONN_B6B-XH-A_JST" value="B6B-XH-A_(LF)(SN)">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="http://www.jst-mfg.com/product/pdf/eng/eXH.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="B6B-XH-A (LF)(SN)"/>
<attribute name="SOURCELIBRARY" value="JST_2020-07-08"/>
<attribute name="VENDOR" value="JST"/>
</element>
<element name="LED_GND" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-10134"/>
<attribute name="SF_SKU" value="PRT-08433"/>
<attribute name="VALUE"/>
</element>
<element name="LED_HOT" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-10134"/>
<attribute name="SF_SKU" value="PRT-08433"/>
<attribute name="VALUE"/>
</element>
<element name="ORANGE_GRAY_WHITE" library="292133-3" package="TE_292133-3" value="292133-3">
<attribute name="COMMENT" value="292133-3"/>
<attribute name="DESCRIPTION" value=" AMP CT Series; 2mm Pitch 3 Way 1 Row Straight PCB Header; Solder Termination "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="A100945-ND"/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=2185732"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=2185732"/>
<attribute name="MP" value="292133-3"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="RED_BLACK_GREEN" library="292133-3" package="TE_292133-3" value="292133-3">
<attribute name="COMMENT" value="292133-3"/>
<attribute name="DESCRIPTION" value=" AMP CT Series; 2mm Pitch 3 Way 1 Row Straight PCB Header; Solder Termination "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="A100945-ND"/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=2185732"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=2185732"/>
<attribute name="MP" value="292133-3"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="X1" library="con-molex" package="5566-8" value="5566-8">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="45"/>
<contactref element="12V_POWER_SUPPLY" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="81"/>
<contactref element="IC1" pad="82"/>
<contactref element="IC1" pad="5"/>
<contactref element="BTTN" pad="1"/>
<contactref element="LED_GND" pad="1"/>
<contactref element="LED_GND" pad="2"/>
<contactref element="LED_GND" pad="3"/>
</signal>
<signal name="+3V3">
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="8"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="7"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="6"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="10"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="11"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="12"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="13"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="14"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="15"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="16"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="17"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="18"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="19"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="33"/>
<contactref element="ORANGE_GRAY_WHITE" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="34"/>
<contactref element="ORANGE_GRAY_WHITE" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="35"/>
<contactref element="ORANGE_GRAY_WHITE" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="36"/>
<contactref element="RED_BLACK_GREEN" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="37"/>
<contactref element="RED_BLACK_GREEN" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="38"/>
<contactref element="RED_BLACK_GREEN" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="39"/>
<contactref element="BLUE_BLACK_RED" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="40"/>
<contactref element="BLUE_BLACK_RED" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="41"/>
<contactref element="BLUE_BLACK_RED" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="49"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="50"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="51"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="N$26">
<contactref element="IC1" pad="52"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="12V">
<contactref element="12V_POWER_SUPPLY" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$27">
</signal>
<signal name="N$29">
<contactref element="LED_HOT" pad="2"/>
<contactref element="IC1" pad="67"/>
</signal>
<signal name="N$30">
<contactref element="LED_HOT" pad="3"/>
<contactref element="IC1" pad="68"/>
</signal>
<signal name="N$31">
<contactref element="BTTN" pad="2"/>
<contactref element="IC1" pad="70"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="66"/>
<contactref element="LED_HOT" pad="1"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="48"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
