<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="1.27" x2="32.055" y2="1.27" width="0" layer="20"/>
<wire x1="32.055" y1="1.27" x2="32.055" y2="22.85" width="0" layer="20"/>
<wire x1="32.055" y1="22.85" x2="1.27" y2="22.85" width="0" layer="20"/>
<wire x1="1.27" y1="22.85" x2="1.27" y2="1.27" width="0" layer="20"/>
<text>Cryptotronix</text>
<text>pi2CryptoCape</text>
<text>BeagleBone P9</text>
<text>BeagleBone P9</text>
<text>Raspberry Pi</text>
<text>Raspberry Pi</text>
<text>Cryptotronix</text>
<text>P1-01</text>
<text>P1-02</text>
<text>pi2CryptoCape</text>
<text>P9-1/2</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP2" library="SparkFun-Connectors" package="AVR_ICSP" value="M05X2PTH"/>
<element name="JP3" library="SparkFun-Connectors" package="1X12" value="M12PTH"/>
<element name="JP4" library="SparkFun-Connectors" package="1X12" value="M12PTH"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="JP2" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="9"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="JP2" pad="8"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="RXD">
<contactref element="JP2" pad="10"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="GPIO4">
<contactref element="JP2" pad="7"/>
<contactref element="JP4" pad="12"/>
</signal>
<signal name="SCL">
<contactref element="JP2" pad="5"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="SDA">
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
