<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-1.035" y1="-7.135" x2="22.685" y2="-7.135" width="0" layer="20"/>
<wire x1="22.685" y1="-7.135" x2="22.685" y2="11.26" width="0" layer="20"/>
<wire x1="22.685" y1="11.26" x2="-1.035" y2="11.26" width="0" layer="20"/>
<wire x1="-1.035" y1="11.26" x2="-1.035" y2="-7.135" width="0" layer="20"/>
<text>SDIN</text>
<text>-2.5V</text>
<text>5V</text>
<text>GND</text>
<text>VIN</text>
<text>AD5453 Breakout
Clemson University
Josiah Hester</text>
<text>SCLK</text>
<text>!SYNC</text>
<text>EN</text>
<text>AD5453 Breakout
Clemson University
Josiah Hester</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="parts">
<packages>
<package name="TSOT23-6">
<description>&lt;b&gt;S6 Package 6-Lead Plastic TSOT-23&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/623012fb.pdf</description>
</package>
<package name="SOP65P490X110-8N">
</package>
<package name="SOT65P210X110-5N">
</package>
<package name="SOT95P280X145-5N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="U2" library="parts" package="TSOT23-6" value="REG710"/>
<element name="CPUMP" library="SparkFun-Capacitors" package="0805" value="0.22uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="COUT" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CIN" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK"/>
<element name="DAC" library="parts" package="SOP65P490X110-8N" value="AD5453YRMZ-REEL7">
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="OC_NEWARK" value="45P6460"/>
<attribute name="MPN" value="AD5453YRMZ-REEL7"/>
<attribute name="SUPPLIER" value="Analog Devices"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="REF1" library="parts" package="SOT65P210X110-5N" value="ADR03AKSZ-REEL7">
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="OC_NEWARK" value="59K2675"/>
<attribute name="MPN" value="ADR03AKSZ-REEL7"/>
<attribute name="SUPPLIER" value="Analog Devices"/>
<attribute name="OC_FARNELL" value="1838919"/>
</element>
<element name="A1" library="parts" package="SOT95P280X145-5N" value="AD8628WARTZ-R7">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="74R6006"/>
<attribute name="MPN" value="AD8628WARTZ-R7"/>
<attribute name="SUPPLIER" value="Analog Devices"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="A2" library="parts" package="SOT95P280X145-5N" value="AD8628WARTZ-R7">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="74R6006"/>
<attribute name="MPN" value="AD8628WARTZ-R7"/>
<attribute name="SUPPLIER" value="Analog Devices"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1pF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="2"/>
<contactref element="CIN" pad="2"/>
<contactref element="COUT" pad="2"/>
<contactref element="A2" pad="2"/>
<contactref element="A2" pad="3"/>
<contactref element="DAC" pad="2"/>
<contactref element="A1" pad="2"/>
<contactref element="A1" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="1"/>
<contactref element="COUT" pad="1"/>
<contactref element="A2" pad="5"/>
<contactref element="DAC" pad="6"/>
<contactref element="A1" pad="5"/>
<contactref element="REF1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="6"/>
<contactref element="CPUMP" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="CPUMP" pad="2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="EN">
<contactref element="U2" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U2" pad="5"/>
<contactref element="CIN" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="A2" pad="4"/>
<contactref element="REF1" pad="4"/>
</signal>
<signal name="-2.5V">
<contactref element="REF1" pad="2"/>
<contactref element="A2" pad="1"/>
<contactref element="DAC" pad="7"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="DAC" pad="1"/>
<contactref element="A1" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="DAC" pad="8"/>
<contactref element="A1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="!SYNC">
<contactref element="DAC" pad="5"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SCLK">
<contactref element="DAC" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SDIN">
<contactref element="DAC" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
