<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-7.239" y1="55.677" x2="-7.239" y2="2.54" width="0" layer="20"/>
<wire x1="-7.239" y1="2.54" x2="-4.699" y2="0" width="0" layer="20" curve="90"/>
<wire x1="-4.699" y1="0" x2="74.148" y2="0" width="0" layer="20"/>
<wire x1="74.148" y1="0" x2="76.688" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="76.688" y1="2.54" x2="76.688" y2="55.677" width="0" layer="20"/>
<wire x1="76.688" y1="55.677" x2="74.148" y2="58.217" width="0" layer="20" curve="90"/>
<wire x1="74.148" y1="58.217" x2="-4.699" y2="58.217" width="0" layer="20"/>
<wire x1="-4.699" y1="58.217" x2="-7.239" y2="55.677" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="notecard">
<packages>
<package name="NOTECARD">
<description>&lt;b&gt;MDT420E01001-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="RaspberryPi_Pico">
<description>&lt;h2&gt;Raspberry Pi Pico Library&lt;/h2&gt;
&lt;h4&gt;SMD &amp; Through Hole Footprints&lt;/h4&gt;
&lt;h4&gt;Pinout Based Schematic Symbol.</description>
<packages>
<package name="RPI_PICO_TH">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="notecard" package="NOTECARD" value="MDT420E01001NOTECARD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="RaspberryPi_Pico" package="RPI_PICO_TH" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X04_1MM_RA" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0">
<attribute name="POPULARITY" value="3"/>
</element>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0">
<attribute name="POPULARITY" value="3"/>
</element>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0">
<attribute name="POPULARITY" value="3"/>
</element>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0">
<attribute name="POPULARITY" value="3"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="GND@1"/>
<contactref element="U1" pad="GND@2"/>
<contactref element="U1" pad="GND@3"/>
<contactref element="U1" pad="GND@4"/>
<contactref element="U1" pad="GND@5"/>
<contactref element="U1" pad="GND@6"/>
<contactref element="U1" pad="GND@7"/>
<contactref element="U1" pad="GND@8"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="11"/>
<contactref element="J1" pad="33"/>
<contactref element="J1" pad="45"/>
<contactref element="J1" pad="39"/>
<contactref element="J1" pad="51"/>
<contactref element="J1" pad="57"/>
<contactref element="J1" pad="73"/>
<contactref element="J1" pad="71"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="MP1"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="18"/>
<contactref element="J1" pad="MP2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="3V3"/>
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="74"/>
<contactref element="J1" pad="72"/>
<contactref element="J1" pad="70"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="GP16"/>
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="42"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="GP17"/>
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="40"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
