<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.2">
<drawing>
<board>
<plain>
<text>Left and Right Side LEDs
are mounted different!</text>
<hole x="3" y="53" drill="2"/>
<hole x="47" y="53" drill="2"/>
<hole x="3" y="3" drill="2"/>
<hole x="47" y="3" drill="2"/>
<wire x1="46.5" y1="0" x2="50" y2="3.5" width="0" layer="20" curve="90"/>
<wire x1="50" y1="3.5" x2="50" y2="52.754" width="0" layer="20"/>
<wire x1="50" y1="52.754" x2="47.008" y2="56" width="0" layer="20" curve="90"/>
<wire x1="47.008" y1="56" x2="3.5" y2="56" width="0" layer="20"/>
<wire x1="3.5" y1="56" x2="0" y2="52.5" width="0" layer="20" curve="90"/>
<wire x1="0" y1="52.5" x2="0" y2="3.5" width="0" layer="20"/>
<wire x1="0" y1="3.5" x2="3.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.5" y1="0" x2="46.5" y2="0" width="0" layer="20"/>
<text>PT4115</text>
<text>LED-</text>
<text>LED+</text>
<text>GND</text>
<text>GND</text>
<text>PWM</text>
<text>VCC</text>
<text>VCC</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>Sense</text>
<text>-</text>
<text>-</text>
<text>-</text>
</plain>
<libraries>
<library name="timon-diverses">
<packages>
<package name="FUSE-HOLDER-5X20MM">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LUXEON">
</package>
</packages>
</library>
<library name="PT4115">
<packages>
<package name="PT4115">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE-KIT">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="inductor-coilcraft">
<description>&lt;b&gt;Coilcraft SMD Inductors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;br&gt;
Modified: by Eugene Sadovoi evgeni@eniks.com&lt;/author&gt;</description>
<packages>
<package name="MSS1260">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GND-CLIP" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="GND-CLIP2" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="LED-1" library="SparkFun-LED" package="LUXEON" value="LUXEONSMD"/>
<element name="LED-2" library="SparkFun-LED" package="LUXEON" value="LUXEONSMD"/>
<element name="LED-3" library="SparkFun-LED" package="LUXEON" value="LUXEONSMD"/>
<element name="LED-4" library="SparkFun-LED" package="LUXEON" value="LUXEONSMD"/>
<element name="PWM-CLIP" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="VCC-CLIP" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="VCC-CLIP2" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="IC4" library="PT4115" package="PT4115" value=""/>
<element name="R2" library="SparkFun-Resistors" package="1206" value="0.3"/>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE-KIT" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="PANASONIC_E" value="100uF"/>
<element name="INDUCTOR" library="inductor-coilcraft" package="MSS1260" value="">
<attribute name="VALUE"/>
</element>
<element name="VCC-CLIP1" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="VCC-CLIP3" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="GND-CLIP1" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="GND-CLIP3" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="PWM-CLIP1" library="timon-diverses" package="FUSE-HOLDER-5X20MM" value="FUSE-HOLDER-5X20MM"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE-KIT" value=""/>
<element name="R1" library="SparkFun-Resistors" package="1206" value="2k"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC4" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="GND">
<contactref element="GND-CLIP" pad="CLIP-INPUT1"/>
<contactref element="GND-CLIP" pad="CLIP-INPUT2"/>
<contactref element="GND-CLIP2" pad="CLIP-INPUT1"/>
<contactref element="GND-CLIP2" pad="CLIP-INPUT2"/>
<contactref element="IC4" pad="2"/>
<contactref element="IC4" pad="2A"/>
<contactref element="C1" pad="-"/>
<contactref element="LED-1" pad="S"/>
<contactref element="GND-CLIP1" pad="CLIP-INPUT2"/>
<contactref element="GND-CLIP1" pad="CLIP-INPUT1"/>
<contactref element="GND-CLIP3" pad="CLIP-INPUT2"/>
<contactref element="GND-CLIP3" pad="CLIP-INPUT1"/>
<contactref element="LED-4" pad="S"/>
</signal>
<signal name="LED-">
<contactref element="LED-3" pad="C"/>
<contactref element="INDUCTOR" pad="P$1"/>
</signal>
<signal name="LED+">
<contactref element="LED-1" pad="A"/>
<contactref element="R2" pad="1"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="PWM">
<contactref element="PWM-CLIP" pad="CLIP-INPUT1"/>
<contactref element="PWM-CLIP" pad="CLIP-INPUT2"/>
<contactref element="PWM-CLIP1" pad="CLIP-INPUT2"/>
<contactref element="PWM-CLIP1" pad="CLIP-INPUT1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="A"/>
<contactref element="IC4" pad="1"/>
<contactref element="INDUCTOR" pad="P$2"/>
</signal>
<signal name="VCC-RAW">
<contactref element="VCC-CLIP2" pad="CLIP-INPUT1"/>
<contactref element="VCC-CLIP2" pad="CLIP-INPUT2"/>
<contactref element="VCC-CLIP" pad="CLIP-INPUT1"/>
<contactref element="VCC-CLIP" pad="CLIP-INPUT2"/>
<contactref element="VCC-CLIP1" pad="CLIP-INPUT2"/>
<contactref element="VCC-CLIP1" pad="CLIP-INPUT1"/>
<contactref element="VCC-CLIP3" pad="CLIP-INPUT2"/>
<contactref element="VCC-CLIP3" pad="CLIP-INPUT1"/>
<contactref element="D1" pad="A"/>
<contactref element="LED-3" pad="S"/>
<contactref element="LED-2" pad="S"/>
</signal>
<signal name="N$2">
<contactref element="LED-4" pad="C"/>
<contactref element="LED-2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="LED-2" pad="C"/>
<contactref element="LED-3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="LED-1" pad="C"/>
<contactref element="LED-4" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="IC4" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
