<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="43.9728" y2="0" width="0" layer="20"/>
<wire x1="43.9728" y1="0" x2="43.9728" y2="32.69" width="0" layer="20"/>
<wire x1="43.9728" y1="32.69" x2="0" y2="32.69" width="0" layer="20"/>
<wire x1="0" y1="32.69" x2="0" y2="0" width="0" layer="20"/>
<hole x="41.91" y="30.7086" drill="3.2"/>
<hole x="2.0828" y="30.6324" drill="3.2"/>
<hole x="2.0066" y="2.032" drill="3.2"/>
<hole x="41.8084" y="2.1082" drill="3.2"/>
<text>G
N
D</text>
<text>V</text>
<text>A</text>
<text>INPUT</text>
<text>OUTPUT</text>
<text>GND</text>
<text>V</text>
<text>A</text>
<text>Intvwiki-rev1
grips03-free</text>
<text>Intvwiki-rev1
grips03-free</text>
<text>+5V</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LONGPADS">
</package>
<package name="1X03_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="15K" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="22K" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="100UF" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="2N3904" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="PROD_ID" value="TRANS-08447"/>
</element>
<element name="100UF,." library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="." library="SparkFun-Connectors" package="1X04_LONGPADS" value=""/>
<element name="," library="SparkFun-Connectors" package="1X03_LONGPADS" value=""/>
<element name="2N3904_" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="PROD_ID" value="TRANS-08447"/>
</element>
<element name="660" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="330" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="51K" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="33K" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="100UF.." library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="75" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="22" library="SparkFun-Resistors" package="AXIAL-0.4" value=""/>
<element name="100UF.," library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="." pad="2"/>
<contactref element="," pad="3"/>
<contactref element="22K" pad="P$1"/>
<contactref element="33K" pad="P$1"/>
<contactref element="330" pad="P$1"/>
<contactref element="22" pad="P$1"/>
</signal>
<signal name="VIDEOIN">
<contactref element="." pad="3"/>
<contactref element="100UF.." pad="2"/>
</signal>
<signal name="AUDIOIN">
<contactref element="100UF,." pad="1"/>
<contactref element="." pad="4"/>
</signal>
<signal name="AUDIOOUT">
<contactref element="100UF,." pad="2"/>
<contactref element="," pad="1"/>
</signal>
<signal name="N$4">
<contactref element="15K" pad="P$1"/>
<contactref element="22K" pad="P$2"/>
<contactref element="2N3904" pad="2"/>
<contactref element="100UF.," pad="2"/>
</signal>
<signal name="VIDEOOUT">
<contactref element="100UF" pad="2"/>
<contactref element="," pad="2"/>
</signal>
<signal name="5V">
<contactref element="." pad="1"/>
<contactref element="15K" pad="P$2"/>
<contactref element="660" pad="P$2"/>
<contactref element="51K" pad="P$2"/>
<contactref element="75" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="2N3904_" pad="3"/>
<contactref element="660" pad="P$1"/>
<contactref element="100UF.," pad="1"/>
</signal>
<signal name="N$5">
<contactref element="2N3904_" pad="1"/>
<contactref element="330" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="2N3904_" pad="2"/>
<contactref element="51K" pad="P$1"/>
<contactref element="33K" pad="P$2"/>
<contactref element="100UF.." pad="1"/>
</signal>
<signal name="N$1">
<contactref element="2N3904" pad="1"/>
<contactref element="22" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="75" pad="P$1"/>
<contactref element="2N3904" pad="3"/>
<contactref element="100UF" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
