<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="16.33105625" y1="10.693825" x2="34.3146875" y2="10.698625" width="0" layer="20"/>
<wire x1="34.3146875" y1="10.698625" x2="34.278878125" y2="39.578275" width="0" layer="20"/>
<wire x1="34.278878125" y1="39.578275" x2="16.36008125" y2="39.586075" width="0" layer="20"/>
<wire x1="16.36008125" y1="39.586075" x2="16.33105625" y2="10.693825" width="0" layer="20"/>
<text>GND</text>
<text>ESP8266-01 Flash
(c) 2017 Roger Parkinson</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="EVQ-Q2">
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA6032">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP5" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CH_PD" library="adafruit" package="EVQ-Q2" value="SPST_TACT-EVQQ2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPIO0" library="adafruit" package="EVQ-Q2" value="SPST_TACT-EVQQ2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA6032" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08390"/>
</element>
<element name="FTDI" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="10k"/>
<element name="R2" library="adafruit" package="R0805" value="10k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP5" pad="1"/>
<contactref element="CH_PD" pad="B"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="P$2"/>
<contactref element="GPIO0" pad="A"/>
<contactref element="FTDI" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP6" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="P$1"/>
<contactref element="FTDI" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GPIO2">
<contactref element="JP5" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="JP5" pad="4"/>
<contactref element="FTDI" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="JP6" pad="4"/>
<contactref element="FTDI" pad="5"/>
</signal>
<signal name="GPIO0">
<contactref element="JP5" pad="3"/>
<contactref element="GPIO0" pad="B"/>
</signal>
<signal name="CH_PD">
<contactref element="JP6" pad="3"/>
<contactref element="CH_PD" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="JP6" pad="2"/>
<contactref element="FTDI" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
