<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.1">
<drawing>
<board>
<plain>
<text>VCC</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<hole x="0" y="195.072" drill="9.525"/>
<wire x1="-7.62" y1="193.04" x2="-7.62" y2="-5.08" width="0.1524" layer="46"/>
<wire x1="7.62" y1="193.04" x2="7.62" y2="-5.08" width="0.1524" layer="46"/>
<wire x1="-7.62" y1="193.04" x2="0" y2="201.93" width="0.1524" layer="46" curve="-90"/>
<wire x1="0" y1="201.93" x2="7.62" y2="193.04" width="0.1524" layer="46" curve="-90"/>
<text>DC26 #Badgelife
Shitty Add-On
Totem</text>
<wire x1="-7.62" y1="-5.08" x2="7.62" y2="-5.08" width="0.1524" layer="46"/>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="AddonTotem">
<packages>
<package name="ONEAAHOLDER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="2X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="2X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="2X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="2X02" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="AddonTotem" package="ONEAAHOLDER" value="EAGLEAABATTERY"/>
<element name="U$2" library="AddonTotem" package="ONEAAHOLDER" value="EAGLEAABATTERY"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="POS"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="U$2" pad="NEG"/>
</signal>
<signal name="SDA">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="POS"/>
<contactref element="U$1" pad="NEG"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
