<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="39.37" x2="56.82" y2="39.37" width="0" layer="20"/>
<wire x1="56.82" y1="39.37" x2="56.82" y2="78.73" width="0" layer="20"/>
<wire x1="56.82" y1="78.73" x2="3.81" y2="78.73" width="0" layer="20"/>
<wire x1="3.81" y1="78.73" x2="3.81" y2="39.37" width="0" layer="20"/>
<text>march 2014 - Alex Sciuto</text>
<text>arduino board v0.1</text>
<text>D3</text>
<text>D0</text>
<text>D6</text>
<text>D9</text>
<text>D12</text>
<text>D13</text>
<text>A0</text>
<text>A3</text>
<text>A5</text>
<text>D1</text>
<text>D2</text>
<text>D4</text>
<text>D5</text>
<text>D7</text>
<text>D8</text>
<text>D10</text>
<text>D11</text>
<text>A1</text>
<text>A2</text>
<text>A4</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-PTH">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-5MM">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="78L05" library="SparkFun-PowerIC" package="78XXL" value=""/>
<element name="RESONATOR" library="SparkFun-FreqCtrl" package="RESONATOR-PTH" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="0.1uF"/>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value=".1uF"/>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value=".33uF"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="10K"/>
<element name="IC2" library="atmel" package="DIL28-3" value="MEGA8-P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X20" value="">
<attribute name="VALUE"/>
</element>
<element name="ICP" library="pinhead" package="2X03" value=""/>
<element name="AREF" library="pinhead" package="1X01" value=""/>
<element name="BBPWR" library="pinhead" package="1X02" value=""/>
<element name="EXTPWR" library="pinhead" package="1X03" value=""/>
</elements>
<signals>
<signal name="N$6">
<contactref element="IC2" pad="10"/>
<contactref element="RESONATOR" pad="3"/>
</signal>
<signal name="A0">
<contactref element="IC2" pad="23"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="A1">
<contactref element="IC2" pad="24"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="A2">
<contactref element="IC2" pad="25"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="A3">
<contactref element="IC2" pad="26"/>
<contactref element="JP2" pad="18"/>
</signal>
<signal name="A4">
<contactref element="IC2" pad="27"/>
<contactref element="JP2" pad="19"/>
</signal>
<signal name="A5">
<contactref element="IC2" pad="28"/>
<contactref element="JP2" pad="20"/>
</signal>
<signal name="D0">
<contactref element="IC2" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D1">
<contactref element="IC2" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="D2">
<contactref element="IC2" pad="4"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D3">
<contactref element="JP2" pad="4"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="D4">
<contactref element="IC2" pad="6"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="D5">
<contactref element="IC2" pad="11"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="D6">
<contactref element="IC2" pad="12"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="D7">
<contactref element="IC2" pad="13"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="D8">
<contactref element="IC2" pad="14"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="D9">
<contactref element="IC2" pad="15"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="D10">
<contactref element="IC2" pad="16"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="D11">
<contactref element="IC2" pad="17"/>
<contactref element="JP2" pad="12"/>
<contactref element="ICP" pad="4"/>
</signal>
<signal name="D12">
<contactref element="IC2" pad="18"/>
<contactref element="JP2" pad="13"/>
<contactref element="ICP" pad="1"/>
</signal>
<signal name="D13">
<contactref element="IC2" pad="19"/>
<contactref element="JP2" pad="14"/>
<contactref element="ICP" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="IC2" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="BBPWR" pad="1"/>
<contactref element="IC2" pad="20"/>
<contactref element="ICP" pad="2"/>
<contactref element="78L05" pad="OUT"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="22"/>
<contactref element="IC2" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="RESONATOR" pad="2"/>
<contactref element="78L05" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="EXTPWR" pad="2"/>
<contactref element="BBPWR" pad="2"/>
<contactref element="ICP" pad="6"/>
</signal>
<signal name="AREF">
<contactref element="AREF" pad="1"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="RESET">
<contactref element="ICP" pad="5"/>
<contactref element="IC2" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="V+">
<contactref element="78L05" pad="IN"/>
<contactref element="C3" pad="1"/>
<contactref element="EXTPWR" pad="1"/>
<contactref element="EXTPWR" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="9"/>
<contactref element="RESONATOR" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
