<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="54.335603125" y1="0.832371875" x2="54.360184375" y2="26.6628" width="0" layer="20"/>
<wire x1="54.360184375" y1="26.6628" x2="53.0835375" y2="27.940175" width="0" layer="20" curve="90.055681"/>
<wire x1="53.0835375" y1="27.940175" x2="45.571215625" y2="27.94001875" width="0" layer="20"/>
<wire x1="45.571215625" y1="27.94001875" x2="44.45" y2="27.072784375" width="0" layer="20" curve="87.480178"/>
<wire x1="44.45" y1="27.072784375" x2="44.45" y2="18.647221875" width="0" layer="20"/>
<wire x1="44.45" y1="18.647221875" x2="43.836778125" y2="17.78" width="0" layer="20" curve="-90"/>
<wire x1="43.836778125" y1="17.78" x2="10.773221875" y2="17.78" width="0" layer="20"/>
<wire x1="10.773221875" y1="17.78" x2="10.16" y2="18.647221875" width="0" layer="20" curve="-90"/>
<wire x1="10.16" y1="18.647221875" x2="10.16" y2="26.818659375" width="0" layer="20"/>
<wire x1="10.16" y1="26.818659375" x2="9.292459375" y2="27.9402" width="0" layer="20" curve="90"/>
<wire x1="9.292459375" y1="27.9402" x2="1.629540625" y2="27.9402" width="0" layer="20"/>
<wire x1="1.629540625" y1="27.9402" x2="0" y2="26.818659375" width="0" layer="20" curve="90"/>
<wire x1="0" y1="26.818659375" x2="0" y2="0.61283125" width="0" layer="20"/>
<wire x1="0" y1="0.61283125" x2="1.378534375" y2="0.00053125" width="0" layer="20" curve="90.279433"/>
<wire x1="1.378534375" y1="0.00053125" x2="53.508921875" y2="0.000825" width="0" layer="20"/>
<wire x1="53.508921875" y1="0.000825" x2="54.335603125" y2="0.832371875" width="0" layer="20" curve="89.765558"/>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>PowerDough V1.1
Phantomic Labs, LLC
2019</text>
<text>PowerDough V1.1
Phantomic Labs, LLC
2019</text>
<text>24V 2A Max.</text>
<text>-</text>
</plain>
<libraries>
<library name="Seeed-Connector">
<packages>
<package name="H2-3.5-7.0X7.0MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BANANA_CONN">
<description>&lt;h3&gt;Banana Plug PTH&lt;/h3&gt;
0.2" diameter pad, 0.1" hole. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BANANA_CONN&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_SMT_POSTS">
<description>&lt;h3&gt;Surface Mount - 2x3 Male Header with Keying Posts&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15881.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_PTH_BREAD">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector Breadboard Compatible&lt;/h3&gt;
Breadboard-friendly pins. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/18742.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="TAB_GATOR_MINI">
</package>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MICROB">
<description>&lt;h3&gt;USB Type microUSB Connector-No Bossed Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5 pins, 4 shield connections&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Micro-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Seeed-Connector" package="H2-3.5-7.0X7.0MM" value="GREEN-2P-3.5"/>
<element name="J2" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="BANANA_CONN" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="2X3_SMT_POSTS" value="">
<attribute name="PROD_ID" value="CONN-11415"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="2X3_SMT_POSTS" value="">
<attribute name="PROD_ID" value="CONN-11415"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="POWER_JACK_PTH_BREAD" value="POWER_JACKPTH_BREAD">
<attribute name="PROD_ID" value="PRT-10811"/>
<attribute name="SPICEPREFIX" value="J"/>
</element>
<element name="U$1" library="SparkFun-Connectors" package="TAB_GATOR_MINI" value="TAB_GATOR_MINI"/>
<element name="U$2" library="SparkFun-Connectors" package="TAB_GATOR_MINI" value="TAB_GATOR_MINI"/>
<element name="J7" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="USB-MICROB" value="">
<attribute name="PROD_ID" value="CONN-09505"/>
<attribute name="SF_ID" value="PRT-08533"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="P$1"/>
<contactref element="J1" pad="2"/>
<contactref element="J6" pad="GND"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="6"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="6"/>
<contactref element="U$1" pad="P1"/>
<contactref element="J7" pad="2"/>
<contactref element="J7" pad="4"/>
<contactref element="J7" pad="6"/>
<contactref element="J7" pad="8"/>
<contactref element="J9" pad="GND"/>
</signal>
<signal name="VIN">
<contactref element="J6" pad="PWR"/>
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="P$1"/>
<contactref element="J4" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="5"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="5"/>
<contactref element="U$2" pad="P1"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="5"/>
<contactref element="J7" pad="7"/>
<contactref element="J9" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
