<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.73" y2="0" width="0" layer="20"/>
<wire x1="31.73" y1="0" x2="31.73" y2="50.47" width="0" layer="20"/>
<wire x1="31.73" y1="50.47" x2="0" y2="50.47" width="0" layer="20"/>
<wire x1="0" y1="50.47" x2="0" y2="0" width="0" layer="20"/>
<text>Servo 1</text>
<text>Servo 2</text>
<text>Servo 3</text>
<text>Servo 4</text>
<text>Power</text>
<text>10DOF</text>
<text>I2C</text>
<text>Rocket Control Board Version 1</text>
<text>Designed By Jeremy Hall</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MINI">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
<package name="1X03">
</package>
<package name="1X08_ROUND">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M_COPPER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Boards" package="ARDUINO_PRO_MINI" value="ARDUINO_PRO_MINI"/>
<element name="J1" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="SERVO1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SERVO2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SERVO3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SERVO4" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M_COPPER" value="OSHW-LOGOM-COPPER"/>
</elements>
<signals>
<signal name="5V">
<contactref element="SERVO1" pad="3"/>
<contactref element="SERVO2" pad="3"/>
<contactref element="SERVO3" pad="3"/>
<contactref element="SERVO4" pad="3"/>
</signal>
<signal name="GND">
<contactref element="SERVO1" pad="2"/>
<contactref element="SERVO2" pad="2"/>
<contactref element="SERVO3" pad="2"/>
<contactref element="SERVO4" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="U$1" pad="23"/>
<contactref element="J3" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="SERVO1">
<contactref element="SERVO1" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="SERVO2">
<contactref element="SERVO2" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="SERVO3">
<contactref element="SERVO3" pad="1"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="SERVO4">
<contactref element="SERVO4" pad="1"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="21"/>
<contactref element="J3" pad="4"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="24"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J6" pad="8"/>
</signal>
<signal name="SCL">
<contactref element="J3" pad="2"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="J3" pad="1"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="3V3">
<contactref element="J2" pad="4"/>
<contactref element="J6" pad="7"/>
</signal>
<signal name="SS">
<contactref element="U$1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
