<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.78" y2="0" width="0" layer="20"/>
<wire x1="50.78" y1="0" x2="50.78" y2="27.61" width="0" layer="20"/>
<wire x1="50.78" y1="27.61" x2="0" y2="27.61" width="0" layer="20"/>
<wire x1="0" y1="27.61" x2="0" y2="0" width="0" layer="20"/>
<text>555 Crowbar STM8 Glitcher, REV A
Layout by Hong's Electronics, LLC
Original design by Jarrett Ranier
https://jrainimo.com/build/2022/01/dumping-firmware-with-a-555/</text>
<text>555 Crowbar STM8 Glitcher, REV A</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TRIM-3386">
</package>
</packages>
</library>
<library name="SparkFun-IC-Special-Function">
<description>&lt;h3&gt;SparkFun Special Function ICs&lt;/h3&gt;
This library contains ICs that do not really fit into the other, more generic categories.  Basically, anything that serves some function but has a bunch of brains or special bias circuitry that prevents it from being used as a general part qualifies for this category.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;555 timers&lt;/li&gt;
&lt;li&gt;LED drivers&lt;/li&gt;
&lt;li&gt;H-Bridge drivers&lt;/li&gt;
&lt;li&gt;Motor drivers&lt;/li&gt;
&lt;li&gt;Waveform generators&lt;/li&gt;
&lt;li&gt;Crypto&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SparkFun-IC-Special-Function" package="SO08" value="555">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="NA-XXXXX"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SparkFun-IC-Special-Function" package="SO08" value="555">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="NA-XXXXX"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="TO220V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="500">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TM1" library="adafruit" package="TRIM-3386" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TM2" library="adafruit" package="TRIM-3386" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="C5" pad="1"/>
<contactref element="TM1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="6"/>
<contactref element="C6" pad="1"/>
<contactref element="TM2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="5"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IN">
<contactref element="C4" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC2" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="1"/>
<contactref element="TM1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="1"/>
<contactref element="TM2" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="Q1" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
