<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0.254" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="67.31" width="0.254" layer="20"/>
<wire x1="30.48" y1="67.31" x2="0" y2="67.31" width="0.254" layer="20"/>
<wire x1="0" y1="67.31" x2="0" y2="0" width="0.254" layer="20"/>
<text>0</text>
<text>7</text>
<text>4</text>
<text>3</text>
<text>A</text>
<text>H</text>
<text>H</text>
<text>A</text>
<text>BRN</text>
<text>BLK</text>
<text>5V</text>
<text>GND</text>
<text>P</text>
<text>G</text>
<text>B</text>
<text>PANEL SHIFT REGISTER BOARD</text>
<text>REV D, 1/21/2018</text>
<text>0</text>
<text>3</text>
<text>7</text>
<text>4</text>
<text>H</text>
<text>A</text>
<text>H</text>
<text>A</text>
<text>P</text>
<text>G</text>
<text>B</text>
<text>5V</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10">
<description>&lt;h3&gt;Plated Through Hole -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="TPIC6B595">
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Logic">
<description>&lt;h3&gt;SparkFun Logic ICs&lt;/h3&gt;
This library contains parts which fit into the standard logic IC families.&lt;br&gt;&lt;br&gt;
This library is special as the devices are most generalized, with manufacturer specific variants stemming from the generalized numbers.  It also uses individual gates for common parts with a power consort.  Place the gates in a schematic such that they are easy to see in the circuit, and apply power to the power symbol for multigate packages. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V-LEDS" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="BUTTON-COL" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="BUTTONS" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
<element name="DRAIN_REG" library="TPIC6B595" package="DIL20" value="TPIC6B595N"/>
<element name="LIGHTS" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="RIBBON" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
</element>
<element name="BUTTON_REG" library="SparkFun-IC-Logic" package="DIP16" value="SN74HC595N ">
<attribute name="PROD_ID" value="IC-13123"/>
</element>
<element name="LIGHT_REG" library="SparkFun-IC-Logic" package="DIP16" value="SN74HC595N ">
<attribute name="PROD_ID" value="IC-13123"/>
</element>
<element name="DRAINS_1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="DRAINS_2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
</elements>
<signals>
<signal name="N$9">
<contactref element="LIGHT_REG" pad="15"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="LIGHT_REG" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="LIGHT_REG" pad="2"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="LIGHT_REG" pad="3"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="LIGHT_REG" pad="4"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="LIGHT_REG" pad="5"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="LIGHT_REG" pad="6"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="LIGHT_REG" pad="7"/>
<contactref element="R11" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="LIGHT_REG" pad="9"/>
<contactref element="DRAIN_REG" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="BUTTON_REG" pad="9"/>
<contactref element="LIGHT_REG" pad="14"/>
</signal>
<signal name="N$19">
<contactref element="R4" pad="P$2"/>
<contactref element="LIGHTS" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R5" pad="P$2"/>
<contactref element="LIGHTS" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R6" pad="P$2"/>
<contactref element="LIGHTS" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="R7" pad="P$2"/>
<contactref element="LIGHTS" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="R8" pad="P$2"/>
<contactref element="LIGHTS" pad="5"/>
</signal>
<signal name="N$24">
<contactref element="R9" pad="P$2"/>
<contactref element="LIGHTS" pad="6"/>
</signal>
<signal name="N$25">
<contactref element="R10" pad="P$2"/>
<contactref element="LIGHTS" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="R11" pad="P$2"/>
<contactref element="LIGHTS" pad="8"/>
</signal>
<signal name="GND">
<contactref element="RIBBON" pad="1"/>
<contactref element="BUTTON_REG" pad="8"/>
<contactref element="DRAIN_REG" pad="10"/>
<contactref element="DRAIN_REG" pad="11"/>
<contactref element="DRAIN_REG" pad="19"/>
<contactref element="LIGHT_REG" pad="8"/>
<contactref element="5V-LEDS" pad="2"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="5V">
<contactref element="RIBBON" pad="2"/>
<contactref element="5V-LEDS" pad="1"/>
</signal>
<signal name="3V">
<contactref element="RIBBON" pad="3"/>
<contactref element="BUTTON_REG" pad="16"/>
<contactref element="BUTTON_REG" pad="10"/>
<contactref element="LIGHT_REG" pad="16"/>
<contactref element="DRAIN_REG" pad="2"/>
<contactref element="LIGHT_REG" pad="10"/>
<contactref element="DRAIN_REG" pad="8"/>
</signal>
<signal name="N$27">
<contactref element="BUTTON_REG" pad="15"/>
<contactref element="BUTTONS" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="BUTTON_REG" pad="1"/>
<contactref element="BUTTONS" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="BUTTON_REG" pad="2"/>
<contactref element="BUTTONS" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="BUTTON_REG" pad="3"/>
<contactref element="BUTTONS" pad="4"/>
</signal>
<signal name="N$31">
<contactref element="BUTTON_REG" pad="4"/>
<contactref element="BUTTONS" pad="5"/>
</signal>
<signal name="N$32">
<contactref element="BUTTON_REG" pad="5"/>
<contactref element="BUTTONS" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="BUTTON_REG" pad="6"/>
<contactref element="BUTTONS" pad="7"/>
</signal>
<signal name="N$34">
<contactref element="BUTTON_REG" pad="7"/>
<contactref element="BUTTONS" pad="8"/>
</signal>
<signal name="CLK">
<contactref element="RIBBON" pad="4"/>
<contactref element="BUTTON_REG" pad="11"/>
<contactref element="LIGHT_REG" pad="11"/>
<contactref element="DRAIN_REG" pad="13"/>
</signal>
<signal name="N$37">
<contactref element="RIBBON" pad="6"/>
<contactref element="BUTTON_REG" pad="14"/>
</signal>
<signal name="OE">
<contactref element="RIBBON" pad="9"/>
<contactref element="BUTTON_REG" pad="13"/>
<contactref element="LIGHT_REG" pad="13"/>
<contactref element="DRAIN_REG" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="RIBBON" pad="7"/>
<contactref element="R1" pad="P$2"/>
<contactref element="BUTTON-COL" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="RIBBON" pad="8"/>
<contactref element="R2" pad="P$2"/>
<contactref element="BUTTON-COL" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="RIBBON" pad="10"/>
<contactref element="R3" pad="P$2"/>
<contactref element="BUTTON-COL" pad="3"/>
</signal>
<signal name="RCK">
<contactref element="DRAIN_REG" pad="12"/>
<contactref element="LIGHT_REG" pad="12"/>
<contactref element="RIBBON" pad="5"/>
<contactref element="BUTTON_REG" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="DRAINS_1" pad="1"/>
<contactref element="DRAIN_REG" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="DRAINS_1" pad="2"/>
<contactref element="DRAIN_REG" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="DRAINS_1" pad="3"/>
<contactref element="DRAIN_REG" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="DRAINS_1" pad="4"/>
<contactref element="DRAIN_REG" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="DRAINS_2" pad="1"/>
<contactref element="DRAIN_REG" pad="14"/>
</signal>
<signal name="N$6">
<contactref element="DRAINS_2" pad="2"/>
<contactref element="DRAIN_REG" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="DRAINS_2" pad="3"/>
<contactref element="DRAIN_REG" pad="16"/>
</signal>
<signal name="N$8">
<contactref element="DRAINS_2" pad="4"/>
<contactref element="DRAIN_REG" pad="17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
