<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="79.756" y2="0" width="0.254" layer="20"/>
<wire x1="79.756" y1="0" x2="79.756" y2="60.198" width="0.254" layer="20"/>
<wire x1="79.756" y1="60.198" x2="0" y2="60.198" width="0.254" layer="20"/>
<wire x1="0" y1="60.198" x2="0" y2="0" width="0.254" layer="20"/>
<text>X</text>
<text>Y</text>
<text>Z</text>
<text>XYZ Axis
 Select</text>
<text>X</text>
<text>Y</text>
<text>Z</text>
<text>A=A</text>
<text>RV-Project.Com 
CylonEye Accelerometer
      Ver L1.0</text>
<text>Coarse XYZ Adj</text>
<text>LED+</text>
<text>GND</text>
<text>DATA</text>
<text>GND</text>
<text>12V</text>
<text>LED+
GND

DATA
GND
+12V</text>
<text>Fine XYZ Adj</text>
<text>Invert</text>
</plain>
<libraries>
<library name="alsstuff">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_200MIL(10MM)">
</package>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>&lt;h3&gt;Ceramic Capacitor&lt;/h3&gt;
Commonly used for small ceramic capacitors 0150 spacing.</description>
</package>
<package name="WAFER5PIN">
</package>
<package name="ADIFRUIT_ADXL335">
</package>
<package name="1/4W_AXIAL">
<description>Standard Axial 1/4Watt Resistor&lt;p&gt;0.45" footprint</description>
</package>
<package name="SR10010-5POSITION">
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="TO-220-HEATSINK-1">
</package>
<package name="CHINESE_TEST_PIN">
</package>
<package name="BOURNS3362_P">
<description>Standard Bourns Cermet Trimmer
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/54/3362-55248.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SP19L">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="alsstuff" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10UF">
<attribute name="PROD_ID" value="CAP-08440"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="alsstuff" package="WAFER5PIN" value="WAFER5PHORIZONTAL">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="alsstuff" package="ADIFRUIT_ADXL335" value="ADAFRUIT_ADXL335">
<attribute name="NAME"/>
</element>
<element name="R1" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="alsstuff" package="1/4W_AXIAL" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="alsstuff" package="1/4W_AXIAL" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="alsstuff" package="1/4W_AXIAL" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="alsstuff" package="1/4W_AXIAL" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="alsstuff" package="1/4W_AXIAL" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="alsstuff" package="1/4W_AXIAL" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="alsstuff" package="SR10010-5POSITION" value="SR10010F(4~5~6POSITIONSWITCH)">
<attribute name="NAME"/>
</element>
<element name="U1" library="alsstuff" package="DIP08" value="TINY85">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="alsstuff" package="TO-220-HEATSINK-1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="alsstuff" package="CHINESE_TEST_PIN" value="CHINESE_TEST_PIN">
<attribute name="NAME"/>
</element>
<element name="TP2" library="alsstuff" package="CHINESE_TEST_PIN" value="CHINESE_TEST_PIN">
<attribute name="NAME"/>
</element>
<element name="R12" library="pot" package="SP19L" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="alsstuff" package="BOURNS3362_P" value="5k">
<attribute name="MARKING" value="103"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R5" pad="1"/>
<contactref element="S1" pad="R1"/>
<contactref element="R6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="GND"/>
<contactref element="C6" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="J1" pad="P$4"/>
<contactref element="J1" pad="P$2"/>
<contactref element="M1" pad="GND"/>
<contactref element="JP1" pad="8"/>
<contactref element="R12" pad="S"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="S1" pad="F4"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="S1" pad="F1"/>
</signal>
<signal name="N$9">
<contactref element="S1" pad="FC"/>
<contactref element="S1" pad="RC"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="OUT"/>
<contactref element="D1" pad="A"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R7" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="J1" pad="P$5"/>
<contactref element="R8" pad="2"/>
<contactref element="M1" pad="VIN"/>
<contactref element="R1" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="12V">
<contactref element="U2" pad="IN"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="P$3"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="S1" pad="F3"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="S1" pad="F2"/>
</signal>
<signal name="N$2">
<contactref element="M1" pad="ZOUT"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="M1" pad="YOUT"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="M1" pad="XOUT"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="3"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="1"/>
<contactref element="R13" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
