<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="46.66" y1="15.24" x2="46.66" y2="68.58" width="0" layer="20"/>
<wire x1="46.66" y1="68.58" x2="42.86" y2="72.38" width="0" layer="20" curve="90"/>
<wire x1="42.86" y1="72.38" x2="17.78" y2="72.38" width="0" layer="20"/>
<wire x1="17.78" y1="72.38" x2="12.7" y2="67.3" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="67.3" x2="12.7" y2="16.51" width="0" layer="20"/>
<wire x1="12.7" y1="16.51" x2="17.78" y2="11.43" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="11.43" x2="42.85" y2="11.43" width="0" layer="20"/>
<wire x1="42.85" y1="11.43" x2="46.66" y2="15.24" width="0" layer="20" curve="90"/>
<text>gnd</text>
<text>5v</text>
<text>CUI - PYB20
48Vdc-5Vdc
03/13/18</text>
<text>PYB20-Q48-S5</text>
<text>5vdc</text>
<text>gnd</text>
<text>48Vdc</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="eagle_libraries">
<packages>
<package name="STANDOFF-ELECTRICAL">
<description>#8 screw hole, 170mill, 0.30 mask</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="th_libraries">
<packages>
<package name="CUI_PYB20_PCB_DC_DC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="eagle_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="U$1" library="th_libraries" package="CUI_PYB20_PCB_DC_DC" value="PYB20">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="J15" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J16" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J17" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J18" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J19" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value=""/>
</elements>
<signals>
<signal name="GND">
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="J17" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="J8" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="J16" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="5"/>
<contactref element="J15" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="J19" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="3"/>
<contactref element="J15" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="J18" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
