<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<text>SDA</text>
<text>AD0</text>
<text>V+</text>
<text>SCL</text>
<text>GND</text>
<text>ALRT</text>
<wire x1="2.54" y1="16.51" x2="17.78" y2="16.51" width="0.1524" layer="20"/>
<wire x1="17.78" y1="16.51" x2="17.78" y2="3.81" width="0.1524" layer="20"/>
<wire x1="17.78" y1="3.81" x2="2.54" y2="3.81" width="0.1524" layer="20"/>
<wire x1="2.54" y1="3.81" x2="2.54" y2="16.51" width="0.1524" layer="20"/>
<text>TMP101</text>
<text>TMP101</text>
<text>UHMC Micro
Climate PROJECT</text>
<text>296-27725</text>
<text>V1</text>
<text>16SEPT17</text>
<text>UHMC Micro
Climate PROJECT</text>
</plain>
<libraries>
<library name="KEMET">
<packages>
<package name="0805_C">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_NO_SILK">
<description>No outline in silkscreen</description>
</package>
</packages>
</library>
<library name="LITTLE_LOGIC">
<packages>
<package name="DBV">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="KEMET" package="0805_C" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="TMP101" library="LITTLE_LOGIC" package="DBV" value="TMP101"/>
</elements>
<signals>
<signal name="SDA">
<contactref element="J2" pad="2"/>
<contactref element="TMP101" pad="6"/>
</signal>
<signal name="ADD0">
<contactref element="J2" pad="3"/>
<contactref element="TMP101" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="TMP101" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="2"/>
<contactref element="TMP101" pad="1"/>
</signal>
<signal name="ALERT">
<contactref element="J1" pad="4"/>
<contactref element="TMP101" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="TMP101" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
