<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.324" y2="0" width="0" layer="20"/>
<wire x1="25.324" y1="0" x2="25.324" y2="25.39" width="0" layer="20"/>
<wire x1="25.324" y1="25.39" x2="0" y2="25.39" width="0" layer="20"/>
<wire x1="0" y1="25.39" x2="0" y2="0" width="0" layer="20"/>
<text>5V</text>
<text>3.3V</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>VIN</text>
<text>GND</text>
<text>5V</text>
<text>3.3V</text>
<hole x="3.683" y="3.683" drill="3.96875"/>
<hole x="3.683" y="21.717" drill="3.96875"/>
<text>CameronTech.io</text>
<text>5v &amp; 3.3v</text>
<text>http://git.io/dualvolt</text>
<text>Dual Regulator</text>
<text>v1.1.1</text>
<text>GND</text>
<text>0.1uF</text>
<text>CT533</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="CAP-PTH-SMALL2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="5VREG" library="v-reg" package="78XXS" value="">
<attribute name="VALUE"/>
</element>
<element name="3.3VREG" library="v-reg" package="78XXS" value="">
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Passives" package="CAP-PTH-SMALL2" value="">
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="CAP-PTH-SMALL2" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="5VOUT" library="SparkFun-Passives" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="3.3VOUT" library="SparkFun-Passives" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="VIN" library="SparkFun-Passives" package="1X02" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="5VREG" pad="GND"/>
<contactref element="3.3VREG" pad="GND"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="5VOUT" pad="2"/>
<contactref element="3.3VOUT" pad="2"/>
<contactref element="VIN" pad="2"/>
</signal>
<signal name="5V">
<contactref element="C2" pad="1"/>
<contactref element="5VREG" pad="OUT"/>
<contactref element="C8" pad="1"/>
<contactref element="5VOUT" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="C5" pad="1"/>
<contactref element="3.3VREG" pad="OUT"/>
<contactref element="C7" pad="1"/>
<contactref element="3.3VOUT" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="5VREG" pad="IN"/>
<contactref element="C4" pad="1"/>
<contactref element="3.3VREG" pad="IN"/>
<contactref element="VIN" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
