<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="1.27" x2="18.72" y2="1.27" width="0" layer="20"/>
<wire x1="18.72" y1="1.27" x2="18.72" y2="49.52" width="0" layer="20"/>
<wire x1="18.72" y1="49.52" x2="1.27" y2="49.52" width="0" layer="20"/>
<wire x1="1.27" y1="49.52" x2="1.27" y2="1.27" width="0" layer="20"/>
<text>Dactyl L
v0.3 @joedevivo</text>
<text>Dactyl L
v0.3 @joedevivo</text>
</plain>
<libraries>
<library name="microchip-23018">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07">
<description>&lt;h3&gt;Plated Through Hole -7 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="my_parts">
<packages>
<package name="SJ-43514_HEADPHONES-3.5MM_X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MCP" library="microchip-23018" package="DIL28-3" value="MCP23018SP">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="MCP23018-E/SP"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="98M1583"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="Rows">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X07" value="Columns">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="my_parts" package="SJ-43514_HEADPHONES-3.5MM_X4" value="SJ-43514_HEADPHONES_3.5MM_X4"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="MCP" pad="15"/>
<contactref element="MCP" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="MCP" pad="11"/>
<contactref element="U$1" pad="4"/>
<contactref element="MCP" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="MCP" pad="13"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="MCP" pad="12"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="MCP" pad="20"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="MCP" pad="21"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="MCP" pad="22"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="MCP" pad="23"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="MCP" pad="24"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="MCP" pad="25"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="MCP" pad="26"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="MCP" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="MCP" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="MCP" pad="5"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="MCP" pad="6"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="MCP" pad="7"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="MCP" pad="8"/>
<contactref element="J1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
