<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>16-BIT ATX ISA SYSTEM BACKPLANE</text>
<text>OPTION ROM</text>
<wire x1="0" y1="0" x2="0" y2="217.4875" width="0" layer="20"/>
<wire x1="0" y1="217.4875" x2="174.9425" y2="217.4875" width="0" layer="20"/>
<wire x1="174.9425" y1="217.4875" x2="174.9425" y2="0" width="0" layer="20"/>
<wire x1="174.9425" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>GROZA  12.18  94V-0  MADE IN ROMANIA</text>
<text>OPTION ROM</text>
<text>VER. 1.6  REV. A</text>
<text>16-BIT ATX ISA SYSTEM BACKPLANE</text>
<text>GROZA  12.18  94V-0  MADE IN ROMANIA</text>
<text>BOTTOM</text>
<text>TOP</text>
<hole x="5.08" y="5.08" drill="3.2"/>
<hole x="169.8625" y="5.08" drill="3.2"/>
<text>ASSY. 2486-SBP-001</text>
<text>VER. 1.6  REV. A  ASSY. 2486-SBP-001</text>
<text>-5 V</text>
<text>INTERNAL</text>
<text>ATX PSU</text>
<text>JP1</text>
<text>1-2</text>
<text>2-3</text>
<text>COPYRIGHT (C) 2018 ALEXANDRU GROZA  ALL RIGHTS RESERVED</text>
</plain>
<libraries>
<library name="con-pc">
<description>&lt;b&gt;PC Connectors/Slots&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ISA-16">
<description>&lt;B&gt;ISA SLOT&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5566-20">
<description>&lt;b&gt;Mini FIT connector 20 pol&lt;/b&gt;&lt;p&gt;
ATX PC-Motherboard Power connector&lt;br&gt;
Source: http://www.molex.com</description>
</package>
<package name="22-23-2031">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="memory">
<description>&lt;b&gt;Generic Memories&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-07">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<description>&lt;b&gt;Resistors in Single Inline Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIL9">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO18A">
<description>&lt;b&gt;TO-18&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ISA0" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-molex" package="5566-20" value="ATX POWER">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA1" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA2" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA3" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA4" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA5" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA6" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISA7" library="con-pc" package="ISA-16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C11" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C14" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C15" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C16" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C17" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C18" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C20" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C21" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C22" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C23" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C24" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C25" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C26" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C27" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C28" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C29" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C30" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C31" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C32" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C33" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C34" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C35" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C36" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C37" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C38" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C39" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C40" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C41" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C42" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C43" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C44" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C45" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C46" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C47" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C48" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="IC2" library="memory" package="DIL28" value="27C64">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="74xx-eu" package="DIL20" value="74LS688">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="special" package="EDG-07" value="ROMCFG">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RN1" library="resistor-sil" package="SIL9" value="10K">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="C49" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C51" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="LED1" library="led" package="LED5MM" value="STDBY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED5MM" value="+5V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="LED5MM" value="-5V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="LED5MM" value="+12V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="LED5MM" value="-12V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="LED5MM" value="CPUACT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="R4" library="rcl" package="0204/7" value="1K2">
<attribute name="NAME"/>
</element>
<element name="R5" library="rcl" package="0204/7" value="1K2">
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="IC6" library="linear" package="TO220H" value="UA7905">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="jumper" package="JP2" value="-5V-SEL">
<attribute name="NAME"/>
</element>
<element name="C53" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C54" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C55" library="rcl" package="E5-8,5" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C57" library="rcl" package="E5-8,5" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C56" library="rcl" package="E5-8,5" value="47uF">
<attribute name="NAME"/>
</element>
<element name="C58" library="rcl" package="E5-8,5" value="47uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="jumper" package="JP2" value="PWR/STB-L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="jumper" package="JP1" value="PWR-L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="jumper" package="JP1" value="STB-L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="R8" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="IC5" library="linear" package="DIL08" value="LM555">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="jumper" package="JP1" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C60" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C61" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C62" library="rcl" package="E5-8,5" value="100uF">
<attribute name="NAME"/>
</element>
<element name="R9" library="rcl" package="0204/7" value="220K">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor-small-signal" package="TO18A" value="2N2222">
<attribute name="NAME"/>
</element>
<element name="IC3" library="74xx-eu" package="DIL14" value="74LS04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="74xx-eu" package="DIL14" value="74LS74">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="0204/7" value="33K">
<attribute name="NAME"/>
</element>
<element name="R11" library="rcl" package="0204/7" value="10K">
<attribute name="NAME"/>
</element>
<element name="R12" library="rcl" package="0204/7" value="470R">
<attribute name="NAME"/>
</element>
<element name="R13" library="rcl" package="0204/7" value="10K">
<attribute name="NAME"/>
</element>
<element name="D1" library="diode" package="DO35-10" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D2" library="diode" package="DO35-10" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="C63" library="rcl" package="E2,5-5" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C64" library="rcl" package="E2,5-6" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C65" library="rcl" package="E5-8,5" value="100uF">
<attribute name="NAME"/>
</element>
<element name="J6" library="con-molex" package="22-23-2031" value="5V FAN">
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="con-molex" package="22-23-2031" value="12V FAN">
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C52" library="rcl" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
</element>
<element name="D3" library="diode" package="DO35-10" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D4" library="diode" package="DO35-10" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="R14" library="rcl" package="0204/7" value="1K">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ISA0" pad="B1"/>
<contactref element="ISA0" pad="B10"/>
<contactref element="ISA0" pad="B31"/>
<contactref element="ISA0" pad="D18"/>
<contactref element="ISA1" pad="B1"/>
<contactref element="ISA1" pad="B10"/>
<contactref element="ISA1" pad="B31"/>
<contactref element="ISA1" pad="D18"/>
<contactref element="ISA2" pad="B1"/>
<contactref element="ISA2" pad="B10"/>
<contactref element="ISA2" pad="B31"/>
<contactref element="ISA2" pad="D18"/>
<contactref element="ISA3" pad="B1"/>
<contactref element="ISA3" pad="B10"/>
<contactref element="ISA3" pad="B31"/>
<contactref element="ISA3" pad="D18"/>
<contactref element="ISA4" pad="B1"/>
<contactref element="ISA4" pad="B10"/>
<contactref element="ISA4" pad="B31"/>
<contactref element="ISA4" pad="D18"/>
<contactref element="ISA5" pad="B1"/>
<contactref element="ISA5" pad="B10"/>
<contactref element="ISA5" pad="B31"/>
<contactref element="ISA5" pad="D18"/>
<contactref element="ISA6" pad="B1"/>
<contactref element="ISA6" pad="B10"/>
<contactref element="ISA6" pad="B31"/>
<contactref element="ISA6" pad="D18"/>
<contactref element="ISA7" pad="B1"/>
<contactref element="ISA7" pad="B10"/>
<contactref element="ISA7" pad="B31"/>
<contactref element="ISA7" pad="D18"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="C7" pad="-"/>
<contactref element="C8" pad="-"/>
<contactref element="C9" pad="-"/>
<contactref element="C10" pad="-"/>
<contactref element="C11" pad="-"/>
<contactref element="C12" pad="-"/>
<contactref element="C24" pad="-"/>
<contactref element="C23" pad="-"/>
<contactref element="C22" pad="-"/>
<contactref element="C21" pad="-"/>
<contactref element="C20" pad="-"/>
<contactref element="C19" pad="-"/>
<contactref element="C18" pad="-"/>
<contactref element="C17" pad="-"/>
<contactref element="C16" pad="-"/>
<contactref element="C15" pad="-"/>
<contactref element="C14" pad="-"/>
<contactref element="C13" pad="-"/>
<contactref element="C25" pad="-"/>
<contactref element="C32" pad="-"/>
<contactref element="C31" pad="-"/>
<contactref element="C30" pad="-"/>
<contactref element="C29" pad="-"/>
<contactref element="C28" pad="-"/>
<contactref element="C27" pad="-"/>
<contactref element="C26" pad="-"/>
<contactref element="C33" pad="+"/>
<contactref element="C40" pad="+"/>
<contactref element="C39" pad="+"/>
<contactref element="C38" pad="+"/>
<contactref element="C37" pad="+"/>
<contactref element="C36" pad="+"/>
<contactref element="C35" pad="+"/>
<contactref element="C34" pad="+"/>
<contactref element="C41" pad="+"/>
<contactref element="C48" pad="+"/>
<contactref element="C47" pad="+"/>
<contactref element="C46" pad="+"/>
<contactref element="C45" pad="+"/>
<contactref element="C44" pad="+"/>
<contactref element="C43" pad="+"/>
<contactref element="C42" pad="+"/>
<contactref element="IC1" pad="17"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="6"/>
<contactref element="SW1" pad="7"/>
<contactref element="IC1" pad="18"/>
<contactref element="C49" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="13"/>
<contactref element="J1" pad="15"/>
<contactref element="J1" pad="16"/>
<contactref element="J1" pad="17"/>
<contactref element="C53" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C55" pad="-"/>
<contactref element="C57" pad="+"/>
<contactref element="C56" pad="+"/>
<contactref element="C58" pad="-"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="K"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="C59" pad="2"/>
<contactref element="C60" pad="2"/>
<contactref element="C61" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="C62" pad="-"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC4" pad="7"/>
<contactref element="C63" pad="-"/>
<contactref element="C64" pad="-"/>
<contactref element="C65" pad="-"/>
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="C50" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="VCC">
<contactref element="ISA0" pad="B3"/>
<contactref element="ISA0" pad="B29"/>
<contactref element="ISA0" pad="D16"/>
<contactref element="ISA1" pad="B3"/>
<contactref element="ISA1" pad="B29"/>
<contactref element="ISA1" pad="D16"/>
<contactref element="ISA2" pad="B3"/>
<contactref element="ISA2" pad="B29"/>
<contactref element="ISA2" pad="D16"/>
<contactref element="ISA3" pad="B3"/>
<contactref element="ISA3" pad="B29"/>
<contactref element="ISA3" pad="D16"/>
<contactref element="ISA4" pad="B3"/>
<contactref element="ISA4" pad="B29"/>
<contactref element="ISA4" pad="D16"/>
<contactref element="ISA5" pad="B3"/>
<contactref element="ISA5" pad="B29"/>
<contactref element="ISA5" pad="D16"/>
<contactref element="ISA6" pad="B3"/>
<contactref element="ISA6" pad="B29"/>
<contactref element="ISA6" pad="D16"/>
<contactref element="ISA7" pad="B3"/>
<contactref element="ISA7" pad="B29"/>
<contactref element="ISA7" pad="D16"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="+"/>
<contactref element="C3" pad="+"/>
<contactref element="C4" pad="+"/>
<contactref element="C5" pad="+"/>
<contactref element="C6" pad="+"/>
<contactref element="C7" pad="+"/>
<contactref element="C8" pad="+"/>
<contactref element="C9" pad="+"/>
<contactref element="C10" pad="+"/>
<contactref element="C11" pad="+"/>
<contactref element="C12" pad="+"/>
<contactref element="C24" pad="+"/>
<contactref element="C23" pad="+"/>
<contactref element="C22" pad="+"/>
<contactref element="C21" pad="+"/>
<contactref element="C20" pad="+"/>
<contactref element="C19" pad="+"/>
<contactref element="C18" pad="+"/>
<contactref element="C17" pad="+"/>
<contactref element="C16" pad="+"/>
<contactref element="C15" pad="+"/>
<contactref element="C14" pad="+"/>
<contactref element="C13" pad="+"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="RN1" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="19"/>
<contactref element="J1" pad="20"/>
<contactref element="C58" pad="+"/>
<contactref element="R2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="C50" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="LED6" pad="A"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="D7">
<contactref element="ISA0" pad="A2"/>
<contactref element="ISA1" pad="A2"/>
<contactref element="ISA2" pad="A2"/>
<contactref element="ISA3" pad="A2"/>
<contactref element="ISA4" pad="A2"/>
<contactref element="ISA5" pad="A2"/>
<contactref element="ISA6" pad="A2"/>
<contactref element="ISA7" pad="A2"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="D6">
<contactref element="ISA0" pad="A3"/>
<contactref element="ISA1" pad="A3"/>
<contactref element="ISA2" pad="A3"/>
<contactref element="ISA3" pad="A3"/>
<contactref element="ISA4" pad="A3"/>
<contactref element="ISA5" pad="A3"/>
<contactref element="ISA6" pad="A3"/>
<contactref element="ISA7" pad="A3"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="D4">
<contactref element="ISA0" pad="A5"/>
<contactref element="ISA1" pad="A5"/>
<contactref element="ISA2" pad="A5"/>
<contactref element="ISA3" pad="A5"/>
<contactref element="ISA4" pad="A5"/>
<contactref element="ISA5" pad="A5"/>
<contactref element="ISA6" pad="A5"/>
<contactref element="ISA7" pad="A5"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="D3">
<contactref element="ISA0" pad="A6"/>
<contactref element="ISA1" pad="A6"/>
<contactref element="ISA2" pad="A6"/>
<contactref element="ISA3" pad="A6"/>
<contactref element="ISA4" pad="A6"/>
<contactref element="ISA5" pad="A6"/>
<contactref element="ISA6" pad="A6"/>
<contactref element="ISA7" pad="A6"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="D2">
<contactref element="ISA0" pad="A7"/>
<contactref element="ISA1" pad="A7"/>
<contactref element="ISA2" pad="A7"/>
<contactref element="ISA3" pad="A7"/>
<contactref element="ISA4" pad="A7"/>
<contactref element="ISA5" pad="A7"/>
<contactref element="ISA6" pad="A7"/>
<contactref element="ISA7" pad="A7"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="D1">
<contactref element="ISA0" pad="A8"/>
<contactref element="ISA1" pad="A8"/>
<contactref element="ISA2" pad="A8"/>
<contactref element="ISA3" pad="A8"/>
<contactref element="ISA4" pad="A8"/>
<contactref element="ISA5" pad="A8"/>
<contactref element="ISA6" pad="A8"/>
<contactref element="ISA7" pad="A8"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="D0">
<contactref element="ISA0" pad="A9"/>
<contactref element="ISA1" pad="A9"/>
<contactref element="ISA2" pad="A9"/>
<contactref element="ISA3" pad="A9"/>
<contactref element="ISA4" pad="A9"/>
<contactref element="ISA5" pad="A9"/>
<contactref element="ISA6" pad="A9"/>
<contactref element="ISA7" pad="A9"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="AEN">
<contactref element="ISA0" pad="A11"/>
<contactref element="ISA1" pad="A11"/>
<contactref element="ISA2" pad="A11"/>
<contactref element="ISA3" pad="A11"/>
<contactref element="ISA4" pad="A11"/>
<contactref element="ISA5" pad="A11"/>
<contactref element="ISA6" pad="A11"/>
<contactref element="ISA7" pad="A11"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="A19">
<contactref element="ISA0" pad="A12"/>
<contactref element="ISA1" pad="A12"/>
<contactref element="ISA2" pad="A12"/>
<contactref element="ISA3" pad="A12"/>
<contactref element="ISA4" pad="A12"/>
<contactref element="ISA5" pad="A12"/>
<contactref element="ISA6" pad="A12"/>
<contactref element="ISA7" pad="A12"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="A18">
<contactref element="ISA0" pad="A13"/>
<contactref element="ISA1" pad="A13"/>
<contactref element="ISA2" pad="A13"/>
<contactref element="ISA3" pad="A13"/>
<contactref element="ISA4" pad="A13"/>
<contactref element="ISA5" pad="A13"/>
<contactref element="ISA6" pad="A13"/>
<contactref element="ISA7" pad="A13"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="A17">
<contactref element="ISA0" pad="A14"/>
<contactref element="ISA1" pad="A14"/>
<contactref element="ISA2" pad="A14"/>
<contactref element="ISA3" pad="A14"/>
<contactref element="ISA4" pad="A14"/>
<contactref element="ISA5" pad="A14"/>
<contactref element="ISA6" pad="A14"/>
<contactref element="ISA7" pad="A14"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="A16">
<contactref element="ISA0" pad="A15"/>
<contactref element="ISA1" pad="A15"/>
<contactref element="ISA2" pad="A15"/>
<contactref element="ISA3" pad="A15"/>
<contactref element="ISA4" pad="A15"/>
<contactref element="ISA5" pad="A15"/>
<contactref element="ISA6" pad="A15"/>
<contactref element="ISA7" pad="A15"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="A15">
<contactref element="ISA0" pad="A16"/>
<contactref element="ISA1" pad="A16"/>
<contactref element="ISA2" pad="A16"/>
<contactref element="ISA3" pad="A16"/>
<contactref element="ISA4" pad="A16"/>
<contactref element="ISA5" pad="A16"/>
<contactref element="ISA6" pad="A16"/>
<contactref element="ISA7" pad="A16"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="A14">
<contactref element="ISA0" pad="A17"/>
<contactref element="ISA1" pad="A17"/>
<contactref element="ISA2" pad="A17"/>
<contactref element="ISA3" pad="A17"/>
<contactref element="ISA4" pad="A17"/>
<contactref element="ISA5" pad="A17"/>
<contactref element="ISA6" pad="A17"/>
<contactref element="ISA7" pad="A17"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="A13">
<contactref element="ISA0" pad="A18"/>
<contactref element="ISA1" pad="A18"/>
<contactref element="ISA2" pad="A18"/>
<contactref element="ISA3" pad="A18"/>
<contactref element="ISA4" pad="A18"/>
<contactref element="ISA5" pad="A18"/>
<contactref element="ISA6" pad="A18"/>
<contactref element="ISA7" pad="A18"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="A12">
<contactref element="ISA0" pad="A19"/>
<contactref element="ISA1" pad="A19"/>
<contactref element="ISA2" pad="A19"/>
<contactref element="ISA3" pad="A19"/>
<contactref element="ISA4" pad="A19"/>
<contactref element="ISA5" pad="A19"/>
<contactref element="ISA6" pad="A19"/>
<contactref element="ISA7" pad="A19"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="A11">
<contactref element="ISA0" pad="A20"/>
<contactref element="ISA1" pad="A20"/>
<contactref element="ISA2" pad="A20"/>
<contactref element="ISA3" pad="A20"/>
<contactref element="ISA4" pad="A20"/>
<contactref element="ISA5" pad="A20"/>
<contactref element="ISA6" pad="A20"/>
<contactref element="ISA7" pad="A20"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="A10">
<contactref element="ISA0" pad="A21"/>
<contactref element="ISA1" pad="A21"/>
<contactref element="ISA2" pad="A21"/>
<contactref element="ISA3" pad="A21"/>
<contactref element="ISA4" pad="A21"/>
<contactref element="ISA5" pad="A21"/>
<contactref element="ISA6" pad="A21"/>
<contactref element="ISA7" pad="A21"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="A9">
<contactref element="ISA0" pad="A22"/>
<contactref element="ISA1" pad="A22"/>
<contactref element="ISA2" pad="A22"/>
<contactref element="ISA3" pad="A22"/>
<contactref element="ISA4" pad="A22"/>
<contactref element="ISA5" pad="A22"/>
<contactref element="ISA6" pad="A22"/>
<contactref element="ISA7" pad="A22"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="A8">
<contactref element="ISA0" pad="A23"/>
<contactref element="ISA1" pad="A23"/>
<contactref element="ISA2" pad="A23"/>
<contactref element="ISA3" pad="A23"/>
<contactref element="ISA4" pad="A23"/>
<contactref element="ISA5" pad="A23"/>
<contactref element="ISA6" pad="A23"/>
<contactref element="ISA7" pad="A23"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="A7">
<contactref element="ISA0" pad="A24"/>
<contactref element="ISA1" pad="A24"/>
<contactref element="ISA2" pad="A24"/>
<contactref element="ISA3" pad="A24"/>
<contactref element="ISA4" pad="A24"/>
<contactref element="ISA5" pad="A24"/>
<contactref element="ISA6" pad="A24"/>
<contactref element="ISA7" pad="A24"/>
<contactref element="IC2" pad="3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="A6">
<contactref element="ISA0" pad="A25"/>
<contactref element="ISA1" pad="A25"/>
<contactref element="ISA2" pad="A25"/>
<contactref element="ISA3" pad="A25"/>
<contactref element="ISA4" pad="A25"/>
<contactref element="ISA5" pad="A25"/>
<contactref element="ISA6" pad="A25"/>
<contactref element="ISA7" pad="A25"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="A5">
<contactref element="ISA0" pad="A26"/>
<contactref element="ISA1" pad="A26"/>
<contactref element="ISA2" pad="A26"/>
<contactref element="ISA3" pad="A26"/>
<contactref element="ISA4" pad="A26"/>
<contactref element="ISA5" pad="A26"/>
<contactref element="ISA6" pad="A26"/>
<contactref element="ISA7" pad="A26"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="A4">
<contactref element="ISA0" pad="A27"/>
<contactref element="ISA1" pad="A27"/>
<contactref element="ISA2" pad="A27"/>
<contactref element="ISA3" pad="A27"/>
<contactref element="ISA4" pad="A27"/>
<contactref element="ISA5" pad="A27"/>
<contactref element="ISA6" pad="A27"/>
<contactref element="ISA7" pad="A27"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="A3">
<contactref element="ISA0" pad="A28"/>
<contactref element="ISA1" pad="A28"/>
<contactref element="ISA2" pad="A28"/>
<contactref element="ISA3" pad="A28"/>
<contactref element="ISA4" pad="A28"/>
<contactref element="ISA5" pad="A28"/>
<contactref element="ISA6" pad="A28"/>
<contactref element="ISA7" pad="A28"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="A2">
<contactref element="ISA0" pad="A29"/>
<contactref element="ISA1" pad="A29"/>
<contactref element="ISA2" pad="A29"/>
<contactref element="ISA3" pad="A29"/>
<contactref element="ISA4" pad="A29"/>
<contactref element="ISA5" pad="A29"/>
<contactref element="ISA6" pad="A29"/>
<contactref element="ISA7" pad="A29"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="A1">
<contactref element="ISA0" pad="A30"/>
<contactref element="ISA1" pad="A30"/>
<contactref element="ISA2" pad="A30"/>
<contactref element="ISA3" pad="A30"/>
<contactref element="ISA4" pad="A30"/>
<contactref element="ISA5" pad="A30"/>
<contactref element="ISA6" pad="A30"/>
<contactref element="ISA7" pad="A30"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="A0">
<contactref element="ISA0" pad="A31"/>
<contactref element="ISA1" pad="A31"/>
<contactref element="ISA2" pad="A31"/>
<contactref element="ISA3" pad="A31"/>
<contactref element="ISA4" pad="A31"/>
<contactref element="ISA5" pad="A31"/>
<contactref element="ISA6" pad="A31"/>
<contactref element="ISA7" pad="A31"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="SBHE">
<contactref element="ISA0" pad="C1"/>
<contactref element="ISA1" pad="C1"/>
<contactref element="ISA2" pad="C1"/>
<contactref element="ISA3" pad="C1"/>
<contactref element="ISA4" pad="C1"/>
<contactref element="ISA5" pad="C1"/>
<contactref element="ISA6" pad="C1"/>
<contactref element="ISA7" pad="C1"/>
</signal>
<signal name="LA23">
<contactref element="ISA0" pad="C2"/>
<contactref element="ISA1" pad="C2"/>
<contactref element="ISA2" pad="C2"/>
<contactref element="ISA3" pad="C2"/>
<contactref element="ISA4" pad="C2"/>
<contactref element="ISA5" pad="C2"/>
<contactref element="ISA6" pad="C2"/>
<contactref element="ISA7" pad="C2"/>
</signal>
<signal name="LA22">
<contactref element="ISA0" pad="C3"/>
<contactref element="ISA1" pad="C3"/>
<contactref element="ISA2" pad="C3"/>
<contactref element="ISA3" pad="C3"/>
<contactref element="ISA4" pad="C3"/>
<contactref element="ISA5" pad="C3"/>
<contactref element="ISA6" pad="C3"/>
<contactref element="ISA7" pad="C3"/>
</signal>
<signal name="LA21">
<contactref element="ISA0" pad="C4"/>
<contactref element="ISA1" pad="C4"/>
<contactref element="ISA2" pad="C4"/>
<contactref element="ISA3" pad="C4"/>
<contactref element="ISA4" pad="C4"/>
<contactref element="ISA5" pad="C4"/>
<contactref element="ISA6" pad="C4"/>
<contactref element="ISA7" pad="C4"/>
</signal>
<signal name="LA20">
<contactref element="ISA0" pad="C5"/>
<contactref element="ISA1" pad="C5"/>
<contactref element="ISA2" pad="C5"/>
<contactref element="ISA3" pad="C5"/>
<contactref element="ISA4" pad="C5"/>
<contactref element="ISA5" pad="C5"/>
<contactref element="ISA6" pad="C5"/>
<contactref element="ISA7" pad="C5"/>
</signal>
<signal name="LA19">
<contactref element="ISA0" pad="C6"/>
<contactref element="ISA1" pad="C6"/>
<contactref element="ISA2" pad="C6"/>
<contactref element="ISA3" pad="C6"/>
<contactref element="ISA4" pad="C6"/>
<contactref element="ISA5" pad="C6"/>
<contactref element="ISA6" pad="C6"/>
<contactref element="ISA7" pad="C6"/>
</signal>
<signal name="LA18">
<contactref element="ISA0" pad="C7"/>
<contactref element="ISA1" pad="C7"/>
<contactref element="ISA2" pad="C7"/>
<contactref element="ISA3" pad="C7"/>
<contactref element="ISA4" pad="C7"/>
<contactref element="ISA5" pad="C7"/>
<contactref element="ISA6" pad="C7"/>
<contactref element="ISA7" pad="C7"/>
</signal>
<signal name="LA17">
<contactref element="ISA0" pad="C8"/>
<contactref element="ISA1" pad="C8"/>
<contactref element="ISA2" pad="C8"/>
<contactref element="ISA3" pad="C8"/>
<contactref element="ISA4" pad="C8"/>
<contactref element="ISA5" pad="C8"/>
<contactref element="ISA6" pad="C8"/>
<contactref element="ISA7" pad="C8"/>
</signal>
<signal name="!MEM_R">
<contactref element="ISA0" pad="C9"/>
<contactref element="ISA1" pad="C9"/>
<contactref element="ISA2" pad="C9"/>
<contactref element="ISA3" pad="C9"/>
<contactref element="ISA4" pad="C9"/>
<contactref element="ISA5" pad="C9"/>
<contactref element="ISA6" pad="C9"/>
<contactref element="ISA7" pad="C9"/>
</signal>
<signal name="!MEM_W">
<contactref element="ISA0" pad="C10"/>
<contactref element="ISA1" pad="C10"/>
<contactref element="ISA2" pad="C10"/>
<contactref element="ISA3" pad="C10"/>
<contactref element="ISA4" pad="C10"/>
<contactref element="ISA5" pad="C10"/>
<contactref element="ISA6" pad="C10"/>
<contactref element="ISA7" pad="C10"/>
</signal>
<signal name="D8">
<contactref element="ISA0" pad="C11"/>
<contactref element="ISA1" pad="C11"/>
<contactref element="ISA2" pad="C11"/>
<contactref element="ISA3" pad="C11"/>
<contactref element="ISA4" pad="C11"/>
<contactref element="ISA5" pad="C11"/>
<contactref element="ISA6" pad="C11"/>
<contactref element="ISA7" pad="C11"/>
</signal>
<signal name="D9">
<contactref element="ISA0" pad="C12"/>
<contactref element="ISA1" pad="C12"/>
<contactref element="ISA2" pad="C12"/>
<contactref element="ISA3" pad="C12"/>
<contactref element="ISA4" pad="C12"/>
<contactref element="ISA5" pad="C12"/>
<contactref element="ISA6" pad="C12"/>
<contactref element="ISA7" pad="C12"/>
</signal>
<signal name="D10">
<contactref element="ISA0" pad="C13"/>
<contactref element="ISA1" pad="C13"/>
<contactref element="ISA2" pad="C13"/>
<contactref element="ISA3" pad="C13"/>
<contactref element="ISA4" pad="C13"/>
<contactref element="ISA5" pad="C13"/>
<contactref element="ISA6" pad="C13"/>
<contactref element="ISA7" pad="C13"/>
</signal>
<signal name="D11">
<contactref element="ISA0" pad="C14"/>
<contactref element="ISA1" pad="C14"/>
<contactref element="ISA2" pad="C14"/>
<contactref element="ISA3" pad="C14"/>
<contactref element="ISA4" pad="C14"/>
<contactref element="ISA5" pad="C14"/>
<contactref element="ISA6" pad="C14"/>
<contactref element="ISA7" pad="C14"/>
</signal>
<signal name="D12">
<contactref element="ISA0" pad="C15"/>
<contactref element="ISA1" pad="C15"/>
<contactref element="ISA2" pad="C15"/>
<contactref element="ISA3" pad="C15"/>
<contactref element="ISA4" pad="C15"/>
<contactref element="ISA5" pad="C15"/>
<contactref element="ISA6" pad="C15"/>
<contactref element="ISA7" pad="C15"/>
</signal>
<signal name="D13">
<contactref element="ISA0" pad="C16"/>
<contactref element="ISA1" pad="C16"/>
<contactref element="ISA2" pad="C16"/>
<contactref element="ISA3" pad="C16"/>
<contactref element="ISA4" pad="C16"/>
<contactref element="ISA5" pad="C16"/>
<contactref element="ISA6" pad="C16"/>
<contactref element="ISA7" pad="C16"/>
</signal>
<signal name="D14">
<contactref element="ISA0" pad="C17"/>
<contactref element="ISA1" pad="C17"/>
<contactref element="ISA2" pad="C17"/>
<contactref element="ISA3" pad="C17"/>
<contactref element="ISA4" pad="C17"/>
<contactref element="ISA5" pad="C17"/>
<contactref element="ISA6" pad="C17"/>
<contactref element="ISA7" pad="C17"/>
</signal>
<signal name="D15">
<contactref element="ISA0" pad="C18"/>
<contactref element="ISA1" pad="C18"/>
<contactref element="ISA2" pad="C18"/>
<contactref element="ISA3" pad="C18"/>
<contactref element="ISA4" pad="C18"/>
<contactref element="ISA5" pad="C18"/>
<contactref element="ISA6" pad="C18"/>
<contactref element="ISA7" pad="C18"/>
</signal>
<signal name="RESET">
<contactref element="ISA0" pad="B2"/>
<contactref element="ISA1" pad="B2"/>
<contactref element="ISA2" pad="B2"/>
<contactref element="ISA3" pad="B2"/>
<contactref element="ISA4" pad="B2"/>
<contactref element="ISA5" pad="B2"/>
<contactref element="ISA6" pad="B2"/>
<contactref element="ISA7" pad="B2"/>
</signal>
<signal name="IRQ9">
<contactref element="ISA0" pad="B4"/>
<contactref element="ISA1" pad="B4"/>
<contactref element="ISA2" pad="B4"/>
<contactref element="ISA3" pad="B4"/>
<contactref element="ISA4" pad="B4"/>
<contactref element="ISA5" pad="B4"/>
<contactref element="ISA6" pad="B4"/>
<contactref element="ISA7" pad="B4"/>
</signal>
<signal name="-5V">
<contactref element="ISA0" pad="B5"/>
<contactref element="ISA1" pad="B5"/>
<contactref element="ISA2" pad="B5"/>
<contactref element="ISA3" pad="B5"/>
<contactref element="ISA4" pad="B5"/>
<contactref element="ISA5" pad="B5"/>
<contactref element="ISA6" pad="B5"/>
<contactref element="ISA7" pad="B5"/>
<contactref element="C41" pad="-"/>
<contactref element="C48" pad="-"/>
<contactref element="C47" pad="-"/>
<contactref element="C46" pad="-"/>
<contactref element="C45" pad="-"/>
<contactref element="C44" pad="-"/>
<contactref element="C43" pad="-"/>
<contactref element="C42" pad="-"/>
<contactref element="C57" pad="-"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="DRQ2">
<contactref element="ISA0" pad="B6"/>
<contactref element="ISA1" pad="B6"/>
<contactref element="ISA2" pad="B6"/>
<contactref element="ISA3" pad="B6"/>
<contactref element="ISA4" pad="B6"/>
<contactref element="ISA5" pad="B6"/>
<contactref element="ISA6" pad="B6"/>
<contactref element="ISA7" pad="B6"/>
</signal>
<signal name="-12V">
<contactref element="ISA0" pad="B7"/>
<contactref element="ISA1" pad="B7"/>
<contactref element="ISA2" pad="B7"/>
<contactref element="ISA3" pad="B7"/>
<contactref element="ISA4" pad="B7"/>
<contactref element="ISA5" pad="B7"/>
<contactref element="ISA6" pad="B7"/>
<contactref element="ISA7" pad="B7"/>
<contactref element="C33" pad="-"/>
<contactref element="C40" pad="-"/>
<contactref element="C39" pad="-"/>
<contactref element="C38" pad="-"/>
<contactref element="C37" pad="-"/>
<contactref element="C36" pad="-"/>
<contactref element="C35" pad="-"/>
<contactref element="C34" pad="-"/>
<contactref element="IC6" pad="2"/>
<contactref element="J1" pad="12"/>
<contactref element="C53" pad="1"/>
<contactref element="C56" pad="-"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="!0WS">
<contactref element="ISA0" pad="B8"/>
<contactref element="ISA1" pad="B8"/>
<contactref element="ISA2" pad="B8"/>
<contactref element="ISA3" pad="B8"/>
<contactref element="ISA4" pad="B8"/>
<contactref element="ISA5" pad="B8"/>
<contactref element="ISA6" pad="B8"/>
<contactref element="ISA7" pad="B8"/>
</signal>
<signal name="+12V">
<contactref element="ISA0" pad="B9"/>
<contactref element="ISA1" pad="B9"/>
<contactref element="ISA2" pad="B9"/>
<contactref element="ISA3" pad="B9"/>
<contactref element="ISA4" pad="B9"/>
<contactref element="ISA5" pad="B9"/>
<contactref element="ISA6" pad="B9"/>
<contactref element="ISA7" pad="B9"/>
<contactref element="C25" pad="+"/>
<contactref element="C32" pad="+"/>
<contactref element="C31" pad="+"/>
<contactref element="C30" pad="+"/>
<contactref element="C29" pad="+"/>
<contactref element="C28" pad="+"/>
<contactref element="C27" pad="+"/>
<contactref element="C26" pad="+"/>
<contactref element="J1" pad="10"/>
<contactref element="C55" pad="+"/>
<contactref element="R4" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="!MEMW">
<contactref element="ISA0" pad="B11"/>
<contactref element="ISA1" pad="B11"/>
<contactref element="ISA2" pad="B11"/>
<contactref element="ISA3" pad="B11"/>
<contactref element="ISA4" pad="B11"/>
<contactref element="ISA5" pad="B11"/>
<contactref element="ISA6" pad="B11"/>
<contactref element="ISA7" pad="B11"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="!MEMR">
<contactref element="ISA0" pad="B12"/>
<contactref element="ISA1" pad="B12"/>
<contactref element="ISA2" pad="B12"/>
<contactref element="ISA3" pad="B12"/>
<contactref element="ISA4" pad="B12"/>
<contactref element="ISA5" pad="B12"/>
<contactref element="ISA6" pad="B12"/>
<contactref element="ISA7" pad="B12"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="!IOW">
<contactref element="ISA0" pad="B13"/>
<contactref element="ISA1" pad="B13"/>
<contactref element="ISA2" pad="B13"/>
<contactref element="ISA3" pad="B13"/>
<contactref element="ISA4" pad="B13"/>
<contactref element="ISA5" pad="B13"/>
<contactref element="ISA6" pad="B13"/>
<contactref element="ISA7" pad="B13"/>
</signal>
<signal name="!IOR">
<contactref element="ISA0" pad="B14"/>
<contactref element="ISA1" pad="B14"/>
<contactref element="ISA2" pad="B14"/>
<contactref element="ISA3" pad="B14"/>
<contactref element="ISA4" pad="B14"/>
<contactref element="ISA5" pad="B14"/>
<contactref element="ISA6" pad="B14"/>
<contactref element="ISA7" pad="B14"/>
</signal>
<signal name="!DACK3">
<contactref element="ISA0" pad="B15"/>
<contactref element="ISA1" pad="B15"/>
<contactref element="ISA2" pad="B15"/>
<contactref element="ISA3" pad="B15"/>
<contactref element="ISA4" pad="B15"/>
<contactref element="ISA5" pad="B15"/>
<contactref element="ISA6" pad="B15"/>
<contactref element="ISA7" pad="B15"/>
</signal>
<signal name="DRQ3">
<contactref element="ISA0" pad="B16"/>
<contactref element="ISA1" pad="B16"/>
<contactref element="ISA2" pad="B16"/>
<contactref element="ISA3" pad="B16"/>
<contactref element="ISA4" pad="B16"/>
<contactref element="ISA5" pad="B16"/>
<contactref element="ISA6" pad="B16"/>
<contactref element="ISA7" pad="B16"/>
</signal>
<signal name="!DACK1">
<contactref element="ISA0" pad="B17"/>
<contactref element="ISA1" pad="B17"/>
<contactref element="ISA2" pad="B17"/>
<contactref element="ISA3" pad="B17"/>
<contactref element="ISA4" pad="B17"/>
<contactref element="ISA5" pad="B17"/>
<contactref element="ISA6" pad="B17"/>
<contactref element="ISA7" pad="B17"/>
</signal>
<signal name="DRQ1">
<contactref element="ISA0" pad="B18"/>
<contactref element="ISA1" pad="B18"/>
<contactref element="ISA2" pad="B18"/>
<contactref element="ISA3" pad="B18"/>
<contactref element="ISA4" pad="B18"/>
<contactref element="ISA5" pad="B18"/>
<contactref element="ISA6" pad="B18"/>
<contactref element="ISA7" pad="B18"/>
</signal>
<signal name="!REFRESH">
<contactref element="ISA0" pad="B19"/>
<contactref element="ISA1" pad="B19"/>
<contactref element="ISA2" pad="B19"/>
<contactref element="ISA3" pad="B19"/>
<contactref element="ISA4" pad="B19"/>
<contactref element="ISA5" pad="B19"/>
<contactref element="ISA6" pad="B19"/>
<contactref element="ISA7" pad="B19"/>
</signal>
<signal name="CLK">
<contactref element="ISA0" pad="B20"/>
<contactref element="ISA1" pad="B20"/>
<contactref element="ISA2" pad="B20"/>
<contactref element="ISA3" pad="B20"/>
<contactref element="ISA4" pad="B20"/>
<contactref element="ISA5" pad="B20"/>
<contactref element="ISA6" pad="B20"/>
<contactref element="ISA7" pad="B20"/>
</signal>
<signal name="IRQ7">
<contactref element="ISA0" pad="B21"/>
<contactref element="ISA1" pad="B21"/>
<contactref element="ISA2" pad="B21"/>
<contactref element="ISA3" pad="B21"/>
<contactref element="ISA4" pad="B21"/>
<contactref element="ISA5" pad="B21"/>
<contactref element="ISA6" pad="B21"/>
<contactref element="ISA7" pad="B21"/>
</signal>
<signal name="IRQ6">
<contactref element="ISA0" pad="B22"/>
<contactref element="ISA1" pad="B22"/>
<contactref element="ISA2" pad="B22"/>
<contactref element="ISA3" pad="B22"/>
<contactref element="ISA4" pad="B22"/>
<contactref element="ISA5" pad="B22"/>
<contactref element="ISA6" pad="B22"/>
<contactref element="ISA7" pad="B22"/>
</signal>
<signal name="IRQ5">
<contactref element="ISA0" pad="B23"/>
<contactref element="ISA1" pad="B23"/>
<contactref element="ISA2" pad="B23"/>
<contactref element="ISA3" pad="B23"/>
<contactref element="ISA4" pad="B23"/>
<contactref element="ISA5" pad="B23"/>
<contactref element="ISA6" pad="B23"/>
<contactref element="ISA7" pad="B23"/>
</signal>
<signal name="IRQ4">
<contactref element="ISA0" pad="B24"/>
<contactref element="ISA1" pad="B24"/>
<contactref element="ISA2" pad="B24"/>
<contactref element="ISA3" pad="B24"/>
<contactref element="ISA4" pad="B24"/>
<contactref element="ISA5" pad="B24"/>
<contactref element="ISA6" pad="B24"/>
<contactref element="ISA7" pad="B24"/>
</signal>
<signal name="IRQ3">
<contactref element="ISA0" pad="B25"/>
<contactref element="ISA1" pad="B25"/>
<contactref element="ISA2" pad="B25"/>
<contactref element="ISA3" pad="B25"/>
<contactref element="ISA4" pad="B25"/>
<contactref element="ISA5" pad="B25"/>
<contactref element="ISA6" pad="B25"/>
<contactref element="ISA7" pad="B25"/>
</signal>
<signal name="!DACK2">
<contactref element="ISA0" pad="B26"/>
<contactref element="ISA1" pad="B26"/>
<contactref element="ISA2" pad="B26"/>
<contactref element="ISA3" pad="B26"/>
<contactref element="ISA4" pad="B26"/>
<contactref element="ISA5" pad="B26"/>
<contactref element="ISA6" pad="B26"/>
<contactref element="ISA7" pad="B26"/>
</signal>
<signal name="T/C">
<contactref element="ISA0" pad="B27"/>
<contactref element="ISA1" pad="B27"/>
<contactref element="ISA2" pad="B27"/>
<contactref element="ISA3" pad="B27"/>
<contactref element="ISA4" pad="B27"/>
<contactref element="ISA5" pad="B27"/>
<contactref element="ISA6" pad="B27"/>
<contactref element="ISA7" pad="B27"/>
</signal>
<signal name="ALE">
<contactref element="ISA0" pad="B28"/>
<contactref element="ISA1" pad="B28"/>
<contactref element="ISA2" pad="B28"/>
<contactref element="ISA3" pad="B28"/>
<contactref element="ISA4" pad="B28"/>
<contactref element="ISA5" pad="B28"/>
<contactref element="ISA6" pad="B28"/>
<contactref element="ISA7" pad="B28"/>
</signal>
<signal name="OSC">
<contactref element="ISA0" pad="B30"/>
<contactref element="ISA1" pad="B30"/>
<contactref element="ISA2" pad="B30"/>
<contactref element="ISA3" pad="B30"/>
<contactref element="ISA4" pad="B30"/>
<contactref element="ISA5" pad="B30"/>
<contactref element="ISA6" pad="B30"/>
<contactref element="ISA7" pad="B30"/>
</signal>
<signal name="!MEMCS16">
<contactref element="ISA0" pad="D1"/>
<contactref element="ISA1" pad="D1"/>
<contactref element="ISA2" pad="D1"/>
<contactref element="ISA3" pad="D1"/>
<contactref element="ISA4" pad="D1"/>
<contactref element="ISA5" pad="D1"/>
<contactref element="ISA6" pad="D1"/>
<contactref element="ISA7" pad="D1"/>
</signal>
<signal name="!I/OCS16">
<contactref element="ISA0" pad="D2"/>
<contactref element="ISA1" pad="D2"/>
<contactref element="ISA2" pad="D2"/>
<contactref element="ISA3" pad="D2"/>
<contactref element="ISA4" pad="D2"/>
<contactref element="ISA5" pad="D2"/>
<contactref element="ISA6" pad="D2"/>
<contactref element="ISA7" pad="D2"/>
</signal>
<signal name="IRQ10">
<contactref element="ISA0" pad="D3"/>
<contactref element="ISA1" pad="D3"/>
<contactref element="ISA2" pad="D3"/>
<contactref element="ISA3" pad="D3"/>
<contactref element="ISA4" pad="D3"/>
<contactref element="ISA5" pad="D3"/>
<contactref element="ISA6" pad="D3"/>
<contactref element="ISA7" pad="D3"/>
</signal>
<signal name="IRQ11">
<contactref element="ISA0" pad="D4"/>
<contactref element="ISA1" pad="D4"/>
<contactref element="ISA2" pad="D4"/>
<contactref element="ISA3" pad="D4"/>
<contactref element="ISA4" pad="D4"/>
<contactref element="ISA5" pad="D4"/>
<contactref element="ISA6" pad="D4"/>
<contactref element="ISA7" pad="D4"/>
</signal>
<signal name="IRQ12">
<contactref element="ISA0" pad="D5"/>
<contactref element="ISA1" pad="D5"/>
<contactref element="ISA2" pad="D5"/>
<contactref element="ISA3" pad="D5"/>
<contactref element="ISA4" pad="D5"/>
<contactref element="ISA5" pad="D5"/>
<contactref element="ISA6" pad="D5"/>
<contactref element="ISA7" pad="D5"/>
</signal>
<signal name="IRQ15">
<contactref element="ISA0" pad="D6"/>
<contactref element="ISA1" pad="D6"/>
<contactref element="ISA2" pad="D6"/>
<contactref element="ISA3" pad="D6"/>
<contactref element="ISA4" pad="D6"/>
<contactref element="ISA5" pad="D6"/>
<contactref element="ISA6" pad="D6"/>
<contactref element="ISA7" pad="D6"/>
</signal>
<signal name="IRQ14">
<contactref element="ISA0" pad="D7"/>
<contactref element="ISA1" pad="D7"/>
<contactref element="ISA2" pad="D7"/>
<contactref element="ISA3" pad="D7"/>
<contactref element="ISA4" pad="D7"/>
<contactref element="ISA5" pad="D7"/>
<contactref element="ISA6" pad="D7"/>
<contactref element="ISA7" pad="D7"/>
</signal>
<signal name="!DACK0">
<contactref element="ISA0" pad="D8"/>
<contactref element="ISA1" pad="D8"/>
<contactref element="ISA2" pad="D8"/>
<contactref element="ISA3" pad="D8"/>
<contactref element="ISA4" pad="D8"/>
<contactref element="ISA5" pad="D8"/>
<contactref element="ISA6" pad="D8"/>
<contactref element="ISA7" pad="D8"/>
</signal>
<signal name="DRQ0">
<contactref element="ISA0" pad="D9"/>
<contactref element="ISA1" pad="D9"/>
<contactref element="ISA2" pad="D9"/>
<contactref element="ISA3" pad="D9"/>
<contactref element="ISA4" pad="D9"/>
<contactref element="ISA5" pad="D9"/>
<contactref element="ISA6" pad="D9"/>
<contactref element="ISA7" pad="D9"/>
</signal>
<signal name="!DACK5">
<contactref element="ISA0" pad="D10"/>
<contactref element="ISA1" pad="D10"/>
<contactref element="ISA2" pad="D10"/>
<contactref element="ISA3" pad="D10"/>
<contactref element="ISA4" pad="D10"/>
<contactref element="ISA5" pad="D10"/>
<contactref element="ISA6" pad="D10"/>
<contactref element="ISA7" pad="D10"/>
</signal>
<signal name="DRQ5">
<contactref element="ISA0" pad="D11"/>
<contactref element="ISA1" pad="D11"/>
<contactref element="ISA2" pad="D11"/>
<contactref element="ISA3" pad="D11"/>
<contactref element="ISA4" pad="D11"/>
<contactref element="ISA5" pad="D11"/>
<contactref element="ISA6" pad="D11"/>
<contactref element="ISA7" pad="D11"/>
</signal>
<signal name="!DACK6">
<contactref element="ISA0" pad="D12"/>
<contactref element="ISA1" pad="D12"/>
<contactref element="ISA2" pad="D12"/>
<contactref element="ISA3" pad="D12"/>
<contactref element="ISA4" pad="D12"/>
<contactref element="ISA5" pad="D12"/>
<contactref element="ISA6" pad="D12"/>
<contactref element="ISA7" pad="D12"/>
</signal>
<signal name="DRQ6">
<contactref element="ISA0" pad="D13"/>
<contactref element="ISA1" pad="D13"/>
<contactref element="ISA2" pad="D13"/>
<contactref element="ISA3" pad="D13"/>
<contactref element="ISA4" pad="D13"/>
<contactref element="ISA5" pad="D13"/>
<contactref element="ISA6" pad="D13"/>
<contactref element="ISA7" pad="D13"/>
</signal>
<signal name="!DACK7">
<contactref element="ISA0" pad="D14"/>
<contactref element="ISA1" pad="D14"/>
<contactref element="ISA2" pad="D14"/>
<contactref element="ISA3" pad="D14"/>
<contactref element="ISA4" pad="D14"/>
<contactref element="ISA5" pad="D14"/>
<contactref element="ISA6" pad="D14"/>
<contactref element="ISA7" pad="D14"/>
</signal>
<signal name="DRQ7">
<contactref element="ISA0" pad="D15"/>
<contactref element="ISA1" pad="D15"/>
<contactref element="ISA2" pad="D15"/>
<contactref element="ISA3" pad="D15"/>
<contactref element="ISA4" pad="D15"/>
<contactref element="ISA5" pad="D15"/>
<contactref element="ISA6" pad="D15"/>
<contactref element="ISA7" pad="D15"/>
</signal>
<signal name="!MASTER">
<contactref element="ISA0" pad="D17"/>
<contactref element="ISA1" pad="D17"/>
<contactref element="ISA2" pad="D17"/>
<contactref element="ISA3" pad="D17"/>
<contactref element="ISA4" pad="D17"/>
<contactref element="ISA5" pad="D17"/>
<contactref element="ISA6" pad="D17"/>
<contactref element="ISA7" pad="D17"/>
</signal>
<signal name="!I/OCHK">
<contactref element="ISA0" pad="A1"/>
<contactref element="ISA1" pad="A1"/>
<contactref element="ISA2" pad="A1"/>
<contactref element="ISA3" pad="A1"/>
<contactref element="ISA4" pad="A1"/>
<contactref element="ISA5" pad="A1"/>
<contactref element="ISA6" pad="A1"/>
<contactref element="ISA7" pad="A1"/>
</signal>
<signal name="D5">
<contactref element="ISA0" pad="A4"/>
<contactref element="ISA1" pad="A4"/>
<contactref element="ISA2" pad="A4"/>
<contactref element="ISA3" pad="A4"/>
<contactref element="ISA4" pad="A4"/>
<contactref element="ISA5" pad="A4"/>
<contactref element="ISA6" pad="A4"/>
<contactref element="ISA7" pad="A4"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="I/ORDY">
<contactref element="ISA0" pad="A10"/>
<contactref element="ISA1" pad="A10"/>
<contactref element="ISA2" pad="A10"/>
<contactref element="ISA3" pad="A10"/>
<contactref element="ISA4" pad="A10"/>
<contactref element="ISA5" pad="A10"/>
<contactref element="ISA6" pad="A10"/>
<contactref element="ISA7" pad="A10"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="1"/>
<contactref element="SW1" pad="14"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="7"/>
<contactref element="SW1" pad="12"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="SW1" pad="11"/>
<contactref element="IC1" pad="9"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="12"/>
<contactref element="SW1" pad="10"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="SW1" pad="9"/>
<contactref element="IC1" pad="14"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="16"/>
<contactref element="SW1" pad="8"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="!ROMW">
<contactref element="IC2" pad="27"/>
<contactref element="SW1" pad="13"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="!ROMCS">
<contactref element="IC1" pad="19"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="LED4" pad="A"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC6" pad="3"/>
<contactref element="C54" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="-5V-PS">
<contactref element="J1" pad="18"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="+5VSB">
<contactref element="J1" pad="9"/>
<contactref element="C59" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="C61" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="T1" pad="C"/>
<contactref element="IC3" pad="14"/>
<contactref element="IC4" pad="14"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="R11" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="R13" pad="2"/>
<contactref element="IC4" pad="13"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="!PS_ON">
<contactref element="J1" pad="14"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="N$17">
<contactref element="R5" pad="2"/>
<contactref element="LED5" pad="K"/>
</signal>
<signal name="N$15">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="K"/>
</signal>
<signal name="N$40">
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="CPUACT">
<contactref element="R6" pad="1"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="N$19">
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="J2" pad="3"/>
<contactref element="J4" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="PWRSW">
<contactref element="J5" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="IC5" pad="2"/>
<contactref element="IC5" pad="6"/>
<contactref element="R9" pad="2"/>
<contactref element="C62" pad="+"/>
<contactref element="T1" pad="B"/>
<contactref element="C65" pad="+"/>
</signal>
<signal name="N$23">
<contactref element="IC5" pad="3"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="IC5" pad="4"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="STDBY">
<contactref element="R1" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="T1" pad="E"/>
</signal>
<signal name="N$33">
<contactref element="IC4" pad="3"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="R12" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="C63" pad="+"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R13" pad="1"/>
<contactref element="C64" pad="+"/>
<contactref element="D2" pad="A"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$36">
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$37">
<contactref element="IC3" pad="6"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="N$38">
<contactref element="IC4" pad="8"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="N$39">
<contactref element="IC4" pad="11"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="1-RPM">
<contactref element="J6" pad="3"/>
</signal>
<signal name="2-RPM">
<contactref element="J7" pad="3"/>
</signal>
<signal name="RDY/!B">
<contactref element="IC2" pad="1"/>
<contactref element="RN1" pad="9"/>
</signal>
<signal name="BTM-RAD">
</signal>
<signal name="TP-RAD">
</signal>
<signal name="N$7">
<contactref element="D4" pad="C"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="D3" pad="C"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="N$9">
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="R14" pad="1"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="2"/>
<contactref element="LED6" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
