<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<text>8MD to DVI-I</text>
<text>by RGB, 2019</text>
<wire x1="0" y1="24.5" x2="1" y2="25.5" width="0" layer="20" curve="-90"/>
<wire x1="1" y1="25.5" x2="36" y2="25.5" width="0" layer="20"/>
<wire x1="36" y1="25.5" x2="37" y2="24.5" width="0" layer="20" curve="-90"/>
<wire x1="37" y1="24.5" x2="37" y2="1" width="0" layer="20"/>
<wire x1="37" y1="1" x2="36" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="36" y1="0" x2="1" y2="0" width="0" layer="20"/>
<wire x1="1" y1="0" x2="0" y2="1" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1" x2="0" y2="24.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="rgb_lib">
<packages>
<package name="HAS_LOGO_TINY">
</package>
<package name="JC-128">
</package>
</packages>
</library>
<library name="mini_din">
<packages>
<package name="M_DIN8">
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CCDVI-29DVISIR-A-2">
<description>&lt;b&gt;FEMALE DVI CONNECTOR INTEGRATED 29 - RIGHT ANGLE&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/CCDVI-29DVISIR-A-2.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="mini_din" package="M_DIN8" value="">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="rgb_lib" package="HAS_LOGO_TINY" value=""/>
<element name="U$1" library="rgb_lib" package="JC-128" value="JC-128"/>
<element name="X2" library="con-cypressindustries" package="CCDVI-29DVISIR-A-2" value="DVI29">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="SH3"/>
<contactref element="X1" pad="SH1"/>
<contactref element="X1" pad="SH2"/>
<contactref element="U$1" pad="1"/>
<contactref element="X2" pad="C5.1"/>
<contactref element="X2" pad="C5.2"/>
</signal>
<signal name="CS">
<contactref element="X1" pad="3"/>
<contactref element="X2" pad="C4"/>
</signal>
<signal name="B">
<contactref element="X1" pad="6"/>
<contactref element="X2" pad="C3"/>
</signal>
<signal name="G">
<contactref element="X1" pad="7"/>
<contactref element="X2" pad="C2"/>
</signal>
<signal name="R">
<contactref element="X1" pad="8"/>
<contactref element="X2" pad="C1"/>
</signal>
<signal name="AUDIO_L">
<contactref element="X1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="AUDIO_R">
<contactref element="X1" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
