<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="1.79605" y1="0" x2="31.2180375" y2="0" width="0" layer="20"/>
<wire x1="31.2180375" y1="0" x2="33" y2="1.7819625" width="0" layer="20" curve="90"/>
<wire x1="33" y1="1.7819625" x2="33" y2="16.07425" width="0" layer="20"/>
<wire x1="33" y1="16.07425" x2="30.98925" y2="18.085" width="0" layer="20" curve="90"/>
<wire x1="30.98925" y1="18.085" x2="2.02324375" y2="18.085" width="0" layer="20"/>
<wire x1="2.02324375" y1="18.085" x2="0" y2="16.06175625" width="0" layer="20" curve="90"/>
<wire x1="0" y1="16.06175625" x2="0" y2="1.79605" width="0" layer="20"/>
<wire x1="0" y1="1.79605" x2="1.79605" y2="0" width="0" layer="20" curve="90"/>
<text>KL27</text>
<text>nRF51</text>
<text>VCC</text>
<text>GND</text>
<text>CLK</text>
<text>IO</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-SHROUDED">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-DPDT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="SWITCH-DPDT" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="JP2" pad="3"/>
<contactref element="S3" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="4"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="BLE_SWDCLK">
<contactref element="JP1" pad="4"/>
<contactref element="S3" pad="6"/>
</signal>
<signal name="KL_SWDIO">
<contactref element="JP1" pad="6"/>
<contactref element="S3" pad="1"/>
</signal>
<signal name="BLE_SWDIO">
<contactref element="JP1" pad="1"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="KL_SWDCLK">
<contactref element="JP1" pad="5"/>
<contactref element="S3" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
