<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="47" width="0.4064" layer="20"/>
<wire x1="40" y1="0" x2="40" y2="42" width="0.4064" layer="20"/>
<wire x1="40" y1="42" x2="34" y2="47" width="0.4064" layer="20"/>
<wire x1="34" y1="47" x2="0" y2="47" width="0.4064" layer="20"/>
<wire x1="0" y1="0" x2="6" y2="0" width="0.4064" layer="20"/>
<wire x1="6" y1="0" x2="6" y2="4" width="0.4064" layer="20"/>
<wire x1="6" y1="4" x2="9" y2="4" width="0.4064" layer="20"/>
<wire x1="9" y1="4" x2="9" y2="0" width="0.4064" layer="20"/>
<wire x1="9" y1="0" x2="11" y2="0" width="0.4064" layer="20"/>
<wire x1="11" y1="0" x2="11" y2="7" width="0.4064" layer="20"/>
<wire x1="11" y1="7" x2="18" y2="7" width="0.4064" layer="20"/>
<wire x1="18" y1="7" x2="18" y2="0" width="0.4064" layer="20"/>
<wire x1="18" y1="0" x2="40" y2="0" width="0.4064" layer="20"/>
<text>1</text>
</plain>
<libraries>
<library name="FPC_Connectors_Flat_Flexible_Cable_rev15c">
<description>&lt;BR&gt;Wurth Elektronik   FPC Connector and FFC Cable&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015b, 08.04.2015&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="686130148922">
<description>WR-FPC 1mm SMT Horiz. Bot. Contact Hinge type WR-FPC 1mm 30pins Hinge type SMT Horizontal Bottom Contact</description>
</package>
</packages>
</library>
<library name="teensy">
<packages>
<package name="TEENSY">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="FPC_Connectors_Flat_Flexible_Cable_rev15c" package="686130148922" value="686130148922"/>
<element name="_1" library="teensy" package="TEENSY" value="TEENSY"/>
<element name="U$1" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$2" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$3" library="holes" package="3,0" value=""/>
</elements>
<signals>
<signal name="N$12">
<contactref element="J1" pad="19"/>
<contactref element="_1" pad="B0"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="29"/>
<contactref element="_1" pad="C7"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="28"/>
<contactref element="_1" pad="C6"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="27"/>
<contactref element="_1" pad="D3"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="26"/>
<contactref element="_1" pad="D2"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="25"/>
<contactref element="_1" pad="D1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="24"/>
<contactref element="_1" pad="D0"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="23"/>
<contactref element="_1" pad="B7"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="22"/>
<contactref element="_1" pad="B3"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="21"/>
<contactref element="_1" pad="B2"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="20"/>
<contactref element="_1" pad="B1"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="18"/>
<contactref element="_1" pad="E6"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="17"/>
<contactref element="_1" pad="D5"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="16"/>
<contactref element="_1" pad="D4"/>
</signal>
<signal name="N$16">
<contactref element="J1" pad="14"/>
<contactref element="_1" pad="D6"/>
</signal>
<signal name="N$17">
<contactref element="J1" pad="13"/>
<contactref element="_1" pad="D7"/>
</signal>
<signal name="N$18">
<contactref element="J1" pad="12"/>
<contactref element="_1" pad="B4"/>
</signal>
<signal name="N$19">
<contactref element="J1" pad="11"/>
<contactref element="_1" pad="B5"/>
</signal>
<signal name="N$20">
<contactref element="J1" pad="10"/>
<contactref element="_1" pad="B6"/>
</signal>
<signal name="N$21">
<contactref element="J1" pad="9"/>
<contactref element="_1" pad="F7"/>
</signal>
<signal name="N$22">
<contactref element="J1" pad="8"/>
<contactref element="_1" pad="F6"/>
</signal>
<signal name="N$23">
<contactref element="J1" pad="7"/>
<contactref element="_1" pad="F5"/>
</signal>
<signal name="N$24">
<contactref element="J1" pad="6"/>
<contactref element="_1" pad="F4"/>
</signal>
<signal name="N$25">
<contactref element="J1" pad="5"/>
<contactref element="_1" pad="F1"/>
</signal>
<signal name="N$26">
<contactref element="J1" pad="4"/>
<contactref element="_1" pad="F0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
