<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="2.2225" x2="21.59" y2="2.2225" width="0.254" layer="20"/>
<wire x1="29.21" y1="9.8425" x2="29.21" y2="23.1775" width="0.254" layer="20"/>
<text>AUX Module
v1.2</text>
<hole x="11.43" y="16.51" drill="2.8"/>
<text>-LD</text>
<text>LED
+</text>
<text>LED
-</text>
<text>+Solnd</text>
<text>-Solnd</text>
<text>+LD</text>
<text>-ND</text>
<text>+ND</text>
<text>+NE</text>
<text>-NE</text>
<text>-LE</text>
<text>+LE</text>
<wire x1="21.59" y1="30.7975" x2="3.81" y2="30.7975" width="0.254" layer="20"/>
<wire x1="1.905" y1="28.8925" x2="1.905" y2="4.1275" width="0.254" layer="20"/>
<wire x1="21.59" y1="2.2225" x2="29.21" y2="9.8425" width="0.254" layer="20" curve="90"/>
<wire x1="3.81" y1="30.7975" x2="1.905" y2="28.8925" width="0.254" layer="20" curve="90"/>
<wire x1="1.905" y1="4.1275" x2="3.81" y2="2.2225" width="0.254" layer="20" curve="90"/>
<text>AUX Module
v1.2</text>
<wire x1="29.21" y1="23.1775" x2="21.59" y2="30.7975" width="0.254" layer="20" curve="90"/>
<text>-&gt;|-</text>
</plain>
<libraries>
<library name="Andy-library">
<packages>
<package name="AXIAL-0.1">
</package>
<package name="RJ45-8">
</package>
<package name="1X06_NO_SILK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.1" value="5.6K">
<attribute name="PARTNO" value="54602-908LF"/>
<attribute name="VALUE"/>
</element>
<element name="NPN" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1" value="82">
<attribute name="PARTNO" value="54602-908LF"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="82">
<attribute name="PARTNO" value="54602-908LF"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1" value="82">
<attribute name="PARTNO" value="54602-908LF"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.1" value="5.6K">
<attribute name="PARTNO" value="54602-908LF"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.1" value="L5.6k">
<attribute name="PARTNO" value="54602-908LF"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Andy-library" package="RJ45-8" value="RJ45"/>
<element name="X3" library="Andy-library" package="1X06_NO_SILK" value="TERMINAL_SMALL_6POS"/>
<element name="X4" library="Andy-library" package="1X06_NO_SILK" value="TERMINAL_SMALL_6POS"/>
<element name="DIODE" library="Andy-library" package="AXIAL-0.1" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Retired" package="SJ_2S" value="SOLDERJUMPERNC">
<attribute name="NAME"/>
</element>
<element name="J5" library="SparkFun-Retired" package="SJ_2S" value="SOLDERJUMPERNC">
<attribute name="NAME"/>
</element>
<element name="J12" library="SparkFun-Retired" package="SJ_2S" value="SOLDERJUMPERNC">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="U$5" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="5"/>
<contactref element="NPN" pad="E"/>
<contactref element="X4" pad="3"/>
<contactref element="X4" pad="1"/>
<contactref element="X3" pad="5"/>
<contactref element="X3" pad="3"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="OUT2">
<contactref element="U$2" pad="2"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="5VDC">
<contactref element="U$2" pad="4"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="12VDC">
<contactref element="U$2" pad="6"/>
<contactref element="J12" pad="1"/>
</signal>
<signal name="3.3VDC">
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="U$2" pad="7"/>
<contactref element="R4" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="P$1"/>
<contactref element="X3" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="P$2"/>
<contactref element="NPN" pad="B"/>
</signal>
<signal name="N$7">
<contactref element="NPN" pad="C"/>
<contactref element="DIODE" pad="P$1"/>
<contactref element="X4" pad="5"/>
</signal>
<signal name="OUT1">
<contactref element="U$2" pad="3"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="IN1">
<contactref element="R4" pad="P$1"/>
<contactref element="X4" pad="4"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="U$2" pad="8"/>
<contactref element="R3" pad="P$1"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$1"/>
<contactref element="X3" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="J3" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J12" pad="2"/>
<contactref element="DIODE" pad="P$2"/>
<contactref element="X4" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="R6" pad="P$1"/>
<contactref element="X3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
