<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.96" y2="0" width="0" layer="20"/>
<wire x1="33.96" y1="0" x2="33.96" y2="39.36" width="0" layer="20"/>
<wire x1="33.96" y1="39.36" x2="0" y2="39.36" width="0" layer="20"/>
<wire x1="0" y1="39.36" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="3.81" drill="5"/>
<hole x="3.81" y="35.56" drill="5"/>
<hole x="30.48" y="35.56" drill="5"/>
<hole x="30.48" y="3.81" drill="5"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA7343">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-123">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2">
</package>
<package name="MOLEX-1X3">
</package>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="smd-special">
<description>&lt;b&gt;Special SMD Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMS-002">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SKHMPXE010">
<description>&lt;b&gt;6.2 X 6.5mm TACT Switch (SMD)&lt;/b&gt;&lt;p&gt;
Source: http://www3.alps.co.jp/WebObjects/catalog.woa/PDF/E/Switch/Tact/SKHM/SKHM.PDF</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="lio">
<packages>
<package name="ESP-07">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="EIA7343" value="100uF">
<attribute name="PROD_ID" value="CAP-07890"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="EIA7343" value="100uF">
<attribute name="PROD_ID" value="CAP-07890"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-123" value="16V">
<attribute name="PROD_ID" value="DIO-12440"/>
</element>
<element name="IC1" library="v-reg" package="DPACK" value="LD117ADT33TR"/>
<element name="IC2" library="v-reg" package="DPACK" value="LD117ADT50TR"/>
<element name="JP1" library="SparkFun-Connectors" package="MOLEX-1X2" value="PWR"/>
<element name="JP2" library="SparkFun-Connectors" package="MOLEX-1X3" value="UART">
<attribute name="3" value="GND"/>
<attribute name="1" value="TX"/>
<attribute name="2" value="RX"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="MOLEX-1X4" value="IIC"/>
<element name="R1" library="SparkFun-Resistors" package="1206" value="4K7"/>
<element name="R2" library="SparkFun-Resistors" package="1206" value="4K7"/>
<element name="R3" library="SparkFun-Resistors" package="1206" value="4K7"/>
<element name="R4" library="SparkFun-Resistors" package="1206" value="150K"/>
<element name="R5" library="SparkFun-Resistors" package="1206" value="10K"/>
<element name="S1" library="smd-special" package="SMS-002" value="FW"/>
<element name="S2" library="switch" package="SKHMPXE010" value="SKHMPSE010">
<attribute name="RST"/>
</element>
<element name="ESP-07" library="lio" package="ESP-07" value="ESP8266-07"/>
<element name="R6" library="SparkFun-Resistors" package="1206" value="4K7"/>
<element name="R7" library="SparkFun-Resistors" package="1206" value="4K7"/>
<element name="JP5" library="SparkFun-Connectors" package="MOLEX-1X3" value="OneWire">
<attribute name="3" value="GND"/>
<attribute name="1" value="TX"/>
<attribute name="2" value="RX"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="1206" value="4K7"/>
<element name="JP4" library="con-lstb" package="MA04-2" value="GPIO">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="C"/>
<contactref element="C1" pad="C"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R5" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="ESP-07" pad="GND"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="A"/>
<contactref element="ESP-07" pad="VCC"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="JP5" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="+5V">
<contactref element="IC2" pad="4"/>
<contactref element="C2" pad="A"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="ESP-07" pad="REST"/>
<contactref element="S2" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="ESP-07" pad="CH_PD"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="ESP-07" pad="TXD"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="ESP-07" pad="RXD"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="ESP-07" pad="GPIO0"/>
<contactref element="S1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="ESP-07" pad="GPIO15"/>
<contactref element="S1" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="ESP-07" pad="ADC"/>
</signal>
<signal name="SCL">
<contactref element="JP3" pad="3"/>
<contactref element="ESP-07" pad="GPIO2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="ESP-07" pad="GPIO16"/>
<contactref element="JP5" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="ESP-07" pad="GPIO4"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="ESP-07" pad="GPIO5"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="ESP-07" pad="GPIO12"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="ESP-07" pad="GPIO14"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="ESP-07" pad="GPIO13"/>
<contactref element="JP4" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
