<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="2" y1="0" x2="63" y2="0" width="0" layer="20"/>
<wire x1="65" y1="2" x2="65" y2="13" width="0" layer="20"/>
<hole x="3" y="8" drill="3"/>
<hole x="51.5" y="8" drill="3"/>
<wire x1="63" y1="15" x2="2" y2="15" width="0" layer="20"/>
<wire x1="0" y1="13" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="13" x2="2" y2="15" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="63" y1="0" x2="65" y2="2" width="0" layer="20" curve="90"/>
<wire x1="63" y1="15" x2="65" y2="13" width="0" layer="20" curve="-90"/>
</plain>
<libraries>
<library name="opto-trans-siemens">
<description>&lt;b&gt;Siemens Opto Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SFH303">
<description>&lt;b&gt;Silicon NPN Phototransistor&lt;/b&gt;&lt;p&gt;
Source: Siemens</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="colin">
<packages>
<package name="SFV14R">
</package>
<package name="D6R">
</package>
<package name="PJ-011">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="T1" library="opto-trans-siemens" package="SFH303" value="SFH303">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="33K">
<attribute name="NAME"/>
</element>
<element name="HOUR" library="colin" package="D6R" value="SWMOM">
<attribute name="MFN" value="D6R90 F1 LFS"/>
<attribute name="MOUSER" value="611-D6R90LFS"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="DIODE-SCHOTTKY-B340A">
<attribute name="PROD_ID" value="DIO-09886"/>
<attribute name="MFN" value="SSA33L-E3/61T"/>
<attribute name="MOUSER" value="625-SSA33L-E3"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="colin" package="SFV14R" value="SFV14R-1STE1HLF">
<attribute name="MFN" value="SFV14R-1STE1HLF"/>
<attribute name="MOUSER" value="649-SFV14R-1STE1HLF"/>
<attribute name="DIGIKEY" value="609-4309-1-ND"/>
</element>
<element name="MIN" library="colin" package="D6R" value="SWMOM">
<attribute name="MFN" value="D6R90 F1 LFS"/>
<attribute name="MOUSER" value="611-D6R90LFS"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="colin" package="PJ-011" value="JACK_SIMPLE">
<attribute name="MFN" value="PJ-011A"/>
<attribute name="MOUSER" value="490-PJ-011A"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.3V">
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="NAME"/>
<attribute name="MFN" value="MM3Z3V3T1G"/>
<attribute name="MOUSER" value="863-MM3Z3V3T1G"/>
</element>
</elements>
<signals>
<signal name="LIGHT_SENSOR">
<contactref element="T1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="14"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="HOUR" pad="Y0"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="5"/>
<contactref element="HOUR" pad="Y1"/>
<contactref element="MIN" pad="Y1"/>
<contactref element="MIN" pad="Y0"/>
<contactref element="U$1" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="+12V">
<contactref element="T1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="MINUTE">
<contactref element="J1" pad="12"/>
<contactref element="MIN" pad="X0"/>
<contactref element="MIN" pad="X1"/>
</signal>
<signal name="HOUR">
<contactref element="HOUR" pad="X0"/>
<contactref element="J1" pad="13"/>
<contactref element="HOUR" pad="X1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="A"/>
<contactref element="U$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
