<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="39.37" x2="22.911" y2="39.37" width="0" layer="20"/>
<wire x1="22.911" y1="39.37" x2="22.911" y2="62.22" width="0" layer="20"/>
<wire x1="22.911" y1="62.22" x2="0" y2="62.22" width="0" layer="20"/>
<wire x1="0" y1="62.22" x2="0" y2="39.37" width="0" layer="20"/>
<text>Moo 1.1 Programmer
Josiah Hester
Clemson University</text>
<text>13</text>
<text>14</text>
<text>GND</text>
<text>GND</text>
<text>RST</text>
<text>TDI</text>
<text>TMS</text>
<text>TDO</text>
<text>TCK</text>
<text>VREG</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="josiahlib">
<packages>
<package name="M10">
</package>
<package name="M07X2">
<description>&lt;b&gt;MSP430FET-UIF connector&lt;/b&gt;&lt;br&gt;
0.1in pitched headers adapted from Sparkfun library.
7x2 for connecting to the MSP430FET-UIF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="U$1" library="josiahlib" package="M10" value="M10"/>
<element name="U$2" library="josiahlib" package="M07X2" value="M7X2UIFCONNECTOR"/>
</elements>
<signals>
<signal name="TDO">
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="TDI">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="TMS">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="TCK">
<contactref element="U$1" pad="9"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
