<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.62" y2="0" width="0" layer="20"/>
<wire x1="40.62" y1="0" x2="40.62" y2="32.69" width="0" layer="20"/>
<wire x1="40.62" y1="32.69" x2="0" y2="32.69" width="0" layer="20"/>
<wire x1="0" y1="32.69" x2="0" y2="0" width="0" layer="20"/>
<text>RS-232 Hard Tap
TX/RX Switch Module
Phantomic Labs, 2018</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;h3&gt;9 Pin Serial Connector - Female PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/DB9-PCB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH_SPDT_PTH_11.6X4.0MM">
<description>&lt;h3&gt;SPDT PTH Slide Switch&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/P040040c.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-6.5MM">
<description>2.5 mm spaced PTHs with 6.5 mm diameter outline</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
<description>&lt;h3&gt;AXIAL-0.1&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="DB9" value="DUT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="DB9" value="TAP0">
<attribute name="PROD_ID" value="CONN-08194"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-6.5MM" value="2.2uF">
<attribute name="PROD_ID" value="CAP-08439"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D4" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="10k">
<attribute name="PROD_ID" value="RES-09435"/>
</element>
<element name="S1" library="SparkFun-Switches" package="SWITCH_SPDT_PTH_11.6X4.0MM" value="">
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102"/>
</element>
<element name="S2" library="SparkFun-Switches" package="SWITCH_SPDT_PTH_11.6X4.0MM" value="">
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102"/>
</element>
</elements>
<signals>
<signal name="CD_DUT">
<contactref element="J1" pad="1"/>
</signal>
<signal name="RX_DUT">
<contactref element="J1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="TX_DUT">
<contactref element="J1" pad="3"/>
<contactref element="D3" pad="C"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="DTR_DUT">
<contactref element="J1" pad="4"/>
</signal>
<signal name="DST_DUT">
<contactref element="J1" pad="6"/>
</signal>
<signal name="RTS_DUT">
<contactref element="J1" pad="7"/>
</signal>
<signal name="CTS_DUT">
<contactref element="J1" pad="8"/>
</signal>
<signal name="RI_DUT">
<contactref element="J1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="7"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="D4" pad="C"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D5" pad="C"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="TX_TAP0">
<contactref element="J2" pad="3"/>
<contactref element="R1" pad="P$2"/>
<contactref element="S1" pad="3"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="RX_TAP0">
<contactref element="J2" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
