<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="93.98" y1="0" x2="93.98" y2="20.3199875" width="0" layer="20"/>
<wire x1="93.98" y1="20.3199875" x2="91.4399875" y2="22.8599875" width="0" layer="20" curve="90.000282"/>
<wire x1="91.4399875" y1="22.8599875" x2="27.95" y2="22.859715625" width="0" layer="20"/>
<wire x1="27.95" y1="22.859715625" x2="0" y2="22.859715625" width="0" layer="20"/>
<wire x1="0" y1="22.859715625" x2="-2.54" y2="20.319715625" width="0" layer="20" curve="90"/>
<wire x1="-2.54" y1="20.319715625" x2="-2.54" y2="0" width="0" layer="20"/>
<wire x1="-2.54" y1="0" x2="0" y2="-2.54" width="0" layer="20" curve="90"/>
<wire x1="0" y1="-2.54" x2="91.44" y2="-2.54" width="0" layer="20"/>
<wire x1="91.44" y1="-2.54" x2="93.98" y2="0" width="0" layer="20" curve="90"/>
<text>UI Board - tobias.einarsson@gmail.com</text>
<hole x="1.27" y="19.05" drill="3.2"/>
<hole x="1.27" y="1.27" drill="3.2"/>
<hole x="90.17" y="1.27" drill="3.2"/>
<hole x="90.17" y="19.05" drill="3.2"/>
<text>BTN 1
BTN 2
BTN 3
BTN 4
ENC A
ENC B
ENC SW
+5V
GND</text>
</plain>
<libraries>
<library name="switch-misc">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, RAFI, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DTE6">
<description>&lt;b&gt;ITT SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-alps">
<description>ALPS Switch from Markus Faust &amp;lt;mfaust@htwm.de&amp;gt;&lt;p&gt;
Source: EC12E.scr from eagle.support.ger on news.cadsoft.de at 08.10.2007</description>
<packages>
<package name="ALPS_EC12E_SW">
<description>ALPS rotary encoder&lt;br&gt;
EC12E series with push-on switch</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BTN1" library="switch-misc" package="DTE6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN2" library="switch-misc" package="DTE6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN3" library="switch-misc" package="DTE6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN4" library="switch-misc" package="DTE6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL2" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL2" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X09" value="M09"/>
<element name="ROTARY" library="switch-alps" package="ALPS_EC12E_SW" value="ENCODER">
<attribute name="OC_NEWARK" value="74M1068"/>
<attribute name="MPN" value="EC12E2424407"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1520813"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="BTN1" pad="3"/>
<contactref element="BTN1" pad="4"/>
<contactref element="BTN2" pad="3"/>
<contactref element="BTN2" pad="4"/>
<contactref element="BTN3" pad="3"/>
<contactref element="BTN3" pad="4"/>
<contactref element="BTN4" pad="3"/>
<contactref element="BTN4" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="9"/>
<contactref element="ROTARY" pad="C"/>
<contactref element="ROTARY" pad="D"/>
</signal>
<signal name="N$1">
<contactref element="BTN1" pad="1"/>
<contactref element="BTN1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="BTN2" pad="1"/>
<contactref element="BTN2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="BTN3" pad="1"/>
<contactref element="BTN3" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="BTN4" pad="1"/>
<contactref element="BTN4" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="P$2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="ROTARY" pad="A"/>
<contactref element="ROTARY" pad="B"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="P$2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="P$1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="7"/>
<contactref element="ROTARY" pad="E"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
