<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.12" y2="0" width="0" layer="20"/>
<wire x1="71.12" y1="0" x2="71.12" y2="54.219" width="0" layer="20"/>
<wire x1="71.12" y1="54.219" x2="0" y2="54.219" width="0" layer="20"/>
<wire x1="0" y1="54.219" x2="0" y2="0" width="0" layer="20"/>
<text>22Ω</text>
<text>22Ω</text>
<text>1kΩ</text>
<text>220Ω</text>
<text>5V</text>
<text>GND</text>
<text>Wireless Pendant v2</text>
<text>github.com/AMPWorks</text>
<hole x="10.414" y="47.752" drill="2.921"/>
<text>ampworksstudio.com</text>
<hole x="52.07" y="2.54" drill="2.921"/>
<text>4.7kΩ*</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="LED-0603">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="PTC-1206">
</package>
<package name="1X12">
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="USB-AB-MICRO-SMD-V03-IN&amp;OUT">
</package>
<package name="QFN-20-0.4MM-V2">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES@1">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="RFM12B-ANTENNA">
</package>
<package name="RFM69W-MINPADS">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P1200X1200X120-44N">
</package>
</packages>
</library>
<library name="APA102">
<packages>
<package name="5050">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R11" library="SparkFun" package="0603-RES" value="1K"/>
<element name="L1" library="SparkFun" package="LED-0603" value="Red"/>
<element name="R2" library="SparkFun" package="0603-RES" value="10K"/>
<element name="C20" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="Y1" library="SparkFun" package="CRYSTAL-SMD-5X3" value="16MHz"/>
<element name="C22" library="SparkFun" package="0603-CAP" value="22pF"/>
<element name="C23" library="SparkFun" package="0603-CAP" value="22pF"/>
<element name="C24" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C25" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="R5" library="SparkFun" package="0603-RES" value="22"/>
<element name="R7" library="SparkFun" package="0603-RES" value="22"/>
<element name="X2" library="Testing" package="USB-AB-MICRO-SMD-V03-IN&amp;OUT" value=""/>
<element name="F1" library="SparkFun" package="PTC-1206" value="500mA"/>
<element name="R8" library="SparkFun-Resistors" package="0603-RES@1" value="220">
<attribute name="PROD_ID" value="RES-07861"/>
</element>
<element name="ISP" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="U$1" library="LowPowerLab" package="RFM12B-ANTENNA" value="RFM12B_ANTENNA"/>
<element name="RMF69" library="LowPowerLab" package="RFM69W-MINPADS" value="RFM69"/>
<element name="IC1" library="Testing" package="QFN-20-0.4MM-V2" value="MPR121"/>
<element name="C27" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="R1" library="SparkFun" package="0603-RES" value="75k"/>
<element name="C28" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="CAPSENSORS" library="SparkFun" package="1X12" value="Electrodes"/>
<element name="R3" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="R4" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="R9" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="S1" library="SparkFun" package="TACTILE_SWITCH_SMD" value="Reset"/>
<element name="PWR" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="7805" library="linear" package="TO220V" value="7805TV"/>
<element name="7803-???" library="linear" package="TO220V" value="7805TV"/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P1200X1200X120-44N" value="ATMEGA32U4-AU">
<attribute name="OC_NEWARK" value="26R5633"/>
<attribute name="OC_FARNELL" value="1748525"/>
<attribute name="PACKAGE" value="TQFP-44"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="MPN" value="ATMEGA32U4-AU"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES@1" value="220">
<attribute name="PROD_ID" value="RES-07861"/>
</element>
<element name="LED0" library="APA102" package="5050" value="APA102"/>
<element name="LED1" library="APA102" package="5050" value="APA102"/>
<element name="LED2" library="APA102" package="5050" value="APA102"/>
<element name="LED3" library="APA102" package="5050" value="APA102"/>
<element name="LED4" library="APA102" package="5050" value="APA102"/>
<element name="LED5" library="APA102" package="5050" value="APA102"/>
<element name="LED6" library="APA102" package="5050" value="APA102"/>
<element name="LED7" library="APA102" package="5050" value="APA102"/>
<element name="LED8" library="APA102" package="5050" value="APA102"/>
<element name="LED9" library="APA102" package="5050" value="APA102"/>
<element name="LED10" library="APA102" package="5050" value="APA102"/>
<element name="LED11" library="APA102" package="5050" value="APA102"/>
<element name="LED12" library="APA102" package="5050" value="APA102"/>
<element name="LED13" library="APA102" package="5050" value="APA102"/>
<element name="LED14" library="APA102" package="5050" value="APA102"/>
<element name="LED15" library="APA102" package="5050" value="APA102"/>
<element name="R10" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="D2" library="SparkFun" package="SOD-323" value=""/>
<element name="R12" library="SparkFun" package="0603-RES" value="10k"/>
<element name="SWITCH" library="SparkFun-Connectors" package="2X3" value="SWITCH">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="L1" pad="C"/>
<contactref element="C20" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="X2" pad="GND1"/>
<contactref element="ISP" pad="6"/>
<contactref element="RMF69" pad="GND"/>
<contactref element="C27" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="C28" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="7805" pad="2"/>
<contactref element="PWR" pad="2"/>
<contactref element="7803-???" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="33"/>
<contactref element="LED0" pad="3-GND"/>
<contactref element="LED1" pad="3-GND"/>
<contactref element="LED2" pad="3-GND"/>
<contactref element="LED3" pad="3-GND"/>
<contactref element="LED4" pad="3-GND"/>
<contactref element="LED5" pad="3-GND"/>
<contactref element="LED6" pad="3-GND"/>
<contactref element="LED7" pad="3-GND"/>
<contactref element="LED8" pad="3-GND"/>
<contactref element="LED9" pad="3-GND"/>
<contactref element="LED10" pad="3-GND"/>
<contactref element="LED11" pad="3-GND"/>
<contactref element="LED12" pad="3-GND"/>
<contactref element="LED13" pad="3-GND"/>
<contactref element="LED14" pad="3-GND"/>
<contactref element="LED15" pad="3-GND"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="5V">
<contactref element="R2" pad="2"/>
<contactref element="ISP" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="7805" pad="3"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="44"/>
<contactref element="U1" pad="24"/>
<contactref element="LED0" pad="4-VCC"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="F1" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C20" pad="2"/>
<contactref element="U1" pad="42"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="1"/>
<contactref element="ISP" pad="5"/>
<contactref element="S1" pad="3"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="RMF69" pad="SCK"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="R11" pad="1"/>
<contactref element="L1" pad="A"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="RMF69" pad="MOSI"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="RAW">
<contactref element="7805" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="SWITCH" pad="4"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="28"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="41"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="40"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="39"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="38"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="37"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="25"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="27"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="1"/>
</signal>
<signal name="LEDS_DI">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="USBVCC">
<contactref element="C25" pad="2"/>
<contactref element="X2" pad="VBUS1"/>
<contactref element="F1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D-">
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="D+">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="D11">
<contactref element="U1" pad="12"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="26"/>
</signal>
<signal name="N$20">
<contactref element="R7" pad="2"/>
<contactref element="X2" pad="D-1"/>
</signal>
<signal name="N$21">
<contactref element="R5" pad="2"/>
<contactref element="X2" pad="D+1"/>
</signal>
<signal name="SS">
<contactref element="RMF69" pad="NSS"/>
<contactref element="U1" pad="8"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="P$1"/>
<contactref element="RMF69" pad="ANA"/>
</signal>
<signal name="VREG">
<contactref element="IC1" pad="5"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="ADDR">
<contactref element="IC1" pad="4"/>
</signal>
<signal name="REXT">
<contactref element="IC1" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CA011">
<contactref element="IC1" pad="19"/>
<contactref element="CAPSENSORS" pad="1"/>
</signal>
<signal name="CAP10">
<contactref element="IC1" pad="18"/>
<contactref element="CAPSENSORS" pad="2"/>
</signal>
<signal name="CAP9">
<contactref element="IC1" pad="17"/>
<contactref element="CAPSENSORS" pad="3"/>
</signal>
<signal name="CAP8">
<contactref element="IC1" pad="16"/>
<contactref element="CAPSENSORS" pad="4"/>
</signal>
<signal name="CAP7">
<contactref element="IC1" pad="15"/>
<contactref element="CAPSENSORS" pad="5"/>
</signal>
<signal name="CAP6">
<contactref element="IC1" pad="14"/>
<contactref element="CAPSENSORS" pad="6"/>
</signal>
<signal name="CAP5">
<contactref element="IC1" pad="13"/>
<contactref element="CAPSENSORS" pad="7"/>
</signal>
<signal name="CAP4">
<contactref element="IC1" pad="12"/>
<contactref element="CAPSENSORS" pad="8"/>
</signal>
<signal name="CAP3">
<contactref element="IC1" pad="11"/>
<contactref element="CAPSENSORS" pad="9"/>
</signal>
<signal name="CAP2">
<contactref element="IC1" pad="10"/>
<contactref element="CAPSENSORS" pad="10"/>
</signal>
<signal name="CAP1">
<contactref element="IC1" pad="9"/>
<contactref element="CAPSENSORS" pad="11"/>
</signal>
<signal name="CAP0">
<contactref element="IC1" pad="8"/>
<contactref element="CAPSENSORS" pad="12"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="20"/>
<contactref element="C28" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="RMF69" pad="VDD"/>
<contactref element="7803-???" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="MPRIRQ">
<contactref element="IC1" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="RMFIRQ">
<contactref element="RMF69" pad="DIO0"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="D14">
<contactref element="U1" pad="22"/>
</signal>
<signal name="XTAL2">
<contactref element="U1" pad="16"/>
<contactref element="Y1" pad="1"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="XTAL1">
<contactref element="U1" pad="17"/>
<contactref element="Y1" pad="3"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="U1" pad="6"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="36"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R8" pad="2"/>
<contactref element="LED0" pad="1-DI"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="2"/>
<contactref element="LED0" pad="2-CI"/>
</signal>
<signal name="LEDS_CI">
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="N$2">
<contactref element="LED0" pad="6-DO"/>
<contactref element="LED1" pad="1-DI"/>
</signal>
<signal name="N$4">
<contactref element="LED0" pad="5-CO"/>
<contactref element="LED1" pad="2-CI"/>
</signal>
<signal name="VCC">
<contactref element="LED1" pad="4-VCC"/>
<contactref element="LED2" pad="4-VCC"/>
<contactref element="LED3" pad="4-VCC"/>
<contactref element="LED4" pad="4-VCC"/>
<contactref element="LED5" pad="4-VCC"/>
<contactref element="LED6" pad="4-VCC"/>
<contactref element="LED7" pad="4-VCC"/>
<contactref element="LED8" pad="4-VCC"/>
<contactref element="LED9" pad="4-VCC"/>
<contactref element="LED10" pad="4-VCC"/>
<contactref element="LED11" pad="4-VCC"/>
<contactref element="LED12" pad="4-VCC"/>
<contactref element="LED13" pad="4-VCC"/>
<contactref element="LED14" pad="4-VCC"/>
<contactref element="LED15" pad="4-VCC"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="6-DO"/>
<contactref element="LED2" pad="1-DI"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="5-CO"/>
<contactref element="LED2" pad="2-CI"/>
</signal>
<signal name="N$7">
<contactref element="LED2" pad="6-DO"/>
<contactref element="LED3" pad="1-DI"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="5-CO"/>
<contactref element="LED3" pad="2-CI"/>
</signal>
<signal name="N$9">
<contactref element="LED3" pad="5-CO"/>
<contactref element="LED4" pad="2-CI"/>
</signal>
<signal name="N$10">
<contactref element="LED3" pad="6-DO"/>
<contactref element="LED4" pad="1-DI"/>
</signal>
<signal name="N$11">
<contactref element="LED4" pad="6-DO"/>
<contactref element="LED5" pad="1-DI"/>
</signal>
<signal name="N$12">
<contactref element="LED4" pad="5-CO"/>
<contactref element="LED5" pad="2-CI"/>
</signal>
<signal name="N$13">
<contactref element="LED5" pad="6-DO"/>
<contactref element="LED6" pad="1-DI"/>
</signal>
<signal name="N$14">
<contactref element="LED6" pad="2-CI"/>
<contactref element="LED5" pad="5-CO"/>
</signal>
<signal name="N$15">
<contactref element="LED6" pad="6-DO"/>
<contactref element="LED7" pad="1-DI"/>
</signal>
<signal name="N$16">
<contactref element="LED7" pad="2-CI"/>
<contactref element="LED6" pad="5-CO"/>
</signal>
<signal name="N$17">
<contactref element="LED7" pad="5-CO"/>
<contactref element="LED8" pad="2-CI"/>
</signal>
<signal name="N$18">
<contactref element="LED8" pad="1-DI"/>
<contactref element="LED7" pad="6-DO"/>
</signal>
<signal name="N$19">
<contactref element="LED8" pad="6-DO"/>
<contactref element="LED9" pad="1-DI"/>
</signal>
<signal name="N$22">
<contactref element="LED9" pad="2-CI"/>
<contactref element="LED8" pad="5-CO"/>
</signal>
<signal name="N$23">
<contactref element="LED9" pad="6-DO"/>
<contactref element="LED10" pad="1-DI"/>
</signal>
<signal name="N$24">
<contactref element="LED10" pad="2-CI"/>
<contactref element="LED9" pad="5-CO"/>
</signal>
<signal name="N$26">
<contactref element="LED10" pad="6-DO"/>
<contactref element="LED11" pad="1-DI"/>
</signal>
<signal name="N$27">
<contactref element="LED11" pad="2-CI"/>
<contactref element="LED10" pad="5-CO"/>
</signal>
<signal name="N$28">
<contactref element="LED11" pad="6-DO"/>
<contactref element="LED12" pad="1-DI"/>
</signal>
<signal name="N$29">
<contactref element="LED12" pad="2-CI"/>
<contactref element="LED11" pad="5-CO"/>
</signal>
<signal name="N$30">
<contactref element="LED13" pad="1-DI"/>
<contactref element="LED12" pad="6-DO"/>
</signal>
<signal name="N$31">
<contactref element="LED12" pad="5-CO"/>
<contactref element="LED13" pad="2-CI"/>
</signal>
<signal name="N$32">
<contactref element="LED13" pad="6-DO"/>
<contactref element="LED14" pad="1-DI"/>
</signal>
<signal name="N$33">
<contactref element="LED14" pad="2-CI"/>
<contactref element="LED13" pad="5-CO"/>
</signal>
<signal name="N$34">
<contactref element="LED14" pad="6-DO"/>
<contactref element="LED15" pad="1-DI"/>
</signal>
<signal name="N$35">
<contactref element="LED14" pad="5-CO"/>
<contactref element="LED15" pad="2-CI"/>
</signal>
<signal name="LEDS_DO">
<contactref element="LED15" pad="6-DO"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="LEDS_CO">
<contactref element="LED15" pad="5-CO"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name=".">
<contactref element="RMF69" pad="MISO"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="PWR" pad="1"/>
<contactref element="SWITCH" pad="6"/>
</signal>
<signal name="N$37">
<contactref element="C4" pad="2"/>
<contactref element="7803-???" pad="3"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="31"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D13">
<contactref element="U1" pad="32"/>
<contactref element="JP2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
