<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.24" y2="0" width="0.254" layer="20"/>
<wire x1="15.24" y1="0" x2="15.24" y2="20.32" width="0.254" layer="20"/>
<wire x1="15.24" y1="20.32" x2="9.8425" y2="20.32" width="0.254" layer="20"/>
<wire x1="5.3975" y1="20.32" x2="0" y2="20.32" width="0.254" layer="20"/>
<wire x1="0" y1="20.32" x2="0" y2="0" width="0.254" layer="20"/>
<text>GND</text>
<text>LEFT</text>
<text>RIGHT</text>
<text>KD0GLS 2019</text>
<wire x1="6.35" y1="18.7325" x2="8.89" y2="18.7325" width="0.254" layer="20"/>
<wire x1="5.3975" y1="19.685" x2="5.3975" y2="20.32" width="0.254" layer="20"/>
<wire x1="9.8425" y1="19.685" x2="9.8425" y2="20.32" width="0.254" layer="20"/>
<wire x1="6.35" y1="18.7325" x2="5.3975" y2="19.685" width="0.254" layer="20" curve="-90"/>
<wire x1="9.8425" y1="19.685" x2="8.89" y2="18.7325" width="0.254" layer="20" curve="-90"/>
<text>GND</text>
<text>GND</text>
<text>RNG</text>
<text>TIP</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="CONN_3.5MM_STEREO_JACK_CUI">
<description>SJ1-3523N</description>
</package>
<package name="CONN_BREAKAWAY_1X5_100">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="kd0gls" package="CONN_3.5MM_STEREO_JACK_CUI" value="CONN_JACK_STEREO_3.5MMCUI"/>
<element name="J3" library="kd0gls" package="CONN_BREAKAWAY_1X5_100" value="CONN_BREAKAWAY_1X5_100"/>
</elements>
<signals>
<signal name="RIGHT">
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="LEFT">
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
