<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="0" x2="19.05" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="0" x2="19.05" y2="74.93" width="0" layer="20"/>
<wire x1="19.05" y1="74.93" x2="-1.27" y2="74.93" width="0" layer="20"/>
<wire x1="-1.27" y1="74.93" x2="-1.27" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>21</text>
<text>22</text>
<text>23</text>
<text>3.3V</text>
<text>AGND</text>
<text>Vin</text>
<text>USB</text>
<text>Teensy
3.1/3.2/4.0
Breakout</text>
<text>Note Reversed Order!</text>
<text>britt@shapetable.com</text>
<text>2x GND</text>
</plain>
<libraries>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1_MOST_BASIC">
</package>
</packages>
</library>
<library name="con-lstb-joe">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA14-1">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MOD1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_MOST_BASIC" value="TEENSY_3.1_MOST_BASIC"/>
<element name="J1B" library="con-lstb-joe" package="MA14-1" value="MA14-1"/>
<element name="J1A" library="con-lstb-joe" package="MA14-1" value="MA14-1"/>
<element name="MOD2" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_MOST_BASIC" value="TEENSY_3.1_MOST_BASIC"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
</elements>
<signals>
<signal name="0">
<contactref element="MOD1" pad="0"/>
<contactref element="J1A" pad="2"/>
</signal>
<signal name="1">
<contactref element="MOD1" pad="1"/>
<contactref element="J1A" pad="3"/>
</signal>
<signal name="2">
<contactref element="MOD1" pad="2"/>
<contactref element="J1A" pad="4"/>
</signal>
<signal name="3">
<contactref element="MOD1" pad="3"/>
<contactref element="J1A" pad="5"/>
</signal>
<signal name="4">
<contactref element="MOD1" pad="4"/>
<contactref element="J1A" pad="6"/>
</signal>
<signal name="5">
<contactref element="MOD1" pad="5"/>
<contactref element="J1A" pad="7"/>
</signal>
<signal name="6">
<contactref element="MOD1" pad="6"/>
<contactref element="J1A" pad="8"/>
</signal>
<signal name="7">
<contactref element="MOD1" pad="7"/>
<contactref element="J1A" pad="9"/>
</signal>
<signal name="8">
<contactref element="MOD1" pad="8"/>
<contactref element="J1A" pad="10"/>
</signal>
<signal name="9">
<contactref element="MOD1" pad="9"/>
<contactref element="J1A" pad="11"/>
</signal>
<signal name="10">
<contactref element="MOD1" pad="10"/>
<contactref element="J1A" pad="12"/>
</signal>
<signal name="11">
<contactref element="MOD1" pad="11"/>
<contactref element="J1A" pad="13"/>
</signal>
<signal name="12">
<contactref element="MOD1" pad="12"/>
<contactref element="J1A" pad="14"/>
</signal>
<signal name="13">
<contactref element="MOD1" pad="13"/>
<contactref element="J1B" pad="14"/>
</signal>
<signal name="14">
<contactref element="MOD1" pad="14/A0"/>
<contactref element="J1B" pad="13"/>
</signal>
<signal name="15">
<contactref element="MOD1" pad="15/A1"/>
<contactref element="J1B" pad="12"/>
</signal>
<signal name="16">
<contactref element="MOD1" pad="16/A2"/>
<contactref element="J1B" pad="11"/>
</signal>
<signal name="17">
<contactref element="MOD1" pad="17/A3"/>
<contactref element="J1B" pad="10"/>
</signal>
<signal name="18">
<contactref element="MOD1" pad="18/A4"/>
<contactref element="J1B" pad="9"/>
</signal>
<signal name="19">
<contactref element="MOD1" pad="19/A5"/>
<contactref element="J1B" pad="8"/>
</signal>
<signal name="20">
<contactref element="MOD1" pad="20/A6"/>
<contactref element="J1B" pad="7"/>
</signal>
<signal name="21">
<contactref element="MOD1" pad="21/A7"/>
<contactref element="J1B" pad="6"/>
</signal>
<signal name="22">
<contactref element="MOD1" pad="22/A8"/>
<contactref element="J1B" pad="5"/>
</signal>
<signal name="23">
<contactref element="MOD1" pad="23/A9"/>
<contactref element="J1B" pad="4"/>
</signal>
<signal name="3V3">
<contactref element="MOD1" pad="3.3V"/>
<contactref element="J1B" pad="3"/>
</signal>
<signal name="AGND">
<contactref element="MOD1" pad="AGND"/>
<contactref element="J1B" pad="2"/>
<contactref element="MOD2" pad="AGND"/>
</signal>
<signal name="VIN">
<contactref element="MOD1" pad="VIN"/>
<contactref element="J1B" pad="1"/>
<contactref element="MOD2" pad="VIN"/>
</signal>
<signal name="GND">
<contactref element="MOD1" pad="GND"/>
<contactref element="J1A" pad="1"/>
<contactref element="MOD2" pad="GND"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="MOD2" pad="3.3V"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
