<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="53.34" y1="83.947" x2="53.34" y2="2.54" width="0" layer="20"/>
<text>Reflow Château</text>
<text>willfj.com</text>
<wire x1="0" y1="3.81" x2="0" y2="8.89" width="0" layer="20"/>
<wire x1="0" y1="8.89" x2="0" y2="83.82" width="0" layer="20"/>
<hole x="39.37" y="4.445" drill="2.8448"/>
<wire x1="50.8" y1="0" x2="3.81" y2="0" width="0" layer="20"/>
<wire x1="3.81" y1="0" x2="0" y2="3.81" width="0" layer="20" curve="-88.430313"/>
<hole x="13.97" y="83.82" drill="2.8448"/>
<wire x1="0" y1="3.81" x2="0" y2="8.89" width="0" layer="20" curve="-1.569649"/>
<wire x1="0" y1="83.82" x2="4.445" y2="88.265" width="0" layer="20" curve="-90"/>
<hole x="39.37" y="83.82" drill="2.8448"/>
<wire x1="48.895" y1="88.265" x2="53.34" y2="83.82" width="0" layer="20" curve="-90"/>
<wire x1="4.445" y1="88.265" x2="48.895" y2="88.265" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="53.34" y2="2.54" width="0" layer="20" curve="90"/>
<hole x="13.97" y="4.445" drill="2.8448"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="RELAY-S108T02">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="F-J">
<packages>
<package name="RAC04">
</package>
<package name="F-J_LOGO">
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="CAPACITIVE_TOUCH">
</package>
<package name="SCREWTERMINAL-5.08MM-4">
</package>
<package name="TEENSY_3.1">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SO08">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U4" library="SparkFun" package="RELAY-S108T02" value="S108T02"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="470">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="150">
<attribute name="VALUE"/>
</element>
<element name="U5" library="SparkFun" package="RELAY-S108T02" value="S108T02"/>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="470">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="150">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="VALUE"/>
</element>
<element name="U2" library="F-J" package="RAC04" value="RAC04"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT3904">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT3904">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-00809"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-09910"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-09910"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="F-J" package="F-J_LOGO" value="FRAME"/>
<element name="JP2" library="F-J" package="SCREWTERMINAL-3.5MM-2_LOCK" value="3.5MM">
<attribute name="VALUE"/>
</element>
<element name="U6" library="F-J" package="CAPACITIVE_TOUCH" value="CAPACITIVE_TOUCH"/>
<element name="U3" library="adafruit" package="SO08" value="MAX6675">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="F-J" package="SCREWTERMINAL-5.08MM-4" value="5.08MM"/>
<element name="U1" library="F-J" package="TEENSY_3.1" value="TEENSY_3.1"/>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="U2" pad="-DC_OUT"/>
<contactref element="U6" pad="GND@2"/>
<contactref element="U6" pad="GND@1"/>
<contactref element="U6" pad="GND"/>
<contactref element="U3" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="GND"/>
</signal>
<signal name="5V">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
<contactref element="LED3" pad="A"/>
<contactref element="R6" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="+DC_OUT"/>
<contactref element="U6" pad="5V"/>
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="COIL">
<contactref element="U4" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U4" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="COIL1">
<contactref element="U5" pad="4"/>
<contactref element="R7" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U5" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U6" pad="D12"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="NEUTRAL">
<contactref element="U2" pad="NEUTRAL"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="LIVE">
<contactref element="U2" pad="LIVE"/>
<contactref element="U4" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="TOP">
<contactref element="U4" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SCLK">
<contactref element="U6" pad="D13"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="TOP_SSR">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="BOT_SSR">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="BOT">
<contactref element="U5" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="THERM_CS">
<contactref element="U3" pad="6"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U6" pad="SCL"/>
<contactref element="U1" pad="19/A5"/>
</signal>
<signal name="SDA">
<contactref element="U6" pad="SDA"/>
<contactref element="U1" pad="18/A4"/>
</signal>
<signal name="MOSI">
<contactref element="U6" pad="D11"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="TFT_DC">
<contactref element="U6" pad="D9"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="TFT_CS">
<contactref element="U6" pad="D10"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="3.3V">
<contactref element="U3" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="3.3V"/>
</signal>
<signal name="N$1">
<contactref element="U3" pad="3"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="U1" pad="AGND"/>
</signal>
<signal name="VBAT">
</signal>
<signal name="THERM_SCLK">
<contactref element="U3" pad="5"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="THERM_MISO">
<contactref element="U3" pad="7"/>
<contactref element="U1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
