<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="23.2575" y1="12.9075" x2="66.59" y2="12.9075" width="0" layer="20"/>
<wire x1="66.59" y1="12.9075" x2="66.59" y2="46.345" width="0" layer="20"/>
<wire x1="66.59" y1="46.345" x2="23.2575" y2="46.345" width="0" layer="20"/>
<wire x1="23.2575" y1="46.345" x2="23.2575" y2="12.9075" width="0" layer="20"/>
<hole x="25.9" y="43.3" drill="2.8"/>
<hole x="51.4" y="18.1" drill="2.8"/>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>LED driver
board</text>
<text>VCC</text>
<text>GND</text>
<text>ATtiny85</text>
<text>platis.solutions</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="DIP08" value="TINY85-20-DIP">
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="LED0" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value="">
<attribute name="VALUE"/>
</element>
<element name="PWR" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.3" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.3" value="">
<attribute name="VALUE"/>
</element>
<element name="DATA" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
</elements>
<signals>
<signal name="N$1">
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="LED4" pad="2"/>
<contactref element="PWR" pad="2"/>
<contactref element="LED0" pad="2"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q4" pad="3"/>
<contactref element="PWR" pad="1"/>
</signal>
<signal name="LED0">
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="P$2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="LED0-GND">
<contactref element="Q1" pad="1"/>
<contactref element="LED0" pad="1"/>
</signal>
<signal name="LED1">
<contactref element="R2" pad="P$1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="P$2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="LED1-GND">
<contactref element="Q2" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="LED4">
<contactref element="R3" pad="P$1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="P$2"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="LED4-GND">
<contactref element="Q3" pad="1"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="LED3">
<contactref element="R4" pad="P$1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="P$2"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="LED3-GND">
<contactref element="Q4" pad="1"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="DATA-IN">
<contactref element="DATA" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="DATA" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
