<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="22.352" y1="0" x2="73.33" y2="0" width="0" layer="20"/>
<wire x1="73.33" y1="0" x2="73.33" y2="40.884" width="0" layer="20"/>
<wire x1="73.33" y1="40.884" x2="22.352" y2="40.884" width="0" layer="20"/>
<wire x1="22.352" y1="40.884" x2="22.352" y2="0" width="0" layer="20"/>
<text>270</text>
<text>RX</text>
<text>-</text>
<text>+</text>
<text>ICSP</text>
</plain>
<libraries>
<library name="Daniel">
<packages>
<package name="ATTINY85-20PU">
</package>
<package name="TRIMPOT-3386P">
</package>
<package name="16X2_LCD">
</package>
<package name="SN74HC595N">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="Daniel" package="ATTINY85-20PU" value=""/>
<element name="R1" library="Daniel" package="TRIMPOT-3386P" value=""/>
<element name="U$1" library="Daniel" package="16X2_LCD" value=""/>
<element name="U1" library="Daniel" package="SN74HC595N" value=""/>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222"/>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="V0"/>
<contactref element="R1" pad="P2"/>
</signal>
<signal name="N$2">
<contactref element="T1" pad="B"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="T1" pad="C"/>
<contactref element="U$1" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="QC"/>
<contactref element="U$1" pad="D6"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="D5"/>
<contactref element="U1" pad="QD"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="QE"/>
<contactref element="U$1" pad="D4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="D7"/>
<contactref element="U1" pad="QB"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="QF"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="A"/>
<contactref element="U$1" pad="VDD"/>
<contactref element="R1" pad="P1"/>
<contactref element="U1" pad="VCC"/>
<contactref element="U2" pad="VCC"/>
<contactref element="U1" pad="SRCLR"/>
<contactref element="J1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="T1" pad="E"/>
<contactref element="U$1" pad="VSS"/>
<contactref element="U$1" pad="RW"/>
<contactref element="R1" pad="P3"/>
<contactref element="U1" pad="GND"/>
<contactref element="U2" pad="GND"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="OE"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="D3"/>
<contactref element="U$1" pad="D0"/>
<contactref element="U$1" pad="D1"/>
<contactref element="U$1" pad="D2"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="QH"/>
<contactref element="U$1" pad="RS"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="E"/>
<contactref element="U1" pad="QA"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="SER"/>
<contactref element="U2" pad="PB0"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="PB1"/>
<contactref element="U1" pad="RCLK"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="SRCLK"/>
<contactref element="U2" pad="PB2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="PB5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="PB3"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
