<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="6.35" x2="0" y2="54.61" width="0.254" layer="20"/>
<wire x1="0" y1="54.61" x2="6.35" y2="60.96" width="0.254" layer="20" curve="-90"/>
<wire x1="6.35" y1="60.96" x2="54.61" y2="60.96" width="0.254" layer="20"/>
<wire x1="54.61" y1="60.96" x2="60.96" y2="54.61" width="0.254" layer="20" curve="-90"/>
<wire x1="6.35" y1="0" x2="54.61" y2="0" width="0.254" layer="20"/>
<wire x1="54.61" y1="0" x2="60.96" y2="6.35" width="0.254" layer="20" curve="90"/>
<wire x1="60.96" y1="6.35" x2="60.96" y2="54.61" width="0.254" layer="20"/>
<wire x1="0" y1="6.35" x2="6.35" y2="0" width="0.254" layer="20" curve="90"/>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>CD</text>
<text>DRV</text>
<text>DRV</text>
<text>PSEL</text>
<hole x="56" y="48" drill="4.8"/>
<hole x="16" y="48" drill="4.8"/>
<hole x="56" y="8" drill="4.8"/>
<hole x="16" y="8" drill="4.8"/>
<text>S</text>
<text>D</text>
<text>G</text>
<text>S</text>
<text>D</text>
<text>ENABLE</text>
<text>BATT</text>
<text>G</text>
</plain>
<libraries>
<library name="32bits">
<packages>
<package name="RGE24_2P7X2P7">
</package>
<package name="PERIODIC_SYMBOL_BACK">
</package>
<package name="20M1">
</package>
<package name="VQFN7">
</package>
<package name="SO-8">
</package>
<package name="DR73">
</package>
<package name="1206">
</package>
<package name="RASM722">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;h3&gt;USB Type Mini-B Surface Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5 main, 4 shield pins&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/miniUSB-Dimensional.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Mini-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X6">
<description>&lt;h3&gt;Plated Through Hole - 2x6&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="AVX_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/04/2012 16:26:10</description>
<packages>
<package name="CAPC1608X94N">
</package>
<package name="CAPC2013X140N">
</package>
<package name="CAPC1005X60N">
</package>
<package name="CAPC3216X127N">
</package>
<package name="CAPC1608X90N">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Bourns_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:04:24</description>
<packages>
<package name="INDC3225X22N">
</package>
</packages>
</library>
<library name="Kemet_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 28/03/2012 12:54:09</description>
<packages>
<package name="CAPC1005X60N">
</package>
<package name="CAPC1608X85N">
</package>
</packages>
</library>
<library name="Vishay_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 16:36:08</description>
<packages>
<package name="RESC1005X40N">
</package>
<package name="RESC1608X60N">
</package>
</packages>
</library>
<library name="Murata_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 21/03/2012 17:47:01</description>
<packages>
<package name="CAPC2013X135N">
</package>
<package name="CAPC3225X270N">
</package>
</packages>
</library>
<library name="Dialight_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 13/06/2012 13:59:22</description>
<packages>
<package name="LED_597-3311-407F">
</package>
<package name="LED_597-3111-407F">
</package>
</packages>
</library>
<library name="Panasonic_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 15:23:17</description>
<packages>
<package name="RESC2013X65N">
<description>RESISTOR, 0805</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U9" library="32bits" package="RGE24_2P7X2P7" value="BQ24168RGET">
<attribute name="MANUFACTURER_PART_NUMBER" value="bq24168rget"/>
<attribute name="VENDOR" value="Texas Instruments"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="USB-MINIB" value="USB_MINI-B_SMT">
<attribute name="PROD_ID" value="CONN-08193"/>
<attribute name="SF_ID" value="PRT-00587"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="2X3" value="ISP">
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
<attribute name="VALUE" value="FEMALE 2x3"/>
</element>
<element name="5" library="32bits" package="PERIODIC_SYMBOL_BACK" value="rev.3">
<attribute name="ELEMENT" value="B"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="out">
<attribute name="VALUE"/>
</element>
<element name="C1" library="AVX_By_element14_Batch_1" package="CAPC1608X94N" value="1uF">
<attribute name="MPN" value="06033D105KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1658868"/>
<attribute name="OC_NEWARK" value="96M1265"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="25V"/>
</element>
<element name="U9_C2" library="AVX_By_element14_Batch_1" package="CAPC2013X140N" value="4.7uF">
<attribute name="MPN" value="08053D475KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1657932"/>
<attribute name="OC_NEWARK" value="27M3797"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="25V"/>
</element>
<element name="U3" library="32bits" package="20M1" value="ATTINY84-20MU">
<attribute name="MANUFACTURER_PART_NUMBER" value="ATTINY8420MU"/>
<attribute name="VENDOR" value="Atmel"/>
</element>
<element name="U2_R1" library="SparkFun-Resistors" package="0402" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U2_C2" library="AVX_By_element14_Batch_1" package="CAPC1005X60N" value="2.2uF">
<attribute name="MPN" value="0402ZD225KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1867952"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="10V"/>
</element>
<element name="U6" library="32bits" package="VQFN7" value="TPS61230A"/>
<element name="L2" library="Bourns_By_element14_Batch_1" package="INDC3225X22N" value="1.0 uH">
<attribute name="MPN" value="PM1210-1R0J-RC"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1180462"/>
<attribute name="OC_NEWARK" value="63K3090"/>
<attribute name="SUPPLIER" value="BOURNS"/>
<attribute name="TOLERANCE" value="±5 %"/>
</element>
<element name="U6_CBST" library="Kemet_By_element14_Batch_1" package="CAPC1005X60N" value="10 nF">
<attribute name="MPN" value="C0402C103K5RACTU"/>
<attribute name="OC_FARNELL" value="1414575"/>
<attribute name="OC_NEWARK" value="78H4783"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
</element>
<element name="U6_RFBT" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="316K Ohms">
<attribute name="MPN" value="CRCW0402316KFKED"/>
<attribute name="OC_FARNELL" value="1652782"/>
<attribute name="OC_NEWARK" value="52K6969"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="U6_RFBB" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="U6_CFF" library="Kemet_By_element14_Batch_1" package="CAPC1608X85N" value="10pF">
<attribute name="MPN" value="C0603C100J5GACTU"/>
<attribute name="OC_FARNELL" value="1414601"/>
<attribute name="OC_NEWARK" value="64K2831"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="VOLTAGERATING" value="50V"/>
</element>
<element name="U6_CIN" library="Murata_By_element14_Batch_1" package="CAPC2013X135N" value="22uF">
<attribute name="MPN" value="GRM21BR60J226ME39L "/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1735531"/>
<attribute name="OC_NEWARK" value="24R6338"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VOLTAGERATING" value="6.3V"/>
</element>
<element name="U6_COUT" library="Murata_By_element14_Batch_1" package="CAPC3225X270N" value="22uF">
<attribute name="MPN" value="GRM32ER61C226KE20L"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9527800"/>
<attribute name="OC_NEWARK" value="97K0673"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="16V"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="JST-2-SMD" value="batt">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="AVX_By_element14_Batch_1" package="CAPC1608X94N" value="1uF">
<attribute name="MPN" value="06033D105KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1658868"/>
<attribute name="OC_NEWARK" value="96M1265"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="25V"/>
</element>
<element name="Q1" library="32bits" package="SO-8" value="Si7137DP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9_C4" library="AVX_By_element14_Batch_1" package="CAPC3216X127N" value="47uF">
<attribute name="MPN" value="12067C332KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="89C3187"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="500V"/>
</element>
<element name="U9_C5" library="AVX_By_element14_Batch_1" package="CAPC1608X90N" value="10nF">
<attribute name="MPN" value="06035C103KAZ2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="7569548"/>
<attribute name="OC_NEWARK" value="10R5936"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
</element>
<element name="U9_L1" library="32bits" package="DR73" value="DR73-2R2-R">
<attribute name="MANUFACTURER_PART_NUMBER" value="DR732R2R"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Cooper Bussmann"/>
</element>
<element name="U9_C6" library="AVX_By_element14_Batch_1" package="CAPC2013X140N" value="4.7uF">
<attribute name="MPN" value="08053D475KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1657932"/>
<attribute name="OC_NEWARK" value="27M3797"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="25V"/>
</element>
<element name="C7" library="AVX_By_element14_Batch_1" package="CAPC1608X94N" value="1uF">
<attribute name="MPN" value="06033D105KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1658868"/>
<attribute name="OC_NEWARK" value="96M1265"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="25V"/>
</element>
<element name="C8" library="AVX_By_element14_Batch_1" package="CAPC1608X94N" value="1uF">
<attribute name="MPN" value="06033D105KAT2A"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1658868"/>
<attribute name="OC_NEWARK" value="96M1265"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="25V"/>
</element>
<element name="U2_R9" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="MPN" value="CRCW0402100KJNED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1652738"/>
<attribute name="OC_NEWARK" value="59M6699"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="U2_R2" library="SparkFun-Resistors" package="0402" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U2_L1" library="SparkFun-Resistors" package="0402" value="1 kOhm @ 100MHz">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U2_L2" library="SparkFun-Resistors" package="0402" value="1 kOhm @ 100MHz">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="J14" library="SparkFun-Connectors" package="2X6" value="debug">
<attribute name="PROD_ID" value="CONN-12423"/>
<attribute name="VALUE" value="2X6 FEMALE"/>
</element>
<element name="5V" library="Dialight_By_element14_Batch_1" package="LED_597-3311-407F" value="QTLP650C-4">
<attribute name="COLOR" value="Green"/>
<attribute name="MPN" value="597-3311-407F"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1519493"/>
<attribute name="OC_NEWARK" value="30K4957"/>
<attribute name="PACKAGE" value="1206- Green LED"/>
<attribute name="SUPPLIER" value="Dialight"/>
</element>
<element name="CHG" library="Dialight_By_element14_Batch_1" package="LED_597-3111-407F" value="QTLP650C-7">
<attribute name="COLOR" value="AlGaAs Red"/>
<attribute name="MPN" value="597-3111-407F"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1519490"/>
<attribute name="OC_NEWARK" value="30K4900"/>
<attribute name="PACKAGE" value="1206-RED LED"/>
<attribute name="SUPPLIER" value="Dialight"/>
</element>
<element name="USB" library="Dialight_By_element14_Batch_1" package="LED_597-3311-407F" value="QTLP650C-4">
<attribute name="COLOR" value="Green"/>
<attribute name="MPN" value="597-3311-407F"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1519493"/>
<attribute name="OC_NEWARK" value="30K4957"/>
<attribute name="PACKAGE" value="1206- Green LED"/>
<attribute name="SUPPLIER" value="Dialight"/>
</element>
<element name="R1" library="Panasonic_By_element14_Batch_1" package="RESC2013X65N" value="150 Ohm">
<attribute name="MPN" value="ERA-6AEB151V"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1811409"/>
<attribute name="OC_NEWARK" value="08N2149"/>
<attribute name="SUPPLIER" value="Panasonic"/>
<attribute name="TOLERANCE" value="±0.1 %"/>
<attribute name="WATTAGE" value="0.125 W"/>
</element>
<element name="R3" library="Panasonic_By_element14_Batch_1" package="RESC2013X65N" value="150 Ohm">
<attribute name="MPN" value="ERA-6AEB151V"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1811409"/>
<attribute name="OC_NEWARK" value="08N2149"/>
<attribute name="SUPPLIER" value="Panasonic"/>
<attribute name="TOLERANCE" value="±0.1 %"/>
<attribute name="WATTAGE" value="0.125 W"/>
</element>
<element name="R5" library="Panasonic_By_element14_Batch_1" package="RESC2013X65N" value="150 Ohm">
<attribute name="MPN" value="ERA-6AEB151V"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1811409"/>
<attribute name="OC_NEWARK" value="08N2149"/>
<attribute name="SUPPLIER" value="Panasonic"/>
<attribute name="TOLERANCE" value="±0.1 %"/>
<attribute name="WATTAGE" value="0.125 W"/>
</element>
<element name="R9" library="32bits" package="1206" value="10K NTC">
<attribute name="NAME"/>
</element>
<element name="RLO" library="Vishay_By_element14_Batch_1" package="RESC1608X60N" value="11.6K">
<attribute name="MPN" value="CRCW060311K0FKEA"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1570716"/>
<attribute name="OC_NEWARK" value="89M6730"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.1 W"/>
</element>
<element name="RHI" library="Vishay_By_element14_Batch_1" package="RESC1608X60N" value="5.5K">
<attribute name="MPN" value="CRCW060311K0FKEA"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1570716"/>
<attribute name="OC_NEWARK" value="89M6730"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.1 W"/>
</element>
<element name="J13" library="32bits" package="RASM722" value="RASM722"/>
<element name="R2" library="Vishay_By_element14_Batch_1" package="RESC1608X60N" value="1M Ohm">
<attribute name="MPN" value="CRCW06031M00JNEA"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1514706"/>
<attribute name="OC_NEWARK" value="59M6756"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="WATTAGE" value="0.1 W"/>
</element>
<element name="R4" library="Vishay_By_element14_Batch_1" package="RESC1608X60N" value="1M Ohm">
<attribute name="MPN" value="CRCW06031M00JNEA"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1514706"/>
<attribute name="OC_NEWARK" value="59M6756"/>
<attribute name="SUPPLIER" value="VISHAY DALE ELECTRONICS"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="WATTAGE" value="0.1 W"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X04" value="drv">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J16" library="SparkFun-Connectors" package="1X04" value="5V">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="NOTIFY" library="Dialight_By_element14_Batch_1" package="LED_597-3311-407F" value="QTLP650C-4">
<attribute name="COLOR" value="Green"/>
<attribute name="MPN" value="597-3311-407F"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1519493"/>
<attribute name="OC_NEWARK" value="30K4957"/>
<attribute name="PACKAGE" value="1206- Green LED"/>
<attribute name="SUPPLIER" value="Dialight"/>
</element>
<element name="R6" library="Panasonic_By_element14_Batch_1" package="RESC2013X65N" value="150 Ohm">
<attribute name="MPN" value="ERA-6AEB151V"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1811409"/>
<attribute name="OC_NEWARK" value="08N2149"/>
<attribute name="SUPPLIER" value="Panasonic"/>
<attribute name="TOLERANCE" value="±0.1 %"/>
<attribute name="WATTAGE" value="0.125 W"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J10" pad="GND"/>
<contactref element="U3" pad="8"/>
<contactref element="U2_C2" pad="1"/>
<contactref element="U6" pad="P$6"/>
<contactref element="U6_RFBB" pad="2"/>
<contactref element="U6_CIN" pad="1"/>
<contactref element="U6_COUT" pad="1"/>
<contactref element="U9_C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="U9" pad="15"/>
<contactref element="U9" pad="17"/>
<contactref element="U9_C4" pad="1"/>
<contactref element="U9" pad="16"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="U9" pad="25"/>
<contactref element="U9" pad="5"/>
<contactref element="U9_C6" pad="2"/>
<contactref element="J12" pad="P2"/>
<contactref element="J4" pad="6"/>
<contactref element="J14" pad="2"/>
<contactref element="5V" pad="1"/>
<contactref element="USB" pad="1"/>
<contactref element="J14" pad="10"/>
<contactref element="J14" pad="6"/>
<contactref element="R9" pad="1"/>
<contactref element="RLO" pad="2"/>
<contactref element="J13" pad="SLEEVE"/>
<contactref element="J11" pad="4"/>
<contactref element="J16" pad="4"/>
<contactref element="U3" pad="21"/>
<contactref element="NOTIFY" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="U9" pad="12"/>
<contactref element="U9" pad="11"/>
<contactref element="C3" pad="1"/>
<contactref element="J14" pad="12"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="P$5"/>
<contactref element="Q1" pad="P$6"/>
<contactref element="Q1" pad="P$7"/>
<contactref element="Q1" pad="P$9"/>
<contactref element="Q1" pad="P$8"/>
</signal>
<signal name="SYS_5V">
<contactref element="U3" pad="9"/>
<contactref element="U2_C2" pad="2"/>
<contactref element="U6" pad="P$7"/>
<contactref element="U6_RFBT" pad="1"/>
<contactref element="U6_CFF" pad="2"/>
<contactref element="U6_COUT" pad="2"/>
<contactref element="U2_R9" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="J12" pad="P1"/>
<contactref element="R1" pad="2"/>
<contactref element="U2_R1" pad="1"/>
<contactref element="U2_R2" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="!RESET">
<contactref element="U3" pad="13"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="U3_PA6">
<contactref element="U2_L1" pad="1"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="MISO">
<contactref element="U3" pad="20"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="L2" pad="2"/>
<contactref element="U6" pad="P$4"/>
<contactref element="U6" pad="P$2"/>
<contactref element="U6_CIN" pad="2"/>
<contactref element="J16" pad="2"/>
<contactref element="J16" pad="3"/>
</signal>
<signal name="U6_CBST">
<contactref element="U6" pad="P$1"/>
<contactref element="U6_CBST" pad="1"/>
</signal>
<signal name="U6_SW">
<contactref element="U6_CBST" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="U6" pad="P$5"/>
</signal>
<signal name="U6_FB">
<contactref element="U6" pad="P$3"/>
<contactref element="U6_RFBT" pad="2"/>
<contactref element="U6_RFBB" pad="1"/>
<contactref element="U6_CFF" pad="1"/>
</signal>
<signal name="U9_PMIDI">
<contactref element="U9" pad="20"/>
<contactref element="U9_C2" pad="1"/>
</signal>
<signal name="U9_BGATE">
<contactref element="Q1" pad="P$4"/>
<contactref element="U9" pad="10"/>
</signal>
<signal name="U9_SYS">
<contactref element="U9" pad="13"/>
<contactref element="U9" pad="14"/>
<contactref element="U9_C4" pad="2"/>
<contactref element="U9_L1" pad="2"/>
<contactref element="J16" pad="1"/>
<contactref element="Q1" pad="P$1"/>
<contactref element="Q1" pad="P$3"/>
<contactref element="Q1" pad="P$2"/>
</signal>
<signal name="U9_SW">
<contactref element="U9" pad="18"/>
<contactref element="U9_C5" pad="2"/>
<contactref element="U9_L1" pad="1"/>
</signal>
<signal name="U9_BOOT">
<contactref element="U9" pad="19"/>
<contactref element="U9_C5" pad="1"/>
</signal>
<signal name="U9_PMIDU">
<contactref element="U9" pad="23"/>
<contactref element="U9_C6" pad="1"/>
</signal>
<signal name="U9_USB">
<contactref element="U9" pad="22"/>
<contactref element="J10" pad="VBUS"/>
<contactref element="C7" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="U9_STAT">
<contactref element="U9" pad="8"/>
<contactref element="CHG" pad="1"/>
</signal>
<signal name="U9_SCL">
<contactref element="U9" pad="3"/>
<contactref element="U2_L2" pad="1"/>
<contactref element="U2_R2" pad="2"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="U9_SDA">
<contactref element="U9" pad="4"/>
<contactref element="U2_L1" pad="2"/>
<contactref element="U2_R1" pad="2"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="U9_CD">
<contactref element="U9" pad="24"/>
<contactref element="J14" pad="1"/>
</signal>
<signal name="U9_IN">
<contactref element="U9" pad="21"/>
<contactref element="C1" pad="1"/>
<contactref element="J13" pad="TIP"/>
</signal>
<signal name="U9_INT">
<contactref element="U9" pad="7"/>
<contactref element="U3" pad="2"/>
<contactref element="U2_R9" pad="2"/>
</signal>
<signal name="VBAT_CON">
<contactref element="J1" pad="2"/>
<contactref element="J14" pad="11"/>
</signal>
<signal name="U3_PA4">
<contactref element="U2_L2" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="U9_PSEL">
<contactref element="U9" pad="2"/>
<contactref element="J14" pad="9"/>
</signal>
<signal name="LA_5">
<contactref element="5V" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="LA_CHG">
<contactref element="CHG" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="LA_USB">
<contactref element="USB" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="U9_TS">
<contactref element="U9" pad="9"/>
<contactref element="R9" pad="2"/>
<contactref element="RHI" pad="2"/>
<contactref element="RLO" pad="1"/>
</signal>
<signal name="GNDBREAK">
<contactref element="J13" pad="SHUNT"/>
</signal>
<signal name="ADC0">
<contactref element="U3" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="ADC2">
<contactref element="U3" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="U9_DRV">
<contactref element="C8" pad="2"/>
<contactref element="J11" pad="1"/>
<contactref element="J14" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="J14" pad="7"/>
<contactref element="RHI" pad="1"/>
</signal>
<signal name="U9_DRV_0">
<contactref element="U9" pad="6"/>
<contactref element="J11" pad="2"/>
<contactref element="J11" pad="3"/>
</signal>
<signal name="LA_1">
<contactref element="NOTIFY" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="1ROU">
<contactref element="U3" pad="15"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
