<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="36.754" y2="0" width="0" layer="20"/>
<wire x1="36.754" y1="0" x2="36.754" y2="26.67" width="0" layer="20"/>
<wire x1="36.754" y1="26.67" x2="1.27" y2="26.67" width="0" layer="20"/>
<wire x1="1.27" y1="26.67" x2="1.27" y2="0" width="0" layer="20"/>
<text>12VDC</text>
<text>GND</text>
<text>GND</text>
<text>Source</text>
<text>Load</text>
<text>12VDC</text>
<text>LED Terminal</text>
<text>R1 (or Jumper)</text>
<text>GND</text>
<text>GND</text>
<text>Switch Adapter</text>
<text>12VDC</text>
<text>12VDC</text>
<text>1oz=4A 28VDC Max
2oz=8A 28VDC Max</text>
<text>1-15-21</text>
<text>SWINT-2A</text>
</plain>
<libraries>
<library name="a-lib">
<description>Archive Library (for old designs) - do not use for new components.</description>
<packages>
<package name="SMTWIREPAD_SMALL">
<description>Pad Size: 0.15"x0.75"</description>
</package>
<package name="BOURNS3306_K_W">
<description>&lt;b&gt;PC Mount Trimmer Potentiometer&lt;/b&gt;

&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/54/3306-8834.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="KEYSTONE3578">
</package>
<package name="KEYSTONE_4910">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
<element name="TB1" library="a-lib_Connectors" package="KEYSTONE3578" value=""/>
<element name="TB2" library="a-lib_Connectors" package="KEYSTONE3578" value=""/>
<element name="TB3" library="a-lib_Connectors" package="KEYSTONE3578" value=""/>
<element name="JP6" library="a-lib" package="SMTWIREPAD_SMALL" value=""/>
<element name="JP5" library="a-lib" package="SMTWIREPAD_SMALL" value=""/>
<element name="TB4" library="a-lib_Connectors" package="KEYSTONE_4910" value="">
<attribute name="TABSIZE" value=".250"/>
</element>
<element name="TB5" library="a-lib_Connectors" package="KEYSTONE_4910" value="">
<attribute name="TABSIZE" value=".250"/>
</element>
<element name="TB6" library="a-lib_Connectors" package="KEYSTONE_4910" value="">
<attribute name="TABSIZE" value=".250"/>
</element>
<element name="TB7" library="a-lib_Connectors" package="KEYSTONE_4910" value="">
<attribute name="TABSIZE" value=".250"/>
</element>
<element name="R1" library="a-lib" package="BOURNS3306_K_W" value="10K">
<attribute name="MARKING" value="103"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP6" pad="P$1"/>
<contactref element="TB6" pad="T3"/>
<contactref element="TB6" pad="T1"/>
<contactref element="TB6" pad="T2"/>
<contactref element="TB5" pad="T3"/>
<contactref element="TB5" pad="T1"/>
<contactref element="TB5" pad="T2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="TB2" pad="P$1"/>
<contactref element="TB2" pad="P$2"/>
<contactref element="TB4" pad="T3"/>
<contactref element="TB4" pad="T1"/>
<contactref element="TB4" pad="T2"/>
</signal>
<signal name="N$3">
<contactref element="TB3" pad="P$1"/>
<contactref element="TB3" pad="P$2"/>
<contactref element="TB7" pad="T3"/>
<contactref element="TB7" pad="T1"/>
<contactref element="TB7" pad="T2"/>
</signal>
<signal name="N$1">
<contactref element="TB1" pad="P$1"/>
<contactref element="TB1" pad="P$2"/>
<contactref element="JP5" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="R1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
