<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="0" x2="20.574" y2="0" width="0" layer="20"/>
<wire x1="20.574" y1="0" x2="20.574" y2="23.368" width="0" layer="20"/>
<wire x1="20.574" y1="23.368" x2="-0.254" y2="23.358" width="0" layer="20"/>
<wire x1="-0.254" y1="23.358" x2="-0.254" y2="0" width="0" layer="20"/>
<text>PAN13XX Breakout V0.1
BLE/SPP
Idle Hands Dev.
idlehandsdevelopment.com</text>
<text>MLDO_IN
CL1.5_LDO_IN
VDD_IO
MLDO_OUT
SLW_CLK_IN
NSHUTD
RF
TX_DBG
GND</text>
<text>AUD_CLK
AUD_IN
AUD_OUT
AUD_FSYNC
HCI_CTS
HCI_RTS
HCI_RX
HCI_TX
GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09_LOCK">
</package>
</packages>
</library>
<library name="BluetoothBLE_SPP">
<description>BlueRadios Module Footprints</description>
<packages>
<package name="PAN13XX">
<description>Footprint for the PAN13XX Series Bluetooth Modules 
https://pideu.panasonic.de/products/wireless-modules/bluetooth/bluetooth-40-dual-mode/pan131626-nowith-antenna-hci-smart-ready-EN.html#tab3</description>
</package>
</packages>
</library>
<library name="IdleHandsProject">
<packages>
<package name="IHD-LOGO-L">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="U$1" library="BluetoothBLE_SPP" package="PAN13XX" value="PAN132X"/>
<element name="LOGO1" library="IdleHandsProject" package="IHD-LOGO-L" value="IDLEHANDS_LOGOL"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="P1"/>
<contactref element="U$1" pad="P12"/>
<contactref element="U$1" pad="P14"/>
<contactref element="U$1" pad="P20"/>
<contactref element="U$1" pad="PA"/>
<contactref element="U$1" pad="PB"/>
<contactref element="U$1" pad="PC"/>
<contactref element="U$1" pad="PD"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="MLDO_IN">
<contactref element="U$1" pad="P15"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="CL1.5_LDO_IN">
<contactref element="U$1" pad="P11"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VDD_IO">
<contactref element="U$1" pad="P22"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="MLDO_OUT">
<contactref element="U$1" pad="P10"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SLW_CLK_IN">
<contactref element="U$1" pad="P8"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RF">
<contactref element="U$1" pad="P13"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="NSHUTD">
<contactref element="U$1" pad="P16"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="AUD_CLK">
<contactref element="U$1" pad="P19"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="AUD_OUT">
<contactref element="U$1" pad="P17"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="AUD_IN">
<contactref element="U$1" pad="P18"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="AUD_FSYNC">
<contactref element="U$1" pad="P7"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="TX_DBG">
<contactref element="U$1" pad="P2"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="HCI_CTS">
<contactref element="U$1" pad="P3"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="HCI_RTS">
<contactref element="U$1" pad="P4"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="HCI_RX">
<contactref element="U$1" pad="P5"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="HCI_TX">
<contactref element="U$1" pad="P6"/>
<contactref element="JP2" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
