<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="9.000875" y1="18.999940625" x2="9" y2="0" width="0" layer="20"/>
<wire x1="9" y1="0" x2="26.5" y2="0" width="0" layer="20"/>
<wire x1="26.5" y1="0" x2="26.5" y2="19" width="0" layer="20"/>
<wire x1="26.5" y1="19" x2="9" y2="19" width="0" layer="20"/>
<text>Designed by</text>
<text>Andrzej Szczepaniak</text>
<text>LittleWire ISP</text>
<text>Programmer</text>
<text>DigiSpark
</text>
<text>Shield</text>
<text>OSHW</text>
<text>http://www.develdsoft.com/</text>
<text>Prototype</text>
<text>Prototype</text>
<text>Not For</text>
<text>Mass Production</text>
<text>Version A</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOCKET-08">
<description>&lt;b&gt;Dual In Line Socket&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="amd">
<packages>
<package name="AVRISP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="SparkFun" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="ic-package" package="SOCKET-08" value="">
<attribute name="VALUE"/>
</element>
<element name="ISP1" library="amd" package="AVRISP" value="AVRISP-6"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="ISP1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="JP2" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="ISP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP3" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="2"/>
<contactref element="IC2" pad="6"/>
<contactref element="ISP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP3" pad="6"/>
<contactref element="IC2" pad="1"/>
<contactref element="ISP1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="JP3" pad="3"/>
<contactref element="IC2" pad="7"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
