<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="42.85" y2="0" width="0" layer="20"/>
<wire x1="42.85" y1="0" x2="42.85" y2="20.31" width="0" layer="20"/>
<wire x1="42.85" y1="20.31" x2="11.43" y2="20.31" width="0" layer="20"/>
<wire x1="11.43" y1="20.31" x2="11.43" y2="12.7" width="0" layer="20"/>
<wire x1="11.43" y1="12.7" x2="0" y2="12.7" width="0" layer="20"/>
<wire x1="0" y1="12.7" x2="0" y2="0" width="0" layer="20"/>
<text>HV Rescue 84</text>
<text>KO4XL Aug'15</text>
<text>Rev 2</text>
<text>ATTINYx4-SU</text>
<text>(IN ADAPTER)</text>
</plain>
<libraries>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X533-8">
</package>
<package name="DIP254P762X533-14">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="ATTINYx5">
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="OC_NEWARK" value="23M5072"/>
<attribute name="MPN" value="ATTINY45-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1288352"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-14" value="ATTINYx4-PU">
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="OC_NEWARK" value="58M3786"/>
<attribute name="MPN" value="ATTINY44-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1455150"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RST">
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCI">
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="14"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="12"/>
<contactref element="U2" pad="13"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="SDO">
<contactref element="U1" pad="7"/>
<contactref element="U2" pad="9"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="SII">
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="8"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="SDI">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
