<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="-8.1" y1="0.4" x2="8.1" y2="0.4" width="0" layer="20"/>
<wire x1="8.1" y1="0.4" x2="8.1" y2="21.7" width="0" layer="20"/>
<wire x1="8.1" y1="21.7" x2="-8.1" y2="21.7" width="0" layer="20"/>
<wire x1="-8.1" y1="21.7" x2="-8.1" y2="0.4" width="0" layer="20"/>
<text>3.3V</text>
<text>Rev 1</text>
<text>Rev 1</text>
<text>Designed by: MrSwirlyEyes</text>
<text>Serial Programmer</text>
<text>5V</text>
<text>3.3V</text>
<text>5V</text>
</plain>
<libraries>
<library name="PiB_capacitors">
<packages>
<package name="CAPC1005X55_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.55 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.55 mm&lt;/p&gt;</description>
</package>
<package name="CAPMP2012X110">
<description>Molded Body, 2.00 X 1.25 X 1.10 mm body
&lt;p&gt;Molded Body package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_connectors">
<packages>
<package name="USB_MICRO-B_1050170001">
</package>
</packages>
</library>
<library name="PiB_ic_bridge">
<packages>
<package name="SOP65P780X200-28">
<description>28-SOP, 0.65 mm pitch, 7.80 mm span, 10.20 X 5.30 X 2.00 mm body
&lt;p&gt;28-pin SOP package with 0.65 mm pitch, 7.80 mm span with body size 10.20 X 5.30 X 2.00 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_leds">
<packages>
<package name="LEDC1005X40_LED-0402">
<description>CHIP, 1 X 0.5 X 0.4 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.4 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_resistors">
<packages>
<package name="RESC1005X35_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.35 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_switches">
<packages>
<package name="SW_SLIDE_SPDT_RA_SMD_4V_300MA_6.7L-2.6W">
</package>
</packages>
</library>
<library name="PiB_connectors">
<packages>
<package name="HDRRAR6W60P254_1X6_1574X850X274B_FTDI">
<description>Single-row, 6-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 15.74 X 8.50 X 2.74 mm body
&lt;p&gt;Single-row (1X6), 6-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) col pitch, 0.60 mm lead width, 3.15 mm tail length and 8.50 mm insulator length with body size 15.74 X 8.50 X 2.74 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_logo">
<packages>
<package name="MRSWIRLYEYES-LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="PiB_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="PiB_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="PiB_capacitors" package="CAPMP2012X110" value="10uF/6.3V">
<attribute name="DATASHEET" value="http://datasheets.avx.com/f92.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=478-8115-1-ND"/>
<attribute name="DISTPN" value="478-8115-1-ND"/>
<attribute name="MFR" value="AVX Corporation"/>
<attribute name="MPN" value="F920J106MPA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI1" library="PiB_connectors" package="HDRRAR6W60P254_1X6_1574X850X274B_FTDI" value="PTH RA FEMALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/10493.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=PPTC061LGBN-RC"/>
<attribute name="DISTPN" value="S5442-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PPTC061LGBN-RC"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="PTH RA FEMALE"/>
</element>
<element name="IC1" library="PiB_ic_bridge" package="SOP65P780X200-28" value="FT232RL">
<attribute name="DATASHEET" value="https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232R.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=768-1007-1-ND"/>
<attribute name="DISTPN" value="768-1007-1-ND"/>
<attribute name="MFR" value="FTDI, Future Technology Devices International Ltd"/>
<attribute name="MPN" value="FT232RL-REEL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX_LED" library="PiB_leds" package="LEDC1005X40_LED-0402" value="GREEN">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402GC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2205-1-ND"/>
<attribute name="DISTPN" value="492-2205-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402GC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX_LED" library="PiB_leds" package="LEDC1005X40_LED-0402" value="RED">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402RC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2208-1-ND"/>
<attribute name="DISTPN" value="492-2208-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402RC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="PiB_switches" package="SW_SLIDE_SPDT_RA_SMD_4V_300MA_6.7L-2.6W" value="300mA/4V">
<attribute name="CREATOR" value="MrSwirlyEyes"/>
<attribute name="DATASHEET" value="https://media.digikey.com/pdf/Data%20Sheets/APEM%20Components%20PDFs/MA_Series_.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=679-1847-1-ND"/>
<attribute name="DISTPN" value="679-1847-1-ND"/>
<attribute name="MFR" value="APEM Inc."/>
<attribute name="MPN" value="MA12RTR"/>
<attribute name="NAME"/>
<attribute name="TESTED" value="YES"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="PiB_connectors" package="USB_MICRO-B_1050170001" value="USB2.0 MICRO-B">
<attribute name="DATASHEET" value="https://www.molex.com/pdm_docs/sd/1050170001_sd.pdf"/>
<attribute name="DATASHEET_CABLE" value="http://www.qualtekusa.com/images/Cable%20Assemblies/PDF_2/3025031-06.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=WM1399CT-ND"/>
<attribute name="DISTLINK_CABLE" value="https://www.digikey.com/products/en?keywords=Q967-ND"/>
<attribute name="DISTPN" value="WM1399CT-ND"/>
<attribute name="DISTPN_CABLE" value="Q967-ND"/>
<attribute name="DIST_CABLE" value="Digikey"/>
<attribute name="MFR" value="Molex, LLC"/>
<attribute name="MFR_CABLE" value="Qualtek"/>
<attribute name="MPN" value="1050170001"/>
<attribute name="MPN_CABLE" value="3025031-06"/>
</element>
<element name="U$1" library="PiB_logo" package="MRSWIRLYEYES-LOGO" value=""/>
</elements>
<signals>
<signal name="D+">
<contactref element="USB1" pad="3"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="D-">
<contactref element="USB1" pad="2"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="GND">
<contactref element="USB1" pad="5"/>
<contactref element="USB1" pad="GND@0"/>
<contactref element="USB1" pad="GND@1"/>
<contactref element="USB1" pad="GND@2"/>
<contactref element="USB1" pad="GND@3"/>
<contactref element="USB1" pad="GND@4"/>
<contactref element="USB1" pad="GND@5"/>
<contactref element="USB1" pad="P$1"/>
<contactref element="USB1" pad="P$2"/>
<contactref element="C3" pad="K"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="26"/>
<contactref element="IC1" pad="25"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="21"/>
<contactref element="FTDI1" pad="GND"/>
</signal>
<signal name="5V">
<contactref element="USB1" pad="1"/>
<contactref element="IC1" pad="20"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="A"/>
<contactref element="TX_LED" pad="A"/>
<contactref element="RX_LED" pad="A"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="17"/>
<contactref element="C1" pad="1"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="TXO">
<contactref element="IC1" pad="1"/>
<contactref element="FTDI1" pad="TX"/>
</signal>
<signal name="RXI">
<contactref element="IC1" pad="5"/>
<contactref element="FTDI1" pad="RX"/>
</signal>
<signal name="CTS">
<contactref element="IC1" pad="11"/>
<contactref element="FTDI1" pad="CTS"/>
</signal>
<signal name="DTR">
<contactref element="IC1" pad="2"/>
<contactref element="FTDI1" pad="DTR"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="23"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$7">
<contactref element="TX_LED" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="RX_LED" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="FTDI1" pad="VCC"/>
<contactref element="SW1" pad="2"/>
<contactref element="IC1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
