<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="13.9575" y2="1.27" width="0.127" layer="20"/>
<wire x1="13.9575" y1="1.27" x2="13.9575" y2="11.42" width="0.127" layer="20"/>
<wire x1="13.9575" y1="11.42" x2="0" y2="11.42" width="0.127" layer="20"/>
<wire x1="0" y1="11.42" x2="0" y2="1.27" width="0.127" layer="20"/>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="#mine">
<packages>
<package name="SMD-4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+5V" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.01uF">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E/D" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="OUT" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="#mine" package="SMD-4" value="HC73">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="+5V" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="3"/>
<contactref element="OUT" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="1"/>
<contactref element="E/D" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
