<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="29.21" y1="17.78" x2="80.95" y2="17.78" width="0" layer="20"/>
<wire x1="80.95" y1="17.78" x2="80.95" y2="53.33" width="0" layer="20"/>
<wire x1="80.95" y1="53.33" x2="29.21" y2="53.33" width="0" layer="20"/>
<wire x1="29.21" y1="53.33" x2="29.21" y2="17.78" width="0" layer="20"/>
<text>GND +5 L C D</text>
<text>GND +5 L C D</text>
<text>Data Panel
Charge Panel
v1
</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="SWITCH-SPDT_LOCK.007S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PROC2" library="SparkFun-Boards" package="ARDUINO_MINI" value="Pro Micro or Mini">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP2" library="SparkFun-Connectors" package="1X03" value="ISP2"/>
<element name="PROC1" library="SparkFun-Boards" package="ARDUINO_MINI" value="Pro Micro or Mini">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="ISP1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="S3" library="SparkFun-Electromechanical" package="SWITCH-SPDT_LOCK.007S" value="Off / On">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="SWITCH-SPDT_LOCK.007S" value="Off / On">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X02" value="5v GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X02" value="5v GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
</elements>
<signals>
<signal name="N$10">
<contactref element="PROC2" pad="15"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="ISP2" pad="2"/>
<contactref element="PROC2" pad="14"/>
</signal>
<signal name="N$12">
<contactref element="ISP2" pad="1"/>
<contactref element="PROC2" pad="21"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="ISP2" pad="3"/>
<contactref element="PROC2" pad="23"/>
<contactref element="JP2" pad="5"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="JP3" pad="2"/>
<contactref element="PROC2" pad="16"/>
</signal>
<signal name="N$15">
<contactref element="PROC2" pad="22"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="PROC2" pad="10"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="PROC2" pad="11"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="PROC1" pad="15"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="ISP1" pad="2"/>
<contactref element="PROC1" pad="14"/>
</signal>
<signal name="N$3">
<contactref element="ISP1" pad="1"/>
<contactref element="PROC1" pad="21"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="ISP1" pad="3"/>
<contactref element="PROC1" pad="23"/>
<contactref element="JP1" pad="5"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP5" pad="2"/>
<contactref element="PROC1" pad="16"/>
</signal>
<signal name="N$6">
<contactref element="PROC1" pad="22"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="PROC1" pad="10"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="PROC1" pad="11"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="JP7" pad="2"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="S4" pad="3"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="PROC1" pad="24"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="JP7" pad="1"/>
<contactref element="PROC2" pad="24"/>
</signal>
<signal name="N$18">
<contactref element="PROC2" pad="12"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="PROC1" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
