<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="42" y2="0" width="0" layer="20"/>
<wire x1="42" y1="0" x2="42" y2="25.2" width="0" layer="20"/>
<wire x1="42" y1="25.2" x2="0" y2="25.2" width="0" layer="20"/>
<wire x1="0" y1="25.2" x2="0" y2="0" width="0" layer="20"/>
<text>Band A</text>
<text>frarossi@gmail.com</text>
</plain>
<libraries>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
</package>
</packages>
</library>
<library name="receiver">
<packages>
<package name="RX5808">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA7343">
</package>
</packages>
</library>
<library name="NPX-LD6836TD_36P">
<packages>
<package name="SOT95P275X110-5N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X09" value="M09"/>
<element name="RECEIVER" library="receiver" package="RX5808" value="RX5808V1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA7343" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="EIA7343" value=""/>
<element name="U1" library="NPX-LD6836TD_36P" package="SOT95P275X110-5N" value="LD6836TD/36P">
<attribute name="PACKAGE" value="TSOP-5"/>
<attribute name="OC_NEWARK" value="69W9609"/>
<attribute name="MPN" value="LD6836TD/36P"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="2308339"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="3"/>
<contactref element="RECEIVER" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="RECEIVER" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="2"/>
<contactref element="RECEIVER" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="9"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="RECEIVER" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="1"/>
<contactref element="RECEIVER" pad="2"/>
</signal>
<signal name="GND">
<contactref element="RECEIVER" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="5"/>
<contactref element="RECEIVER" pad="3"/>
<contactref element="RECEIVER" pad="12"/>
<contactref element="JP1" pad="7"/>
<contactref element="RECEIVER" pad="7"/>
<contactref element="C2" pad="C"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
<contactref element="RECEIVER" pad="11"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="C1" pad="C"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="5"/>
<contactref element="RECEIVER" pad="8"/>
<contactref element="C2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
