<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<circle x="2.54" y="8.89" radius="1.651" width="0.0254" layer="20"/>
<circle x="45.72" y="59.69" radius="1.651" width="0.0254" layer="20"/>
<circle x="17.78" y="59.69" radius="1.651" width="0.0254" layer="20"/>
<wire x1="0" y1="1.905" x2="1.905" y2="0" width="0.0254" layer="20"/>
<wire x1="1.905" y1="0" x2="51.435" y2="0" width="0.0254" layer="20"/>
<wire x1="51.435" y1="0" x2="53.34" y2="1.905" width="0.0254" layer="20"/>
<wire x1="53.34" y1="1.905" x2="53.34" y2="62.865" width="0.0254" layer="20"/>
<wire x1="53.34" y1="62.865" x2="51.435" y2="64.77" width="0.0254" layer="20"/>
<wire x1="51.435" y1="64.77" x2="1.905" y2="64.77" width="0.0254" layer="20"/>
<wire x1="1.905" y1="64.77" x2="0" y2="62.865" width="0.0254" layer="20"/>
<wire x1="0" y1="62.865" x2="0" y2="1.905" width="0.0254" layer="20"/>
<text>22</text>
<text>23</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>GND</text>
<text>AREF</text>
<text>25</text>
<text>24</text>
<text>SDA</text>
<text>SCL</text>
<text>A7</text>
<text>A6</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>TX0</text>
<text>RX0</text>
<text>TX1</text>
<text>RX1</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>3.3V</text>
<text>RESET</text>
<text>IOREF</text>
<text>31</text>
<text>30</text>
<text>29</text>
<text>28</text>
<text>27</text>
<text>26</text>
<text>I C</text>
<text>2</text>
<text>5V  3.3V</text>
<text>DIGITAL (  PWM)</text>
<text>ANALOG IN</text>
<text>POWER</text>
<text>UART</text>
<text>SPI</text>
<text>5V   3.3V</text>
<text>22-RX</text>
<text>23-TX</text>
<text>10-SS</text>
<text>11-MOSI</text>
<text>12-MISO</text>
<text>13-SCK</text>
<text>24-SCL</text>
<text>SDA</text>
<text>I C</text>
<text>I C</text>
<text>2</text>
<text>2</text>
<text>Pullups</text>
<text>Pullups</text>
<text>SCL</text>
<text>SDA</text>
<text>SCL</text>
<text>POWER</text>
<text>PIN 13</text>
<text>RX LED</text>
<text>TX LED</text>
<text>DIGITAL</text>
<text>'DUINO</text>
<text>POWER</text>
<text>GND</text>
<text>3.3V</text>
<text>5V</text>
<text>Pre-level shifter</text>
<text>Post-level shifter</text>
<text>5VDC</text>
<text>3.3VDC</text>
<text>Pch</text>
<text>Nch</text>
<text>ICSP</text>
<text>GND</text>
<text>MOSI</text>
<text>VCC</text>
<text>MISO</text>
<text>SCK</text>
<text>RESET</text>
</plain>
<libraries>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P1200X1200X120-44N">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_NO_SILK">
</package>
<package name="1X06_NO_SILK">
</package>
<package name="2X3-NS">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
<package name="PANASONIC_D">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SOT23-3">
</package>
<package name="0603-RES">
</package>
<package name="SOT323">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP20_L">
<description>Longer version of SSOP-20 Package</description>
</package>
<package name="PVQFN-20">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
<package name="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P1200X1200X120-44N" value="ATMEGA1284P-AU">
<attribute name="PACKAGE" value="TQFP-44"/>
<attribute name="OC_NEWARK" value="15R0263"/>
<attribute name="MPN" value="ATMEGA1284P-AU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1715480"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-SMD" value="16MHZ">
<attribute name="PROD_ID" value="XTAL-08900"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD-REDUNDANT">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="U$1" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920"/>
<element name="U$2" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920"/>
<element name="C4" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="PANASONIC_D" value=""/>
<element name="D3" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="MBRA140">
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MOSFET-PCHANNELSMD"/>
<element name="C7" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun-Connectors" package="USB-MINIB" value="USB-MINIB-5PIN"/>
<element name="U3" library="SparkFun-DigitalIC" package="SSOP20_L" value="FTS31XS-U">
<attribute name="PROD_ID" value="IC-11524"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z1" library="SparkFun-DiscreteSemi" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="EIA3216" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="U2" library="SparkFun-DigitalIC" package="PVQFN-20" value="TXB0108PVQFN-20"/>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ7" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ8" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ9" library="SparkFun-Passives" package="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ10" library="SparkFun-Passives" package="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value="">
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="U1" pad="37"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="36"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="35"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="34"/>
<contactref element="JP9" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="33"/>
<contactref element="JP9" pad="5"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="32"/>
<contactref element="JP9" pad="6"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="31"/>
<contactref element="JP9" pad="7"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="30"/>
<contactref element="JP9" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP5" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="C4" pad="A"/>
<contactref element="C7" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="JP1" pad="7"/>
<contactref element="U2" pad="P19"/>
<contactref element="SJ9" pad="2"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP10" pad="2"/>
<contactref element="JP10" pad="3"/>
<contactref element="JP10" pad="4"/>
<contactref element="JP10" pad="5"/>
<contactref element="JP10" pad="6"/>
</signal>
<signal name="XTAL1">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="XTAL2">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="D22">
<contactref element="U1" pad="11"/>
<contactref element="SJ1" pad="3"/>
<contactref element="U2" pad="P20"/>
</signal>
<signal name="D23">
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="P18"/>
<contactref element="SJ2" pad="3"/>
</signal>
<signal name="D24">
<contactref element="U1" pad="19"/>
<contactref element="U2" pad="P13"/>
<contactref element="SJ7" pad="3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="D25">
<contactref element="U1" pad="20"/>
<contactref element="SJ8" pad="3"/>
<contactref element="U2" pad="P12"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="D26">
<contactref element="U1" pad="21"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="D27">
<contactref element="U1" pad="22"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="D28">
<contactref element="U1" pad="23"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="D29">
<contactref element="U1" pad="24"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D30">
<contactref element="U1" pad="25"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="D31">
<contactref element="U1" pad="26"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="29"/>
<contactref element="JP7" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP5" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="39"/>
<contactref element="Y1" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP5" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="R3" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="U$2" pad="2"/>
<contactref element="C5" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="-"/>
<contactref element="U$1" pad="2"/>
<contactref element="C4" pad="C"/>
<contactref element="C7" pad="2"/>
<contactref element="JP6" pad="GNDBREAK"/>
<contactref element="U$3" pad="MTN3"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$3" pad="MTN1"/>
<contactref element="U$3" pad="MTN4"/>
<contactref element="U$3" pad="MTN2"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="16"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="C"/>
<contactref element="JP12" pad="6"/>
<contactref element="JP12" pad="5"/>
<contactref element="JP12" pad="4"/>
<contactref element="JP12" pad="3"/>
<contactref element="JP12" pad="2"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="9"/>
<contactref element="JP8" pad="8"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="10"/>
<contactref element="JP8" pad="7"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="40"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="13"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="14"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="15"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="16"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="41"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="42"/>
<contactref element="JP7" pad="8"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="43"/>
<contactref element="JP7" pad="7"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="44"/>
<contactref element="SJ3" pad="3"/>
<contactref element="U2" pad="P17"/>
</signal>
<signal name="D11">
<contactref element="U1" pad="1"/>
<contactref element="JP5" pad="4"/>
<contactref element="U2" pad="P16"/>
<contactref element="SJ4" pad="3"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="U2" pad="P15"/>
<contactref element="SJ5" pad="3"/>
</signal>
<signal name="D13">
<contactref element="U1" pad="3"/>
<contactref element="JP5" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="P14"/>
<contactref element="SJ6" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="JP1" pad="5"/>
<contactref element="U$2" pad="3"/>
<contactref element="C5" pad="A"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="14"/>
<contactref element="U3" pad="13"/>
<contactref element="U3" pad="3"/>
<contactref element="C9" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="U2" pad="P2"/>
<contactref element="U2" pad="P10"/>
<contactref element="SJ10" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="VIN">
<contactref element="JP1" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="C6" pad="+"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C2" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP6" pad="PWR"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="JP6" pad="GND"/>
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="USBVCC">
<contactref element="Q1" pad="3"/>
<contactref element="Z1" pad="2"/>
<contactref element="U3" pad="15"/>
<contactref element="C12" pad="A"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="D-"/>
<contactref element="R5" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="D+"/>
<contactref element="R6" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="2"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="2"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="N$13">
<contactref element="Z1" pad="1"/>
<contactref element="U$3" pad="VBUS"/>
</signal>
<signal name="N$16">
<contactref element="U3" pad="20"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="4"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="D5" pad="A"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="D4" pad="A"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="D5" pad="C"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="17"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="U3" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="DD10">
<contactref element="JP7" pad="6"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="DD11">
<contactref element="JP7" pad="5"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="DD12">
<contactref element="JP7" pad="4"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="DD13">
<contactref element="JP7" pad="3"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="XSCL">
<contactref element="JP11" pad="2"/>
<contactref element="SJ7" pad="2"/>
</signal>
<signal name="DD22">
<contactref element="JP2" pad="2"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="DD23">
<contactref element="JP2" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="P1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="SJ2" pad="1"/>
<contactref element="U2" pad="P3"/>
</signal>
<signal name="N$28">
<contactref element="U2" pad="P4"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="SJ4" pad="1"/>
<contactref element="U2" pad="P5"/>
</signal>
<signal name="N$30">
<contactref element="SJ8" pad="1"/>
<contactref element="U2" pad="P9"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U2" pad="P8"/>
<contactref element="SJ7" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="SJ6" pad="1"/>
<contactref element="U2" pad="P7"/>
</signal>
<signal name="N$33">
<contactref element="U2" pad="P6"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="XSDA">
<contactref element="SJ8" pad="2"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R15" pad="1"/>
<contactref element="SJ9" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R16" pad="1"/>
<contactref element="SJ9" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="SJ10" pad="3"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="SJ10" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
