<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.04" y2="0" width="0" layer="20"/>
<wire x1="39.04" y1="0" x2="39.04" y2="19.04" width="0" layer="20"/>
<wire x1="39.04" y1="19.04" x2="0" y2="19.04" width="0" layer="20"/>
<wire x1="0" y1="19.04" x2="0" y2="0" width="0" layer="20"/>
<text>DAN CORWIN</text>
<text>KD2BBW</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4,16O1,6">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="custom">
<packages>
<package name="BNC">
</package>
<package name="SDR0403_IND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="2P">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="3P">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.01">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.01">
<attribute name="NAME"/>
</element>
<element name="NOR" library="wirepad" package="4,16O1,6" value="NOR">
<attribute name="NAME"/>
</element>
<element name="JJY" library="wirepad" package="4,16O1,6" value="JJY">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="100K">
<attribute name="NAME"/>
</element>
<element name="U$1" library="custom" package="BNC" value="BNC"/>
<element name="SHLD" library="wirepad" package="4,16O1,6" value="SHD">
<attribute name="NAME"/>
</element>
<element name="SHLD2" library="wirepad" package="4,16O1,6" value="NORSHD">
<attribute name="NAME"/>
</element>
<element name="+14V" library="wirepad" package="4,16O1,6" value="+14V">
<attribute name="NAME"/>
</element>
<element name="GND" library="wirepad" package="4,16O1,6" value="GND">
<attribute name="NAME"/>
</element>
<element name="U$2" library="custom" package="SDR0403_IND" value="SDR0403_IND"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="S"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="SHLD2" pad="1"/>
<contactref element="SHLD" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="+14V" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="2"/>
<contactref element="NOR" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C1" pad="2"/>
<contactref element="JJY" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
