<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="-1.8" y1="1.4" x2="31" y2="1.4" width="0" layer="20"/>
<wire x1="31" y1="21.4" x2="-4" y2="21.4" width="0" layer="20"/>
<text>VG1</text>
<text>VG2</text>
<text>Vsrc</text>
<text>Vsrc</text>
<hole x="28.5" y="18.6" drill="2.4"/>
<hole x="28.5" y="4.5" drill="2.4"/>
<text>Vin</text>
<text>Vout</text>
<wire x1="-4" y1="21.4" x2="-4" y2="15" width="0.00635" layer="20"/>
<wire x1="-4" y1="15" x2="0" y2="15" width="0.00635" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="8" width="0.00635" layer="20"/>
<wire x1="-4" y1="8" x2="-4" y2="1.4" width="0.00635" layer="20"/>
<wire x1="-4" y1="1.4" x2="-1.8" y2="1.4" width="0.00635" layer="20"/>
<wire x1="0" y1="8" x2="-4" y2="8" width="0.00635" layer="20"/>
<wire x1="31" y1="21.4" x2="31" y2="15" width="0.00635" layer="20"/>
<wire x1="31" y1="15" x2="27" y2="15" width="0.00635" layer="20"/>
<wire x1="27" y1="15" x2="27" y2="8" width="0.00635" layer="20"/>
<wire x1="27" y1="8" x2="31" y2="8" width="0.00635" layer="20"/>
<wire x1="31" y1="8" x2="31" y2="1.4" width="0.00635" layer="20"/>
<hole x="-1" y="18.6" drill="2.4"/>
<hole x="-1" y="4.5" drill="2.4"/>
</plain>
<libraries>
<library name="Tinkercad">
<packages>
<package name="CAPC1608X85">
<description>Chip, 1.60 X 0.80 X 0.85 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.85 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Tutorial - Fusion 360">
<description>Library of several components used in the Getting Started With Fusion Electronics tutorial.</description>
<packages>
<package name="RESC1608X60">
<description>Chip, 1.60 X 0.82 X 0.60 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.82 X 0.60 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="4K AMP LIBRARY">
<packages>
<package name="ATF34143">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Tinkercad" package="CAPC1608X85" value="">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C2" library="Tinkercad" package="CAPC1608X85" value="">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C3" library="Tinkercad" package="CAPC1608X85" value="">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="R1" library="Tutorial - Fusion 360" package="RESC1608X60" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Tutorial - Fusion 360" package="RESC1608X60" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Tutorial - Fusion 360" package="RESC1608X60" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Tutorial - Fusion 360" package="RESC1608X60" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="4K AMP LIBRARY" package="ATF34143" value="ATF34143">
</element>
<element name="U$2" library="4K AMP LIBRARY" package="ATF34143" value="ATF34143">
</element>
<element name="R5" library="Tutorial - Fusion 360" package="RESC1608X60" value="">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Tinkercad" package="CAPC1608X85" value="">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C5" library="Tinkercad" package="CAPC1608X85" value="">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="GATE"/>
</signal>
<signal name="VG1">
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="S1"/>
<contactref element="U$1" pad="S2"/>
<contactref element="U$2" pad="S1"/>
<contactref element="U$2" pad="S2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="D"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="VSRC">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="U$2" pad="GATE"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VG2">
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="D"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
