<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="12.7" x2="15.24" y2="12.7" width="0" layer="20"/>
<wire x1="15.24" y1="12.7" x2="15.24" y2="0" width="0" layer="20"/>
<wire x1="15.24" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="12.7" width="0" layer="20"/>
<text>VCC</text>
<text>D-</text>
<text>D+</text>
<text>3.3</text>
<text>GND</text>
<text>Breakout</text>
<text>VCC</text>
<text>D-</text>
<text>D+</text>
<text>3.3</text>
<text>GND</text>
<text>mini USB</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X05">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="SOT23" value="MCP1703CB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun-Connectors" package="USB-MINIB-OLD" value="USBOLD">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="GND"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="X1" pad="VBUS"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="D-">
<contactref element="X1" pad="D-"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D+">
<contactref element="X1" pad="D+"/>
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
