<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30" y2="0" width="0" layer="20"/>
<wire x1="30" y1="0" x2="30" y2="29" width="0" layer="20"/>
<wire x1="30" y1="29" x2="0" y2="29" width="0" layer="20"/>
<wire x1="0" y1="29" x2="0" y2="0" width="0" layer="20"/>
<hole x="5" y="8" drill="2"/>
<hole x="25" y="8" drill="2"/>
<text>RADDS SD
</text>
<text>RADDS</text>
<text>EXT</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>by Overtuner 12/2015
</text>
<text>RADDS SD
</text>
<text>V 0.4 by Overtuner 12/2015
</text>
<text>MISO</text>
<text>3V3</text>
<text>CS1</text>
<text>CD</text>
<text>MOSI</text>
<text>CLK</text>
<text>CS0</text>
<text>SCL1</text>
<text>RST</text>
<text>CS0</text>
<text>SCL1</text>
<text>RST</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SDCARD_4UCONN">
<description>4UConn part#19646</description>
</package>
</packages>
</library>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="2X03SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RADDS-SD" library="pinhead-1" package="2X05SMD" value=""/>
<element name="U1" library="SparkFun-Connectors" package="SDCARD_4UCONN" value="SD_CARD_SOCKET4UCON"/>
<element name="EXT" library="pinhead-1" package="2X03SMD" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
<element name="U$3" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
</elements>
<signals>
<signal name="3V3">
<contactref element="U1" pad="4"/>
<contactref element="RADDS-SD" pad="7"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="SH@1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="SH@2"/>
<contactref element="RADDS-SD" pad="5"/>
<contactref element="EXT" pad="2"/>
<contactref element="EXT" pad="4"/>
<contactref element="EXT" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="7"/>
<contactref element="RADDS-SD" pad="4"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="5"/>
<contactref element="RADDS-SD" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="2"/>
<contactref element="RADDS-SD" pad="8"/>
</signal>
<signal name="CS1">
<contactref element="U1" pad="1"/>
<contactref element="RADDS-SD" pad="9"/>
</signal>
<signal name="CD">
<contactref element="U1" pad="CD"/>
<contactref element="RADDS-SD" pad="10"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="RST">
<contactref element="RADDS-SD" pad="1"/>
<contactref element="EXT" pad="1"/>
</signal>
<signal name="SCL1">
<contactref element="RADDS-SD" pad="2"/>
<contactref element="EXT" pad="3"/>
</signal>
<signal name="CS0">
<contactref element="RADDS-SD" pad="3"/>
<contactref element="EXT" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
